# SensorML 2.0 Examples Index

NOTE: SensorML 2.0 is not yet approved by the Open Geospatial Consortium (OGC). Examples here are provided for evaluation and are subject to change during the standards review and approval process. Contact mike.botts@botts-inc.net for questions or recommendations.

> #### "Hello Sensor World!"

> - Friendly sensor
> - Friendly and informative sensor
> - Friendly process (linear equation)
> - Sensor instance (simple extension)

> #### Metadata

> - Lots of Metadata
> - Identifiers and Classifiers
> - Characteristics and Capabilities
> - Constraints
> - Feature of interest (FoI)
> - Documentation
> - Contacts
> - Sensor history

> #### Physical Components

> - Detector (digital)
> - Detector (analog)
> - Actuator (digital)
> - Filter (analog)
> - Platform

> #### Physical Systems

> - Weather station
> - Web cam

> #### Computational Processes

> - Simple process (Wind Chill Factor)
> - Simple Process (Orbit Propagator)
> - Aggregate process (components described inline)
> - Aggregate process (configured components)

> #### Location and Position

> - Sensor with location by description (byDescription)
> - Sensor with GML point location (byPoint)
> - Sensor with static location (byLocation)
> - Sensor with orientation (byState)
> - Sensor with dynamic position (byTrajectory)
> - Sensor with location output (byTrajectory)
> - Sensor with orbit propagator (byProcess)
> - Sensor with SOS for location (byProcess)

> #### Inheritance and Configuration

> - Simple extension of process
> - Constraining on a process
> - Simple extension of sensor
> - Supporting modes
> - Supporting configuration
> - Complex configuration

> #### Web-based Processes

> - Web-based Process Client
> - SOS Client Process
> - SOS Client (Configured Instance)
> - SPS Client Process

> #### Using Extensions

> - Security tagging
> - Using MathML

> #### Data Interface / Streaming Data

> - Simple streaming (return latest value)
> - Simple streaming (returns RTP stream)
> - Simple multiplexed streaming
> - Homogeneous sensor network (identical sensor output)
> - Disparate sensor network
> - Complex multiplexed sensor (CBRN)
> - Streaming navigation data

> #### Inernet of Things / Web of Things

> - Simple Sensor
> - Sensor System
> - Sensor System (multiple output streams)

> #### Data Interface Types

> - RS-232
> - Real-Time Protocol (RTP)
> - http protocol

> #### Output Encodings

> - ASCII encoding
> - Binary encoding

> #### Various Output Types

> - Time Series
> - Imagery
> - Video
> - Alerts
> - Multiplex Messages

> #### Precise Geolocation

> - Community Sensor Model (CSM) Frame Camera
> - My High-Definition Camera
> - CSM Frame Camera with Platform
> - Static Web Camera
> - Dynamic Video Camera

> #### Miscellaneous

> - Outputting Parameter Values (sensor settings)
> - Outputting Sensor Position