# SensorML 2.0 Examples

## Friendly Process

SensorML supports non-physical processes, as well as physical processes (such as sensors). A linear interpolator, based on the equation y = mx + b, is a simple process that is described in the example below. In this example, x is treated as input, y is the output, and m (slope) and b (y-intercept) are parameters of the process.

The designation of "any" for the units of measure (uom) [highlighted sections] is a special code that tells the units checker to allow any units for this process.

NOTE: SensorML 2.0 is not yet approved by the Open Geospatial Consortium (OGC). Examples are provided for evaluation and are subject to change during the standards review and approval process. Contact mike.botts@botts-inc.net for questions or recommendations.