# SensorML 2.0 Examples

## Sensor Outputting Static Location

In one wishes to include the static position of a sensor or actuator as output, they simply need to reference the data component from the position property. This is done using the xlink:href attribute on the output or field property and referencing the id value of the position property. These two properties are highlighted below.

NOTE: SensorML 2.0 is not yet approved by the Open Geospatial Consortium (OGC). Examples are provided for evaluation and are subject to change during the standards review and approval process. Contact mike.botts@botts-inc.net for questions or recommendations.