Open Geospatial Consortium Inc.

Date:   2012-09-12

Reference number of this OGC® document:  OGC 12-000

OGC name of this OGC® project document: http://www.opengis.net/doc/IS/SensorML/2.0

Version: 2.0.0

Category: OGC® Encoding Standard

Editor: Mike Botts

Co-Editor: Alexandre Robin

OGC® SensorML:  
 Model and XML Encoding Standard

**Copyright notice**

Copyright © 2012 Open Geospatial Consortium  
To obtain additional rights of use, visit <http://www.opengeospatial.org/legal/>.

**Warning**

This document is not an OGC Standard. It is distributed for review and comment. It is subject to change without notice and may not be referred to as an OGC Standard.

Document type:    OGC® Publicly Available Standard

Document subtype:    Encoding

Document stage:    Draft

Document language:  English

Recipients of this document are invited to submit, with their comments, notification of any relevant patent rights of which they are aware and to provide supporting documentation.

(Page intentionally left blank)

Contents

i. Preface ix

ii. Submitting Organizations ix

Submission Contact Points x

iii. Revision History x

iv. Future Work x

v. Changes to the OGC® Abstract Specification x

Sensor Model Language (SensorML): An Implementation Specification 14

1 Scope 14

2 Conformance 16

2.1 Overview 16

2.2 Specification identifier 16

2.3 Conformance classes 16

3 Normative References 18

4 Terms and Definitions 19

5 Conventions 24

5.1 Abbreviated terms 24

5.2 UML notation 25

5.3 Table notation used to express requirements 25

6 Requirements Class: Core Concepts (normative core) 27

6.1 Introduction 27

6.2 Process Definitions 28

7 UML Conceptual Models (normative) 30

7.1 Package Dependencies 30

7.1.1 Dependency on GML Feature Model and ISO TC 211 Models 30

7.1.2 Dependency on SWE Common Data Models 33

7.1.3 Relationship to Observations and Measurements (O&M) 35

7.2 Requirements Class: Core Abstract Process 37

7.2.1 ObservableProperty 37

7.2.2 DescribedObject 38

7.2.3 AbstractProcess 43

7.3 Requirements Class: Simple Process 50

7.3.1 Simple Process Definition 50

7.3.2 Process Method Definition 51

7.4 Requirements Class: Aggregate Process 53

7.4.1 Aggregate Process Definition 53

7.5 Requirements Class: Non-Physical Processes 56

7.6 Requirement Class: Physical Component 57

7.6.1 Abstract Physical Process Defined 57

7.6.2 Physical Component Defined 61

7.7 Requirement Class: Physical System 62

7.8 Requirements Class: Physical Processes 64

7.9 Requirements Class: Configurable Processes 65

7.9.1 Modes 66

7.9.2 Settings 67

8 XML Schema Implementation (normative) 70

8.1 Requirements Class: Core Abstract Process Schema 71

8.1.1 General XML Principles 71

8.1.2 General XSD Dependencies and XML Heading 75

8.1.3 DescribedObject Properties 77

8.1.4 Abstract Process 96

8.2 Requirements Class: Simple Process Schema 116

8.2.1 Simple Process 116

8.2.2 Process Method 117

8.3 Requirements Class: Aggregate Process Schema 119

8.3.1 Aggregate Process 120

8.3.2 Components 126

8.3.3 Connections 127

8.4 Requirements Class: Physical Component Schema 132

8.4.1 Abstract Physical Process 133

8.4.2 Physical Component 144

8.5 Requirements Class: Physical System Schema 147

8.5.1 Physical System 148

Requirements Class: Configurable Process Schema 152

8.5.2 Modes 153

8.5.3 Settings 155

A.1 Conformance Test Class: Core Concepts 159

A.1.1 Core concepts are the base of all derived models 159

A.1.2 A process model has inputs, outputs, parameters, and method 159

A.1.3 A process model has a unique ID 160

A.1.4 A process model has metadata 160

A.1.5 Metadata not used in process execution 160

A.2 Conformance Test Class: Core Abstract Process 161

A.2.1 Dependency on core 161

A.2.2 DescribedObject derived from GML AbstractFeature 161

A.2.3 Using GML identifier for uniqueID in CoreProcess 162

A.2.4 Extensions must be in a separate namespace 162

A.2.5 Extensions shall not be required for process execution 162

A.2.6 ObservableProperty and SWE Common Data used for process input, output, and parameters 163

A.2.7 Use of SWE Common Data aggregate models for process input, output, and parameters 163

A.2.8 Application and requirements of *typeOf* property 163

A.2.9 Simple inheritance extends a base class referenced by typeOf 164

A.2.10 Supporting configuration in processes 164

A.3 Conformance Test Class: Simple Process 165

A.3.1 Dependency on core 165

A.3.2 Simple process definition 165

A.3.3 Simple process has method 166

A.4 Conformance Test Class: Aggregate Process 167

A.4.1 Dependency on core 167

A.4.2 Definition of Aggregate Process 167

A.4.3 Aggregate Process requires one or more components 168

A.5 Conformance Test Class: Non-physical Processes 169

A.5.1 Dependency on simple and aggregate processes 169

A.6 Conformance Test Class: Physical Component 170

A.6.1 Dependency on core process 170

A.6.2 Position by point 170

A.6.3 Position by location and orientation 171

A.6.4 Position by trajectory 171

A.6.5 Position by process 172

A.6.6 Physical Component definition 172

A.7 Conformance Test Class: Physical System 173

A.7.1 Physical System definition 173

A.7.2 Physical System dependency 173

A.8 Conformance Test Class: Physical Processes 174

A.8.1 Physical Process dependency 174

A.9 Conformance Test Class: Configurable Processes 175

A.9.1 Definition of Configurable Process 175

A.9.2 Definition of Configured Process 175

A.9.3 *ModeChoice* requires 2 or more *Modes* 176

A.9.4 A configured process requires a Settings element 176

A.9.5 Only *parameter* values can be set by *setValue* 176

A.9.6 Only *parameter* array values can be set by *setArrayValues* 177

A.9.7 Only *parameter* values can be constrained with *setConstraint* 177

A.10 Conformance Test Class: Core Abstract Process Schema 178

A.10.1 Compliance with core XML schemas and Schematron patterns 178

A.10.2 XML property values are included inline or by reference 178

A.10.3 Each extension uses a different namespace 179

A.10.4 Extensions do not redefine XML elements or types 179

A.10.5 The value of the definition attribute is a resolvable URI 179

A.10.6 Dependence on GML 3.2 180

A.10.7 Dependence on SWE Common Data 2.0 180

A.10.8 Globally unique ID required 180

A.10.9 External namespace required for security constraints 181

A.10.10 *Extension* element used for security tagging of individual properties 181

A.10.11 Xlink role or arcrole shall be used to define relationship of contacts 181

A.10.12 The *typeOf* property shall provide the uniqueID and resolvable location of the description on the referenced object 182

A.10.13 The feature of interest property shall specify a role, and if available, the uniqueID of the feature 182

A.10.14 The *definition* attribute required for *ObservableProperty* 183

A.10.15 Use aggregate data for related data elements 183

A.10.16 Use Vector for *inputs*, *outputs*, and *parameters* that specify position 183

A.10.17 Use of resolvable URL to reference data streams 184

A.10.18 Use *DataChoice* in multiplexed data streams 184

A.11 Conformance Test Class: Simple Process Schema 185

A.11.1 Compliance with simple\_process XML schemas and Schematron patterns 185

A.12 Conformance Test Class: Aggregate Process Schema 186

A.12.1 Compliance with simple\_process XML schemas and Schematron patterns 186

A.12.2 Title and resolvable URL required for components provided by Reference 186

A.13 Conformance Test Class: Physical Component Schema 189

A.13.1 Compliance with physical\_component XML schemas and Schematron patterns 189

A.13.2 A physical process can only attach to a physical process 189

A.13.3 The *attachedTo* element must have *xlink:title* and *xlink:href* 190

A.13.4 Position requires a DataRecord with two Vectors 190

A.13.5 Dynamic state requires a Data Array or Process 190

A.13.6 Trajectory requires a DataArray with a time field and one or more Vectors 191

A.13.7 Process required for positions or state provided on-demand 191

A.14 Conformance Test Class: Physical System Schema 192

A.14.1 Compliance with physical\_system XML schemas and Schematron patterns 192

A.15 Conformance Test Class: Configurable Process Schema 193

A.15.1 Compliance with configuration XML schemas and Schematron patterns 193

A.15.2 Modes can change values of parameters 193

A.15.3 Modes can only set values of parameters to those allowed by its constraints 194

Table of Figures

Figure 5.1 – UML Notation 25

Figure 7.1 – Internal Package Dependencies 30

Figure 7.2 – External Package Dependencies – GML 31

Figure 7.3 – Models for dependent GML Feature classes 32

Figure 7.4 – External Package Dependencies – ISO TC 211 32

Figure 7.5 – ISO 19115 Models for dependent classes. 33

Figure 7.6 – External Package Dependencies – SWE Common Data 34

Figure 7.7 –Models for dependent SWE Common AbstractDataComponent class. 35

Figure 7.8 – DescribedObject with Metadata Properties 40

Figure 7.9 – Models for Metadata Elements 40

Figure 7.10 – Model for history events 43

Figure 7.11 – UML models for DescribedObject and AbstractProcess 44

Figure 7.12 – UML models for process inputs, outputs, and parameters. 45

Figure 7.13 – Model for Simple Process 51

Figure 7.14 – Model for ProcessMethod 52

Figure 7.15 – Model for Aggregate Process 55

Figure 7.16 – Model for Physical Process Component 58

Figure 7.17 – Models for ReferenceFrame and PositionUnion 59

Figure 7.18 – Model for Physical Processing System 64

Figure 7.19 – Model for Modes 68

Figure 7.20 – Model for Configured Process Settings 69

Figure 7.21 – Model for Settings Elements 70

# Preface

The primary focus of the Sensor Model Language (SensorML) is to provide a robust means of defining processes and processing components associated with the measurement and post-measurement transformation of observations. This includes sensors and actuators as well as computational processes applied pre- and post-measurement.

The main objective is to enable interoperability, at both the syntactic and semantic levels, so that sensors and processes can be better understood by machines, utilized automatically in complex workflows, and easily shared between intelligent sensor web nodes.

This standard is one of several implementation standards produced under OGC’s Sensor Web Enablement (SWE) activity. This standard is a revision of content that was previously integrated in the SensorML version 1.0 standard (OGC 07-000).

# Submitting Organizations

The following organizations have contributed and submitted this Encoding Standard to the Open Geospatial Consortium Inc.:

* Botts Innovative Research, Inc.
* Spot Image, S.A.
* Seicorp, Inc.
* US National Geospatial Intelligence Agency (NGA)
* TASC

# Submission Contact Points

All questions regarding this submission should be directed to the editor or the submitters:

|  |  |  |
| --- | --- | --- |
| Contact | Company | Email |
| Michael E. Botts | Botts Innovative Research, Inc | [mike.botts@botts-inc.net](mailto:mike.botts@botts-inc.net) |
| Alexandre Robin | SensiaSoftware | [alex.robin@sensiasoftware.com](mailto:alex.robin@sensiasoftware.com) |
| Jim Greenwood | Seicorp, Inc. | [jgreenwood@Seicorp.com](mailto:jgreenwood@Seicorp.com) |
| David Wesloh | US National Geospatial Intelligence Agency | [David.G.Wesloh@nga.mil](mailto:David.G.Wesloh@nga.mil) |
|  |  |  |

# Revision History

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Date | Release | Author | Paragraph modified | Description |
| 2012-03-16 | 2.0 draft | Mike Botts | All | Initial reviewed version |
| 2012-07-27 | 2.0 | Mike Botts | All | Completed specification |
| 2012-09-12 | 2.0 | John Greybeal | All | Edits and corrections throughout |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

# Future Work

Future work will target the description of specialized processes, sensors, and actuators by restricting (via profiles) the generic models and schema defined in this standard. Such profiles will allow interoperability of models and schema both within specific processing and measurement communities as well as between disparate.

# Changes to the OGC® Abstract Specification

The OGC**®** Abstract Specification does not require changes to accommodate this OGC**®** Standard.

Foreword

Attention is drawn to the possibility that some of the elements of this document may be the subject of patent rights. Open Geospatial Consortium Inc. shall not be held responsible for identifying any or all such patent rights. However, to date, no such rights have been claimed or identified. Recipients of this document are requested to submit, with their comments, notification of any relevant patent claims or other intellectual property rights of which they may be aware that might be infringed by any implementation of the specification set forth in this document, and to provide supporting documentation.

Introduction

This Standard arises from work originally undertaken through the Open Geospatial Consortium’s Sensor Web Enablement (SWE) activity. SWE is concerned with establishing interfaces and encodings that will enable a “Sensor Web” through which applications and services will be able to access sensors of all types, and observations generated by them, over the Web. SWE has defined, prototyped and tested several components needed for a Sensor Web, namely:

* Sensor Model Language (SensorML)
* Observations & Measurements (O&M)
* Sensor Observation Service (SOS)
* Sensor Planning Service (SPS)
* SWE Common Data and Services

This Standard specifies models and an XML implementation for the SensorML.

This document deprecates and replaces the first version of OGC® Sensor Model Language (SensorML) Specification version 1.0.0 (OGC 07-000) and the SensorML Corrigendrum version 1.0.1 (OGC 07-122r2).

The main changes from SensorML version 1.0.1 are:

* The separation of SWE Common Data into a separate specification (OGC 07-094r1)
* Improved derivation and association of SensorML from GML 3.2 and ISO 19115
* More explicit definition of the standard and its requirements
* Separation of SensorML into several conformance classes to allow software to support only the part of SensorML that is relevant to the application (e.g. non-physical processes only)
* Improved support for inheritance, configuration, and modes (e.g. for describing a particular model of a sensor and then an instance of that sensor with particular configuration)
* Improved explicit support for data streaming (associated with inputs, outputs, and parameters)
* Addition of Feature of Interest for support of discovery
* Addition of extension points for domain or community-specific schema
* Improved support for defining position of both static and dynamic components and systems
* Inclusion of DataInterface and DataStream as a possible input, output, or parameter value

Additionally, much additional and improved functionality of SensorML has been gained through additions and improvements of the SWE Common Data Model specification. Thus, the following additions to SWE Common Data Model are reflected as improvements in SensorML v2.0:

* A DataChoice component providing support for variable (multiplexed) data types
* The DataStream object improving support for real-time data streams
* The XMLBlock encoding providing support for simple XML encoded data
* Support for definition of NIL values and associated reasons
* The CategoryRange class to define ranges of ordered categorical quantities
* Extension points for domain or community-specific schema
* Ability to provide security tagging of individual data components through the use of extension points

Also, some elements of the SWE Common Data Model specification have been removed and will be replaced by their soft-typed equivalents. The list is given are:

* Position, SquareMatrix
* SimpleDataRecord, ObservableProperty
* ConditionalData, ConditionalValue
* Curve, NormalizedCurve

The derivation from GML has also been improved by making all elements substitutable for GML AbstractValue (and thus transitively for GML AbstractObject) and AbstractFeature so that they can be used directly by GML application schemas. The GML encoding rules as defined in ISO 19136 have also been used to generate XML schemas from the UML models with only minor modifications.

This release is not fully backwards compatible with version 1.0.1 even though changes were kept to a minimum.

Sen­sor Model Language (SensorML):   
An Implementation Specification

# Scope

This standard defines models and XML Schema encoding for SensorML. The primary focus of SensorML is to provide a framework for defining processes and processing components associated with the measurement and post-measurement transformation of observations. Thus SensorML has more of a focus on the process of measurement and observation, rather than on sensor hardware, while still provding a robust means of defining the physical characteristics and functional capabilities of physical processes such as sensors and actuators.

The aims SensorML are to:

* Provide sensor and process information in support of asset and observation discovery
* Support the processing and analysis of the sensor observations
* Support the geolocation of observed values (measured data)
* Provide performance and quality of measurement characteristics (e.g., accuracy, threshold, etc.)
* Provide general descriptions of components (e.g. a particular model or type of a sensor) as well as the specific configuration of that component when its deployed
* Provide descriptions of sensors and sensor systems for inventory management
* Provide a machine interpretable description of the interfaces and data streams flowing in and out of a component
* Provide an explicit description of the process by which an observation was obtained (i.e., its lineage)
* Provide an executable aggregate process for deriving new data products on demand (i.e., derivable products)
* Archive fundamental properties and assumptions regarding sensor systems and computational processes

SensorML provides a common framework for any process, but is particularly well-suited for the description of sensor and systems and the processes surrounding sensor observations. Within SensorML, sensor systems and transducer components (detectors, transmitters, actuators, and filters) are all modeled as physical processes that can be connected and participate equally within a process network or system, and utilize the same model framework as any other process.

Processes are entities that take one or more inputs and through the application of well-defined methods and configurable parameters, produce one or more outputs. The process model defined in SensorML can be used to describe a wide variety of processes, including actuators, spatial transforms, and data processes, to name a few. SensorML also supports explicit linking between processes and thus supports the concept of aggregate processes or workflows, which are themselves defined as processes.

SensorML provides a framework within which the geometric, dynamic, and observational characteristics of sensors and sensor systems can be defined. There are a great variety of sensor types, from simple thermometers to complex electron microscopes and earth observing satellites. These can all be supported through the definition of simple and aggregate processes.

The models and schema within the core SensorML specification provide a “skeletal” framework for describing processes, aggregate processes, and sensor systems. Interoperability within and between various sensor communities, is greatly improved through the definition of shared community semantics (within online dictionaries or ontologies) that can be utilized within the framework. In addition, we envision the profiling of small, general-use, atomic processes that can serve as components within aggregate processes and systems.

# Conformance

## Overview

This standard has been written to be compliant with the OGC Specification Model – A Standard for Modular Specification (OGC 08-131r3). Extensions of this standard shall themselves be conformant to the OGC Specification Model.

This Standard defines conceptual models and an XML implementation of these models for describing non-physical and physical processes surrounding the act of measurement and subsequent processing of observations. The conceptual models are described using UML while the implementation is described using the XML Schema language and Schematron. It is envisioned that OWL (Web Ontology Language) and RDF (Resource Description Framework) versions could also be generated from the models if deemed useful and desired.

## Specification identifier

All requirements-classes and conformance-classes described in this document are owned by the specification identified as **<http://www.opengis.net/spec/sensorML/2.0>**.

## Conformance classes

The conformance rules are based on XML validation using the XML Schema representation of SensorML, together with processing of constraints expressed using Schematron assertions and reports.

Conformance with this specification shall be checked using all the relevant tests specified in Annex A. The framework, concepts, and methodology for testing, and the criteria to be achieved to claim conformance are specified in ISO 19105: Geographic information — Conformance and Testing. In order to conform to this OGC™encoding standard, a standardization target shall implement the core conformance class, and choose to implement any one or more of the other conformance classes.

**Table 1** — Conformance classes related SensorML instances

|  |  |  |
| --- | --- | --- |
| **Conformance class** | **Description** | **Clause** |
| **Core Concepts** |  |  |
| [http://www.opengis.net/spec/SensorML/2.0/req/core](http://www.opengis.net/spec/SWE/2.0/req/core) | Core Concepts | A.1 |
| **Conceptual Models:** |  |  |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/core>Process | Abstract process | A.2 |
| http://www.opengis.net/spec/SensorML/2.0/req/model/simpleProcess | Non-physical simple process | A.3 |
| http://www.opengis.net/spec/SensorML/2.0/req/model/aggregateProcess | Non-physical aggregate process | A.4 |
| http://www.opengis.net/spec/SensorML/2.0/req/model/nonPhysicalProcess | Non-physical process | A.5 |
| http://www.opengis.net/spec/SensorML/2.0/req/model/physicalComponent | Physical process component | A.6 |
| http://www.opengis.net/spec/SensorML/2.0/req/model/physicalSystem | Physical process system | A.7 |
| http://www.opengis.net/spec/SensorML/2.0/req/model/physicalProcess | Physical process | A.8 |
| http://www.opengis.net/spec/SensorML/2.0/req/model/configurableProcess | Configurable Process | A9 |
|  |  |  |
| **XML Schema:** |  |  |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/core>Process | Core process | A.10 |
| http://www.opengis.net/spec/SensorML/2.0/req/xml/simpleProcess | Non-physical simple process | A.11 |
| http://www.opengis.net/spec/SensorML/2.0/req/xml/aggregateProcess | Non-physical aggregate process | A.12 |
| http://www.opengis.net/spec/SensorML/2.0/req/xml/nonPhysicalProcess | Non-physical process | A13 |
| http://www.opengis.net/spec/SensorML/2.0/req/xml/physicalComponent | Physical process component | A.14 |
| http://www.opengis.net/spec/SensorML/2.0/req/xml/physicalSystem | Physical process system | A.15 |
| http://www.opengis.net/spec/SensorML/2.0/req/xml/physicalProcess | Physical process | A16 |
| http://www.opengis.net/spec/SensorML/2.0/req/xml/configurableProcess | Configurable process | A.17 |

# Normative References

The following normative documents contain provisions which, through reference in this text, constitute provisions of document OGC 08-094. For dated references, subsequent amendments to, or revisions of, any of these publications do not apply. However, parties to agreements based on this document are encouraged to investigate the possibility of applying the most recent editions of the normative documents indicated below. For undated references, the latest edition of the normative document referred to applies.

* OGC 08-131r3 – The Specification Model – A Standard for Modular Specification
* ISO/IEC 11404:2007 – General-Purpose Datatypes
* ISO 8601:2004 – Representation of Dates and Times
* ISO 19103:2005 – Conceptual Schema Language
* ISO 19108:2002 – Temporal Schema
* ISO 19111:2007 – Spatial Referencing by Coordinates
* ISO 19115:2006 – All Metadata
* Unified Code for Units of Measure (UCUM) – Version 1.8, July 2009
* Unicode Technical Std #18 – Unicode Regular Expressions, Version 13, Aug. 2009
* The Unicode Standard, Version 5.2, October 2009
* W3C Extensible Markup Language (XML) – Version 1.0 (4th Edition), Aug. 2006
* W3C XML Schema – Version 1.0 (Second Edition), October 2004
* IEEE 754:2008 – Standard for Binary Floating-Point Arithmetic
* IETF RFC 2045 – Multipurpose Internet Mail Extensions (MIME) Part One: Format of Internet Message Bodies, November 1996
* IETF RFC 5234 – Augmented BNF for Syntax Specifications: ABNF

# Terms and Definitions

For the purpose of this document, the following terms and definitions apply:

* 1. Actuator

A type of transducer that converts a signal to some real-world action or phenomenon.

* 1. Aggregate Process

Composite process consisting of interconnected sub-processes, which can in turn be **Simple Processes** or themselves **Aggregate Processes**. A decription of an aggregate process should explicitly define connections that link input and output signals of sub-processes together. Since it is a process itself, an aggregate process also has its own inputs, outputs and parameters.

* 1. Coordinate Reference System (CRS)

A spatial or temporal framework within which a position and/or time can be defined. According to ISO 19111, a **coordinate system** that is related to the real world by a **datum**.

* 1. Coordinate System (CS)

According to ISO19111, a set of (mathematical) rules for specifying how coordinates are assigned to points. In this document, a Coordinate System is extended to be defined as a set of axes with which location and orientation can be defined.

* 1. Data Component

Element of sensor data definition corresponding to an atomic or aggregate data type

*Note: A data component is a part of the overall dataset definition. The dataset structure can then be seen as a hierarchical tree of data components.*

* 1. Datum

A means of relating a coordinate system to the real world by specifying the physical location of the coordinate system and the orientation of the axes relative to the physical object. For a geodetic datum, the definition may also include a reference ellipsoid that approximates the physical or gravitational surface of the planetary body. (Undefined in ISO 19111)

* 1. Detector

Atomic part of a composite **Measurement** **System**defining sampling and response characteristic of a simple detection device. A detector has only one input and one output, both being scalar quantities. More complex **Sensors***,* such as a frame camera, which are composed of multiple detectors, can be described as a detector group or array using a **System** or **Sensor** model.

* 1. Determinand

A Parameter or a characteristic of a phenomenon subject to **observation.** Synonym for **observable.** *[O&M]*

* 1. Feature

Abstraction of real-world phenomena [ISO 19101:2002, definition 4.11]

*Note: A feature may occur as a type or an instance. Feature type or feature instance should be used when only one is meant.*

* 1. Location

A point or extent in space relative to a **coordinate system**. For point-based systems, this is typical expressed as a set of n-dimensional coordinates within the **coordinate system**. For bodies, this is typically expressed by relating the translation of the origin of an object’s local **coordinate system** with respect to the origin of an external reference **coordinate system**.

* 1. Location Model

A model that allows one to position objects in one local **reference frame** relative to another **reference frame**.

* 1. Measurand

Physical parameter or a characteristic of a phenomenon subject to a **measurement,** whose value is described using a Measure (ISO 19103). Subset of **determinand** or **observable**. *[O&M]*

* 1. Measure (noun)

**Value** described using a numeric amount with a scale or using a scalar reference system  *[ISO/TS 19103]*. When used as a noun, measure is a synonym for physical quantity

* 1. Measurement

An **observation** whose result is a **measure** *[O&M]*

* 1. Measurement (verb)

An instance of a procedure to estimate the value of a natural phenomenon, typically involving an instrument or sensor. This is implemented as a dynamic feature type, which has a property containing the result of the measurement. The measurement feature also has a location, time, and reference to the method used to determine the value. A measurement feature effectively binds a value to a location and to a method or instrument.

* 1. Muliplexed Data Stream

A data stream that consists of disparate but well defined data packets within the same stream.

* 1. Observable, Observable Property

A parameter or a characteristic of a **phenomenon** subject to **observation.** Synonym for **determinand.** *[O&M]*  
  
A property of a phenomenon that can be observed and measured (e.g. temperature, gravitational force, position, chemical concentration, orientation, number-of-individuals, physical switch status, etc.), or a characteristic of one or more feature types, the value for which must be estimated by application of some procedure in an observation. It is thus a physical stimulus that can be sensed by a detector or created by an actuator.

* 1. Observation

Act of observing a property or phenomenon (ISO/DIS 19156, definition 4.10)

*Note: The goal of an observation may be to measure, estimate or otherwise determine the value of a property.*

* 1. Observation Procedure

Method, algorithm or instrument, or system of these which may be used in making an observation

[ISO/DIS 19156, definition 4.11]

*Note: In the context of the sensor web, an observation procedure is often composed of one or more sensors that transform a real world phenomenon into digital information, plus additional processing steps.*

* 1. Observed Value

A **value** describing a natural phenomenon, which may use one of a variety of scales including nominal, ordinal, ratio and interval. The term is used regardless of whether the value is due to an instrumental observation, a subjective assignment or some other method of estimation or assignment.  [O&M]

* 1. Orientation

The rotational relationship of an object relative to an external coordinate system. Typically expressed by relating the rotation of an object’s local coordinate axes relative to the axes of an external reference coordinate system.

* 1. Phenomenon

A physical state that can be observed and its properties measured.

* 1. Position

The location and orientation of an object relative to an external coordinate system. For body-based systems (in lieu of point-based systems) is typically expressed by relating the object’s local coordinate system to an external reference coordinate system. This definition is in contrast to some definitions (e.g. ISO 19107) which equate position to location.

* 1. Process

An operation that generates one or more outputs, based on one or more inputs, a set of parameters, and a methodology.

* 1. Process Method

Definition of the algorithm of a **Process***.*

* 1. Property

Facet or attribute of an object referenced by a name

[ISO/DIS 19143:2010]

*Example : Abby's car has the color red, where "color" is a property of the car instance, and “red” is the value of that property.*

* 1. Reference Frame

A coordinate system by which the position (location and orientation) of an object can be referenced.

* 1. Result

An estimate of the value of some property generated by a known procedure *[O&M]*

* 1. Sample

A representative part of the physical entity on which an observation is made.

* 1. Sensor

An entity capable of observing a phenomenon and returning an observed value. Type of observation procedure that provides the estimated value of an observed property at its output.

*Note: A sensor uses a combination of physical, chemical or biological means in order to estimate the underlying observed property. At the end of the measuring chain electronic devices often produce signals to be processed.*

* 1. Sensor Model

In line with traditional definitions of the remote sensing community, a sensor model is a type of Location Model that allows one to georegister or co-register observations from a sensor (particularly remote sensors). The sensor model characterizes the sensor sufficiently to allow registration of observations with a defined accuracy.

* 1. Sensor Data

List of digital values produced by a sensor that represents estimated values of one or more observed properties of one or more features.

*Note: Sensor data is usually available in the form of data streams or computer files.*

* 1. (Sensor) Platform

An entity to which can be attached sensors or other platforms. A platform has an associated local reference frame that can be positioned relative to an external coordinate reference frame and to which the reference frames of attached sensors and platforms can be positioned.

* 1. Physical System

An aggregate model of a group or array of process components, which can include detectors, actuators, or sub-systems. A **Physical System** relates an **Aggregate Process** to the real world and therefore provides additional definitions regarding relative positions of its components and communication interfaces.

* 1. Transducer

An entity that receives a signal as input and generates a modified signal as output. Includes detectors, actuators, and filters.

* 1. Value

A member of the value-space of a datatype. A value may use one of a variety of scales including nominal, ordinal, ratio and interval, spatial and temporal. Primitive datatypes may be combined to form aggregate datatypes with aggregate values, including vectors, tensors and images *[*[*ISO11404*](#ISO11404)*]*.

# Conventions

## Abbreviated terms

In this document the following abbreviations and acronyms are used or introduced:

CRS Coordinate Reference System

DN Digital Number

ECEF Earth-Centered Earth-Fixed

ECI Earth Centered Inertial

GPS Global Positioning System

ISO International Organization for Standardization

MISB Motion Imagery Standards Board

OGC Open Geospatial Consortium

SAS Sensor Alert Service

SensorML Sensor Model Language

SI Système International (International System of Units)

SOS Sensor Observation Service

SPS Sensor Planning Service

SWE Sensor Web Enablement

TAI Temps Atomique International (International Atomic Time)

uom Unit(s) of measure

UCUM Unified Code for Units of Measure

UML Unified Modeling Language

UTC Coordinated Universal Time

XML eXtended Markup Language

1D One Dimensional

2D Two Dimensional

3D Three Dimensional

## UML notation

The diagrams that appear in this standard are presented using the Unified Modeling Language (UML) static structure diagram. The UML notations used in this standard are described in the diagram below.




Figure 5.1 – UML Notation

## Table notation used to express requirements

For clarity, each normative statement in this standard is in one and only one place and is set in a **bold font** within the tabular format shown below. If the statement of the requirement is repeated for clarification, the “bold font” home of the statement is considered the official statement of the normative requirement. Individual requirements are clearly highlighted and identified throughout the document by using tables and URL identifiers of the following format:

|  |
| --- |
| Requirement |
| http://www.opengis.net/spec/SWE/2.0/req/{req-class-name}/{req-name} |
| **Req N. Textual description of requirement.** |

In this standard, all requirements are associated to tests in the abstract test suite in 0. The reference to the requirement in the test case is done by its URL.

Requirements classes are separated into their own clauses and named, and specified according to inheritance (direct dependencies). The Conformance test classes in the test suite are similarly named to establish an explicit and mnemonic link between requirements classes and conformance test classes. There are formally identified by URL and described within a tabular format as shown below:

|  |  |
| --- | --- |
| Requirements Class | |
| http://www.opengis.net/spec/SensorML/2.0/req/{req-class-name} | |
| Target Type | Description of standardization target type |
| **Dependency** | http://www.opengis.net/spec/SensorML/2.0/req/{req-class-name} |

Examples will be indicated using a grey text box and are considered to be informative rather than normative:

**Example**

This is an example text box that will include informative notes and examples.

# Requirements Class: Core Concepts (normative core)

|  |  |
| --- | --- |
| Requirements Class | |
| <http://www.opengis.net/spec/SensorML/2.0/req/core> | |
| Target Type | Derived Models, Encodings, and Software Implementations |

## Introduction

In SensorML, all components are modeled as processes. This includes components normally viewed as hardware, such as detectors, actuators, and physical processors (which are viewed as physical components) and sensors and platforms (which are viewed as physical systems). All components are modeled as processes that receive input and, through the application of an algorithm defined by a method and set parameter values, generate output. All such components can therefore participate in process networks (or aggregate processes). Aggregate processes are themselves processes with their own inputs, outputs, and parameters.

Hence, SensorML can be viewed as a specialized process description language with an emphasis on application to sensor data. Process descriptions in SensorML are agnostic of the environment in which they might be executed, or the protocol by which data is exchanged between process execution modules.

In order to support the use of SensorML within specialized applications (e.g. processing centers or image processing software), the SensorML models and encodings have been divided into several conformance classes. Thus if one wishes to use SensorML for computation processes only, the software only needs to conform to the requirements for non-physical processes. Similarly, by only adhering to the Simple Process conformance class, a piece of software can describe internal processes using SensorML while supporting chaining of these processes in a proprietary way.

However, all derived model and encodings based on SensorML must implement the core concepts of SensorML, regardless of whether they deal strictly with non-physical computational processes or sensor systems.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/core/core-concepts-used> |
| 1. All derived models or encodings shall correctly implement the modeling concepts defined in the core of this specification. |

## Process Definitions

In SensorML, all relevant components are modeled as processes, including both computation and physical processes (e.g. detectors, actuators, and sensor systems). Processes in SensorML are conceptually divided into two types: (1) those that are physical processes, such as detectors, actuators, and sensor systems, where information regarding their positions may be relevant, and (2) non-physical or “pure” processes which can be treated as merely mathematical operations or functions.

Fundamentally, a process is a physical or computational operation that may receive input and based on configurable parameters and a methodology, generate output.

**Example**

For a process representing the standard linear equation, x would be the input, m and b the parameters, y the output, and the equation y = mx + b would define the methodology.

For a detector, the input would typically be a physical stimulus (or observable property), the parameters might include a calibration curve and other factors that affect the measurement, and the output would be a digital number representing some quantity representation of that observed property.

Inputs and outputs may be digital numbers or physical stimuli (i.e. observable properties of the environment). Parameters can be variable or constant, but they don’t typically vary at the same frequency as the input values. In essence, however, parameters can be viewed as just another input into the process with the following exception. A parameter changes the state of a process but does not necessarily trigger an action. An input typically triggers the process to execute.

A process can consist of a single atomic operation, or an explicitly defined network of operations (e.g. an aggregate process or system).

Any process must have a definable method of operation. In the case of an aggregate process or physical system, the explicit description of the process components and the flow of data between them will itself serve as the process methodology.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/core/processes> |
| 1. The core model for a process shall define inputs, outputs, parameters, and methodology of that process. |

Any process description must provide a unique ID that can be used for discovery of that process and for retrieving the definition of that process.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/core/uniqueID> |
| 1. The core model for a process shall include a unique ID for distinguishing that process from all others. |

To be useful, the core process model shall include metadata about the process that aid in identification, discovery, and qualification of the process but do not themselves affect the execution of the process.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/core/metadata> |
| 1. The core model for a process shall include metadata that support identification, discovery, and qualification of the process. |

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/core/execution> |
| 1. The metadata descriptions for a process shall not be required for successful execution of that process. All information required for execution of a simple process shall be contained within the inputs, outputs, parameters, and methodology descriptions of the process. |

Process definitions can support general representations of a process or a specific instance of a process.

**Example**

A general process for the linear equation would define the allowable inputs, outputs, and parameters. A specific instance of the process might define constant values for the parameters.

An example of a general physical process would be the manufacturer’s description of the characteristics and configurable options for a particular model of a sensor (i.e. one that describes the common characteristics of all instances of that model of sensor). The description of a specific instance of that model of sensor would include information that is relevant to that particular instance of the sensor (e.g. serial number, owner’s name, location, etc.).

# UML Conceptual Models (normative)

This standard defines normative UML models with which derived encoding models as well as all future separate extensions should be compliant. The standardization target type for the UML requirements classes defined in this clause is thus a software implementation or an encoding model that directly implements the conceptual models defined in this standard.

## Package Dependencies

The packages defined by the SensorML Model and their dependencies are shown in figure below:




Figure 7.1 – Internal Package Dependencies

SensorML also has dependencies on several external packages defined within other standards, namely GML 3.2, ISO 19103, ISO 19108, ISO 19111, and ISO 19115, as described below.

### Dependency on GML Feature Model and ISO TC 211 Models

A process represents a feature type as defined by the ISO General Feature Model and is thus modelled as an instance of the <<metaclass>> *GF\_FeatureType* (ISO 19109:2006). These models are further refined within the GML 3.2 standard (ISO 19136) which will provide the basis for XML encodings in the following section 8 of this specification document. This association of SensorML process with GML primarily brings recognition of SensorML processes as features and provides important identity properties.




Figure 7.2 – External Package Dependencies – GML

The base feature classes in GML from which all processes in SensorML derive include AbstractGML and AbstractFeature, as shown in the figure below:




Figure 7.3 – Models for dependent GML Feature classes

SensorML is dependent on ISO 19111 Models for Referencing by Coordinates, as well as ISO 19108:206 for Temporal Schema. While the Temporal Schema classes TM\_Instant and TM\_Period are used within the core SensorML model for Abstract Process, the ISO 19111 classes for SC\_EngineeringCRS, and TM\_TemporalCRS are only used in Physical Processes.




Figure 7.4 – External Package Dependencies – ISO TC 211

The SensorML specification utilizes the ISO 19115 models for common metadata properties such as citations, online resources, responsible party, and constraints. While Version 1.0 of SensorML defined encoding based on the ISO 19115 models, this version utilizes these models directly.




Figure 7.5 – ISO 19115 Models for dependent classes.

### Dependency on SWE Common Data Models

In particular, SensorML is heavily dependent on the SWE Common Data Model standard for defining inputs, outputs, and parameters, as well as for specifying characteristics, capabilities, interfaces, and event properties. The SWE Common Data Models, which were originally defined within the version 1.0 SensorML specification, are in version 2.0 defined as a separate specification and are utilized throughout the SWE family of encoding and web service specifications.




Figure 7.6 – External Package Dependencies – SWE Common Data

The SWE Common specification provides a flexible yet robust means of defining data types and data values, including support for simple data types such as *Quantity*, *Boolean*, *Category*, *Count*, *Text*, and *Time*, as well as aggregate data such as *DataRecord*, *DataArray*, *Vector*, and *Matrix*. Additionally, SWE Common supports the concept of *DataChoice,* which will is used by SensorML to describe multiplexed messages in data streams and configurable options for processes and physical systems.

The data models in SWE Common provide additional properties to those provided by basic data types, including units of measure (uom), quality indications, allowable constraints, significant digit counts, and in particular, the meaning (semantics) of a data component. Both simple and aggregate data components in SWE Common allow for unambiguous definition of that data component through a resolvable link to an online dictionary or ontology. The definition of the SWE Common Data Models can be found in OGC 08-094r1.

The main objective of SWE Common Data Models is to achieve interoperability, first at the syntactic level, and later at the semantic level (by using ontologies and semantic mediation) so that sensor data can be better understood by machines, processed automatically in complex workflows, and easily shared between intelligent sensor web nodes.

SensorML depends heavily on the *AbstractDataComponent* element defined in SWE Common. This element serves as the base component from which all relevant data types in SWE Common are derived, including *Quantity*, *Count*, *Category*, *Boolean*, *Text*, *DataRecord*, *DataArray*, *Vector*, *Matrix*, and *DataChoice*. *AbstractDataComponent* thus serves as a substitution group that any of these data types can satisfy. *AbstractSWEIdentifiable* will serve as the basis for the *ObservableProperty* element defined in this specification (Section 7.2.1).

The model for the SWE Common *AbstractDataComponent* is given in the figure below:




Figure 7.7 –Models for dependent SWE Common AbstractDataComponent class.

### Relationship to Observations and Measurements (O&M)

Conceptual models for Observations and Measurements are provided by ISO 19156, which also provides models for sampling feature types. XML Schema encodings of these models are provided by the OGC Observations and Measurements XML Implementation Document (OGC 10-025). The model for *Observation* defines a procedure of type *AbstractFeature* which references or describes the origin of the observation (i.e. how the observation came to be).

SensorML has an association to the OGC O&M models but no direct dependencies on them. The result of a SensorML process is typically considered to be an observation result if it is measuring or deriving some value of a physical property or phenomenon. Thus, the *output* values described in SensorML and resulting from a sensor or process may be packaged in an O&M *Observation* object, or provided as a SWE Common *DataStream*. Inversely, the *procedure* property within an *Observation* instance may reference a SensorML description of the measurement process.

## Requirements Class: Core Abstract Process

|  |  |
| --- | --- |
| Requirements Class | |
| <http://www.opengis.net/spec/sensorML/2.0/req/model/coreProcess> | |
| Target Type | Derived Models, Encodings, and Software Implementations |
| Dependency | [**http://www.opengis.net/spec/SensorML/2.0/req/core**](http://www.opengis.net/spec/SensorML/2.0/req/core) |
| Dependency | [**http://www.opengis.net/spec/SWE/2.0/req/uml-block-components**](http://www.opengis.net/spec/SWE/2.0/req/uml-block-components) |
| Dependency | ISO 19115:2006 (All Metadata) |
| Dependency | ISO 19136 (GML) |
| Dependency | OGC SWE Common Data 2.0 |

All major classes in SensorML are based on a process model, as presented in the core concepts. Processes are features as defined in ISO 19109:2006 and modelled in GML 3.2. SensorML also supports interoperable discovery, identification, and qualification of these processes through the definition of a standard collection of metadata.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/coreProcess/dependency-core> |
| 1. An encoding or software passing the “Core Abstract Process” model conformance class shall first pass the “Core Concepts” requirements test class. |

### ObservableProperty

An *ObservableProperty* is a physical property of a phenomenon that can be observed and measured (e.g. temperature, gravitational force, position, chemical concentration, orientation, number-of-individuals, physical switch status, etc.), or a characteristic of one or more feature types, the value for which must be estimated by application of some procedure in an observation. It is thus a physical stimulus that can be sensed by a detector or created by an actuator.

Example: The *ObservableProperty* element allows one to reference a measurable property of a phenomenon or feature for detector inputs or actuator outputs. For example, the temperature of the atmosphere is an ObservableProperty. Before measurement, it is simply a property of the atmosphere that can be defined and measured. After measurement by a detector, the temperature may be represented as a Quantity with units of measure, a value, and an indication of our degree of confidence in the measurement.

*ObservableProperty* is derived as a concrete instance of the SWE Common *AbstractSWEIdentifiable* and adds the *definition* property to this model. It will be used as a potential input (e.g. for detectors), output (e.g. for actuators), and for parameters (e.g. for a sensor whose measurement algorithm varies with fluctuations of atmospheric pressure on a diaphragm).

In *ObservableProperty* the phenomenon property will be defined by reference using the *definition* attribute. The *definition* attribute value will reference a property defined within a dictionary or ontology. An *ObservableProperty* may also include a name and a description. However, unlike the simple data types in SWE Common, an *ObservableProperty* does NOT include uom, quality, or constraints, since these are typically characteristics of the measuring procedure and not properties of the observable phenomenon itself.

### DescribedObject

As shown in the UML model below, the *DescribedObject* class provides a specific set of metadata for all process classes in SensorML. Since *DescribedObject* is itself derived from GML *AbstractFeature*, all processes in SensorML are themselves features, which conforms to the conceptual models for processes as stated in Section 6.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/coreProcess/gmlDependency> |
| 1. *DescribedObject* shall derive from the GML base class, *AbstractFeature*, and is thus modeled as a feature with well-defined metadata properties. Any model or encoding derived from *DescribedObject* shall thus be of type *featureType*. |

The GML *AbstractFeature* inheritance provides a unique ID, and support for multiple names and a description. The unique ID in SensorML will be supported by a single *gml:identifier* property inherited from GML *AbstractFeature*.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/coreProcess/uniqueID> |
| 1. A single, required *gml:identifier* property inherited from GML *AbstractFeature* shall be used to provide a unique ID for the *DescribedObject*. |

Metadata about each process is essential to supporting identification, discovery, and qualification of the process. Metadata is provided by the base class, *DescribedObject*, from which *AbstractProcess* is derived. While these metadata may provide relevant information to understand quality of output from the process, the values of properties within the *DescribedObject* should not be required for execution of the process. The model for the *DescribedObject* is shown in Fig. 7.8., while the models for the individual property values are provided in either Fig. 7.9 or in the ISO 19115 models in Fig. 7.5.

The DescribedObject includes several descriptive properties that support rapid discovery (*keywords*, *identification*, and *classification*), constraints (*validTime*, *securityConstraints*, *legalConstraints*), qualification (*characteristics* and *capabilities*), references (*contacts* and *documentation*), and *history*. These are each grouped in lists, which provide for easy seaparation and parsing of these properties.

#### Extension Property

The *extension* property allows one to add domain or community-specific content to a *DescribedObject* instance. This might include, for example, security taggings, vendor or community-specific metadata, or information encoded in other models or schema. Extension properties must exist in a separate namespace and SensorML-compliant software is not required to understand or utilize the information contained within the extension property.

The constraints on the *extension* property include: (a) the *extension* model must be defined in a separate namespace, (b) the information added by the *extension* model must not be required for execution of the process, and (3) SensorML-compliant parsers may parse and utilize the information within these extensions but they are not required to do so in order to be compliant to the SensorML standard.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/coreProcess/extensionIndependence> |
| 1. Models inside of the extension property must exist within a namespace other than SensorML. |

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/coreProcess/extensionRestrictions> |
| 1. Models inside of the extension property must not be required for execution of the process and shall not alter the execution of the process. |




Figure 7.8 – DescribedObject with Metadata Properties




Figure 7.9 – Models for Metadata Elements

#### Keywords

Keywords provide a simple means of discovery using short tokens that may be recognized by the general audience or specific communities. Keywords are unqualified terms in that they are not necessarily required to be related to a specific codespace or ontology, as are classifiers and identifiers. A *DescribedObject* can have multiple *keyword* properties enabling lists of keywords from different *codespace* references.

#### Identifiers

The identifier property takes a Term as its value. The element Term has a definition attribute that specifies in this case the type of identifier, while the *codeSpace* attribute specifies that the value of the identifier is according to the rules or enumerations of a particular authority. For example, an identifier with a *definition* of “http://sensors.ws/def/tailNumber” might take “N291PV” as its *value* based on the *codespace* of a US Air Force rules dictionary. Other possible definitions for identifiers might include, for example, shortName, longName, acronym, missionID, processorID, serialNumber, manufacturerID, or partNumber. The *identification* properties should be considered as information suitable for the discovery applications.

#### Classifiers

The classifier property provides a list of possible classifiers that might aid in the rapid discovery or organization of processes, sensors, or sensor systems. Definitions for a classifier Term might include, for instance, sensorType, observableType, processType, intendedApplication, or missionType. The classifier properties should be considered as information suitable for the discovery and categorization applications.

#### Security Constraints

The model for specification of security constraints shall be based on external security models, such as the Security Banner Marking model of the Intelligence Community Information Security Marking (IC ISM) Standard. The *securityConstraints* property takes a value of *xs:Any* which allows various communities and countries to utilize their standard XML encoding for security tags. This security constraint is for the overall document. As will be discussed in the XML encoding, extension points provided with SWE Common Data elements will allow security tagging for individual properties or property aggregates.

#### Valid Time Constraint

The validTime property indicates the time instance or time range over which this process description is valid. Time constraints are important for processes in which parameter values or operation modes may change with time, or instrument deployment times change.

#### Legal Constraint

The legalConstraints property is based on ISO 19115 and specifies whether such legal and ethical considerations as privacy acts, intellectual property rights, copyrights, or scientific publication ethics apply to the process description and its use.

#### Capabilities

The *capabilities* property is intended for the definition of properties that further qualify the input or output of the process, component, or system for the purpose of discovery. For example, a particular remote sensor on a satellite might measure radiation between a certain spectral range (e.g. 700 to 900 nanometers) at a particular ground resolution (e.g. 5 meter), and with a typical spatial repeat period (e.g. 3.25 – 4.3 days). Alternatively, a particular process might have certain quality constraints. Any process may have certain limits (e.g., operational and survivable limits), based on physical or mathematical conditions. Once a user has identified candidate sensors or processes based on the classifiers described above, the capabilities parameters might prove useful for further filtering of processes or sensor system during this discovery stage. The *capabilities* properties should be considered as information suitable for the discovery process.

These properties are defined using one or more SWE Common *DataRecord* elements.

#### Characteristics

A physical or non-physical process may have *characteristics* that may not directly qualify the output. For example, a component may have certain physical measurements such as dimensions and weight, and be constructed of a particular material. A component may have particular power demands, or anticipated lifetime. The *characteristics* properties may or may not be considered as information suitable for the discovery process.

These properties are defined using one or more SWE Common *DataRecord* elements.

#### Contacts

Contact information can provide access to manufacturers, system experts, equipment owners, or any other persons responsible in some way for design, deployment, maintainance, or additional information regarding the *DescribedObject*. The *member* property within the *ContactList* takes the ISO 19115 classes *CI\_ResponsibleParty* as its values.

#### Documentation

Documentation can be provided which provides further clarification about the *DescribedObject*. This might include technical manuals, manufacturer brochures, journal references, or theoretical-basis documents. The *DocumentList* *member* property takes the ISO 19115 *CI\_OnlineResource* as it value.

#### History

Within SensorML, the history of a process can be provided through a collection of *Event* objects. These are provided within an EventList that serves as the value of the history property. Events might for instance, specify calibration or maintenance history of a sensor, changes to an algorithm or parameter within a computational process, or deployment and maintenance events.




Figure 7.10 – Model for history events

### AbstractProcess

As discussed in the Core Concepts, the major elements of SensorML are modelled as physical and non-physical processes. All SensorML process elements shall derive from *AbstractProcess,* shown in Figure 7.11. The class *AbstractProcess* itself derives from the *DescribedObject* class and thus inherits a wide range of optional metadata supporting discovery, identification, and qualification and an option for domain and community-specific extensions. In addition to the metadata provided by *DescribedObject*, the *AbstractProcess* includes the properties of *inputs*, *outputs*, and *parameters*, as required by the process model defined in the Core Concepts, as well as the properties *typeOf*, *featureOfInterest*, *configuration*, and *modes* which will be discussed below.




Figure 7.11 – UML models for DescribedObject and AbstractProcess

#### Inputs, Outputs, and Parameters

As discussed in the Core Concepts, any process can have *inputs*, *outputs*, and *parameters*. Processes typically receive input and based on the parameter settings and methodology, generate output. Some processes, such as detectors, receive physical stimulus as input and generate digital numbers as output. In such cases, the input would be represented as an *ObservableProperty*, and the output as a *DataComponent* (e.g. a *Quantity*). If this output is encoded and accessible directly, then the output could be represented as a *DataInterface*.

Example: A digital thermometer is stimulated by an observable property of the environment (temperature), which is modelled as its input (ObservableProperty), and outputs a digital number (Quantity) that represents a measure of that property.

Thus, an *AbstractProcess* model supports the *inputs*, *outputs*, and *parameters* properties in conformance with the Core Concepts. These properties can accept *ObservableProperty* or SWE Common elements *AbstractDataComponent* or *DataStream* as their values. Classes derived from *AbstractDataComponent* include *Quantity*, *Count*, *Category*, *Boolean*, *Text*, and *Time*, as well as ranges and aggregates of these simple data types.




Figure 7.12 – UML models for process inputs, outputs, and parameters.

The core process model will utilize the SWE Common Data Models for defining inputs, outputs, and parameters, as well as for other metadata properties. SensorML models are required to support the SWE Common Data Model up to the Block Components Requirements Class, but many instances of SensorML will find ALL conformance levels of SWE Common Data to be useful, including binary encodings.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/coreProcess/SWE-Common-dependency> |
| 1. Any derived model or encoding for process shall utilize *ObservableProperty* or SWE Common Data Components as values for inputs, outputs, and parameters, and shall at a minimum conform to the SWE Common Data “Block Components Package” class (<http://www.opengis.net/spec/SWE/2.0/req/uml-block-components>). |

The input, output, or parameters of many processes include multiple values, possibly of different data types, that are tightly related to one another. Sometimes referred to as tuples or records, these data aggregates can consist of values that are perhaps meaningless without the other associated values (e.g. the coordinates within a spatial reference system), or provide a more complete understanding because of their association with one another (e.g. a set of measured values taken by a sensor at a given time). Such data shall be modelled as an aggregate data type, such as a data reord, vector, or matrix.

Example: The location of a dynamic object can be specified through the aggregate values of time, latitude, longitude, and altitude. In such cases, the expression of one of the values separate from the others is meaningless or less complete than the expression of these values as a set or aggregate.

Example: Weather stations often express a set of measurements of the atmosphere as a single record that might include for instance temperature, pressure, relative humidity, cloudiness, wind speed, and wind direction. These would be considered a tuple of values that provides a more complete picture of the environment at a particular time.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/coreProcess/aggregateData> |
| 1. Multiple input, output, and parameter values that are tightly related with one another shall be modelled as SWE Common Data aggregate data types, such as *DataRecord*, *Vector*, or *Matrix*. |

#### Feature of Interest

Most sensors and many non-physical processes have been deployed or implemented with a focus on one or more features of interest. For example, the features of interest of an installed web camera might include a particular building, a particular street, or a general area of observation surrounding the camera. Features of interest for other sensors might include the Gulf of Mexico, a particular drilling well, the atmosphere surrounding a particular weather station, a particular patient, or a particular automobile. Features of interest for a model or other process might include a particular river basin, a particular toxic plume release, or a particular metropolitan area.

Within SensorML, the primary purpose of including a *FeatureOfInterest* property for *AbstractProcess* is to support discovery as well as to further clarify the intended purpose of the physical or non-physical process.

#### Inheritance, Extension, and Configuration

SensorML supports the concepts of inheritance, extension, and configuration. In other words, generalized base processes can be described in SensorML and then that description can be augmented or further constrained by one or more separate descriptions. Thus, a single, generalized description of a physical or non-physical process can serve as a basis for one or many more specific process descriptions. This provides support for more simple and concise process descriptions while also providing the ability for the user or application to “drill down” to greater and greater detail as desired.

The inheritance model will support two cases:

* 1. Simple inheritance – the specific process description provides only additional information to the description of the general process, without modifying or restricting any property values of the general process.
  2. Configuration – the specific process description is able to set or restrict property values within the allowable range provided by the general process description, as well as provide additional information.

The key to inheritance, extension, and configuration of a process lies in the *typeOf* property, by which a specific process can reference its more general base process. The *typeOf* property takes as its value any process model derived from *AbstractProcess*. This will be “by-reference-only” meaning that the value must be in the form of a resolvable link to another process instance.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/coreProcess/typeOf> |
| 1. A process that is a specific instance of another process shall reference the more general process through its *typeOf* property. The value of the *typeOf* property shall be a resolvable link to an instance of a process derived from *AbstractProcess*. |

##### Simple Inheritance

In the simple inheritance model, a process (referred to as the “specific process”) inherits and augments information from another process (referred to as the “general process”).

Example: An Original Equipment Manufacturer (OEM) provides a description of a particular model of their sensor that would define inputs, outputs, and parameters, as well as perhaps capabilities, characteristics, manufacturer contact information and documentation relevant to that model. Thousands of sensors of this model type may of course be manufactured and sold by the OEM.

When one purchases and deploys an instance of that model of sensor, the owner can then reference the OEM’s description of the model and provide additional information that’s specific to his specific instance of the sensor. Additional information might include, for example, serial number, owner’s contact information, the sensor’s location, calibration data, and the interface description for accessing the data.

The simple inheritance model is fully supported in the Core Process conformance class and will be supported solely through the use of the *typeOf* property within the specific process. The *typeOf* property within the specific process will reference the general process through a resolvable reference.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/coreProcess/simpleInheritance> |
| 1. A process instance that references another process through the *typeOf* property, but does not include the *configuration* property, shall inherit properties of the referenced process through simple inheritance. The complete description of that process is thus the addition of information from both process descriptions. |

##### Support for Configurable Processes

A configurable process is one that includes options or choices that can be selected, restricted, or enabled during deployment, operation, or execution of that process.

Example: An Original Equipment Manufacturer (OEM) can provide a description of a particular model of their sensor that would define inputs, outputs, and parameters, as well as perhaps capabilities, characteristics, manufacturer contact information and documentation relevant to that model. In addition, the OEM enables an individual instance of that model of sensor to be configured by providing options for setting parameter values, setting modes, or choosing a particular interface. Thousands of sensors of this model type may of course be manufactured and sold by the OEM.

When one purchases and deploys an instance of that model of sensor, the owner can then reference the OEM’s description of the model and provide additional information that’s specific to that particular instance of the sensor. In addition, the owner can configure the sensor by setting values, selecting modes, and enabling particular interfaces. These settings would be provided in the instance description.

The configuration model will utilize both the *typeOf* and *configuration* properties. The *typeOf* property references the more general process as with simple inheritance, while the *configuration* property provides a means to further restrict the options and allowed values for the specific process. The configuration property in the *AbstractProcess* takes an *AbstractSettings* class as its value. A concrete implementation of a *Settings* class will be provided in a later Conformance Clause.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/coreProcess/configuration> |
| 1. A process instance that references another process through the *typeOf* property, and further restricts options or allowed values provided in the referenced process, shall specify those restrictions through the *configuration* property. |

## Requirements Class: Simple Process

|  |  |
| --- | --- |
| Requirements Class | |
| <http://www.opengis.net/spec/sensorML/2.0/req/model/simpleProcess> | |
| Target Type | Derived Models, Encodings, and Software Implementations |

Simple process is derived from abstract process model, as presented in Clause 7.2.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/simpleProcess/dependency-core> |
| 1. An encoding or software passing the “Simple Process” model conformance class shall first pass the “Abstract Process” requirements test class. |

### Simple Process Definition

A simple process is a process that, for whatever reason, is considered indivisible. That is, there is no intent to further divide the process description into an aggregation of sub-processes. While the process method may describe several steps within the algorithm, the actual execution of this process is expected to occur as a single modular unit.

Often simple processes are computational processes that can be executed with an associated piece of software. Simple processes are often one component of a physical or non-physical aggregate process.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/simpleProcess/definition> |
| 1. A process shall be considered a “simple process” if it provides a processing function with well-defined inputs and outputs, if there is no intent to further divide the process description into subprocess components, and if knowledge of its physical location is unknown or of no importance. |

The *SimpleProcess* model, as shown in Fig. 7.13, is a concrete instantiation of the *AbstractProcess* model. The *SimpleProcess* requires a method description.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/simpleProcess/method> |
| 1. Any derived model or encoding for simple process shall include a mandatory *method* property for identifying and describing the execution methodology. |




Figure 7.13 – Model for Simple Process

### Process Method Definition

The *ProcessMethod* provides a description of the methodology used by the process to execute and generate output based on the input and parameter values. This includes a textual description, as well as an optional description of the algorithm in an appropriate format (e.g. mathML) and optional references to particular executable implementations.

The *ProcessMethod* definition should be sufficient to allow one to understand how input values are converted to output values, given a particular set of parameter values, and be able to write software that is capable of executing this process.

A *ProcessMethod* description may be protected by security or legal constraints, which would purposely prevent access to the method description as well as restrict knowledge of the methodology to authorized personnel only. However, regardless of access restrictions, a *ProcessMethod* should always be able to be referenced and identified by a unique identifier.




Figure 7.14 – Model for ProcessMethod

## Requirements Class: Aggregate Process

|  |  |
| --- | --- |
| Requirements Class | |
| <http://www.opengis.net/spec/sensorML/2.0/req/model/aggregateProcess> | |
| Target Type | Derived Models, Encodings, and Software Implementations |

Simple process is derived from abstract process model, as presented in Clause 7.2.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/aggregateProcess/dependency-core> |
| 1. An encoding or software passing the “Aggregate Process” model conformance class shall first pass the “Abstract Process” requirements test class. |

### Aggregate Process Definition

An aggregate process is a collection of autonomous component processes with an explicit mapping of the data flow between these processes. Components of an aggregate process can be simple atomic processes or be aggregate process themselves. Aggregate processes can include both physical and non-physical components.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/aggregateProcess/definition> |
| 1. A process shall be considered an “aggregate process” if it provides a processing function with well-defined inputs and outputs, if there is intent to further divide the process description into subprocessing components, and if knowledge of its physical location is unknown or of no importance. |

|  |
| --- |
| Requirement |
| [http://www.opengis.net/spec/SensorML/2.0/req/model/aggregateProcess/components](http://www.opengis.net/spec/SensorML/2.0/req/model/processChain/components) |
| 1. Any derived model or encoding for an aggregate process shall include one or more component processes and explicit linking of data flow between these components. |

In SensorML, an aggregate process is agnostic to the execution engine that may perform the actual execution of individual component processes and manage the execution sequencing and the flow of data between the components. Also, while it is possible in SensorML to more explicitly define the data encoding if desired by using the encoding specifications defined in the SWE Common Data Specification, SensorML is typically agnostic to the protocol and format of data flowing between processes.

This provides significant flexibility as to where and how a SensorML-defined aggregate process is executed. While the ProcessMethod explicitly defines the algorithm for executing an atomic process, the actual execution of that algorithm and the management of data flow between processes can be handled by any software system able to parse a SensorML-defined aggregate process and sequence the execution of the processes.

A SensorML-defined process component or aggregate processes can be executed through web services, within the CPU of a laptop, mobile device, or supercomputer, or a mix of these. Furthermore, a SensorML-defined aggregate process can be executed wherever desired, be it at a large data or computation center, within a visualization and analysis client on a laptop, or on-board a sensor or actuator system. Thus, SensorML provides one the choice to either bring the process to the data or bring the data to the process.

The model for *AggregateProcess* is shown in the figure below. *AggregateProcess* extends the *AbstractProcess* model and adds one or more process components and explicit linking of data flow between these components. The *component* property takes any component derived from *AbstractProcess* as its value. Component process descriptions can be provided inline or by reference.

The derivation from *AbstractProcess* and *ProcessType* means that an *AggregateProcess* instance itself has its own inputs, outputs, and parameters, as well as identification and possible metadata.




Figure 7.15 – Model for Aggregate Process

## Requirements Class: Non-Physical Processes

|  |  |
| --- | --- |
| Requirements Class | |
| <http://www.opengis.net/spec/sensorML/2.0/req/model/nonPhysicalProcess> | |
| Target Type | Derived Models, Encodings, and Software Implementations |

Derived models and software systems that are only concerned with pure calculations, modeling, or post-processing of observations may conform to the Non-Physical Process Requirements Class for SensorML. Such systems would (1) utilize SensorML *SimpleProcess* for describing atomic processes that are perhaps each associated with a particular computational class or coherent piece of software, and (2) use SensorML *AggregateProcess* for explicitly defining the reconfigurable chaining of these processes into a more complex workflow, script, or algorithm.

However, to be conformant to the Non-Physical Process Requirement, the system must properly support both the simple process and aggregate process requirements defined in previous sections.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/nonPhysicalProcess/supports> |
| 1. A derived model or encoding supporting non-physical processes shall meet the requirements for both simple process (clause 7.4) and aggregate process (clause 7.5). |

## Requirement Class: Physical Component

|  |  |
| --- | --- |
| Requirements Class | |
| <http://www.opengis.net/spec/sensorML/2.0/req/model/physicalComponent> | |
| Target Type | Derived Models and Encodings |

In the context of SensorML, physical processes are those where knowledge of the temporal-spatial position of the physical process, itself, is important. Examples of physical processes include detectors, actuators, sensor systems, and actuator systems. Such processes typically, but not always, involve interactions beween a real-world domain (or environment) and a digital domain.

For example a detector or sensor system typically senses an environmental stimulus and provides a digital number representing the measure of a property of that environment (e.g. temperature). Likewise, an actuator receives a digital number and based on its values causes an action in the real-world environment.

Because physical processes typically interact with the real-world environment, the position (location and orientation), as well as perhaps the dyamic state (velocity and acceleration), are usually of importance. We wish to either measure an observable property at a particular location in the environment or we wish to affect a physical action at a particular place in the environment. Thus, the position where the physical process measures or acts becomes important.

### Abstract Physical Process Defined

The *AbstractPhysicalProcess* model is derived from *AbstractProcess* and thus includes the metadata and properties of a core process. Additionally, *AbstractPhysicalProcess* supports additional properties that allow one to define spatial and temporal coordinates for the physical process device.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/physicalComponent/dependency-core> |
| 1. An encoding or software passing the “Physical Component” model conformance class shall first pass the “Abstract Process” requirements test class. |

The model for *AbstractPhysicalProcess* is shown in Figure 7.16 below. The additional properties of the *AbstractPhysicalProcess* will be discussed in subsequent clauses.




Figure 7.16 – Model for Physical Process Component

#### attachedTo Property

A physical process (“child process”) may be attached to another physical process (“parent process”) such that the movement of the parent process affects the position of the child process. The *attachedTo* property provides a reference from the attached process to the process to which it is attached.

Example: A video camera is attached to a gimbal that allows rotation of the camera to view a 360o area surrounding the camera. In such a case, the camera is said to be attached to the gimbal. Both are physical processes (the camera, a sensor; the gimbal, an actuator). The video camera description should thus use the *attachedTo* property to reference the gimbal description.

#### Position and Spatial Reference Frames

In this specification, the position or dynamic state of a physical object is defined as a relationship of the reference frame of the object to some external reference frame.

A reference frame is defined by its origin and its axes, which are described relative to the physical object itself and not relative to any relationship of the object to some external frame. The relationship of that object’s reference frame to an external reference frame defines by the position or dynamic state of the object. The models for reference frames and spatial position are provided in Figure 7.17.

Example: The origin of an airplane’s spatial reference frame can be defined as the being at the center of the Inertial Navigation Unit main gyro. The axes can be defined by the following statements: “X is along the symmetric axis of the airplane’s fuselage from the gyro to the nose of the airplane (along the platform roll axis of the airplane), Z is perpendicular to X and toward the belly of the airplane (along the yaw axis of the aircraft), and Y is Z cross X (in the direction of of the right wing and along the pitch axis of the airplane)”.

The location of this aircraft can then be given as the spatial relationship of the origin of this reference frame to some external reference frame (e.g. Earth-Centered-Earth-Fixed XYZ or latitude-longitude-altitude). Likewise, the orientation of the aircraft can be specified as the angular relationship of the axes of its reference frame to the axes of some external reference frame (e.g. ECEF or North-East-Down).




Figure 7.17 – Models for ReferenceFrame and PositionUnion

In this specification, position is defined as the combination of location and orientation. Location is the spatial relationship of the origin of the object’s spatial reference frame to some external reference frame (which must be designated). The orientation of an object is the angular relationship between the axes of the object’s reference axes to those of some external reference frame. The dynamic state of an object can include its location, orientation, linear velocity, angular velocity, and the various derivatives of linear and angular velocity (e.g. linear and angular acceleration).

An external reference frame can include another object’s reference frame (e.g. the reference frame of a ship) or a geographic reference frame (e.g. WGS84 latitude-longitude-altitude).

The *PositionUnion* class provides various means of specifying the location, position, or dynamic state of an object. These will be described in more detail in the appropriate XML encoding section, but the following rules apply to the SensorML models.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/physicalComponent/byPointOrLocation> |
| 1. Specification of position byPoint or byLocation shall specify the location of the origin of the object’s reference frame relative to a well-defined and specified external reference frame. |

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/physicalComponent/byPosition> |
| 1. Specification of position byPosition shall specify, using two Vectors, the location and orientation of the object’s reference frame relative to a well-defined and specified external reference frame. |

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/physicalComponent/byTrajectory> |
| 1. Specification of position byTrajectory shall specify, at a minimum, the time-tagged location of the object’s reference frame relative to a well-defined and specified external reference frame, but may also include the orientation, linear and angular velocity, and any derivatives of the linear and angular velocity of the object’s reference frame. |

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/physicalComponent/byProcess> |
| 1. Specification of position byProcess shall specify SensorML-modeled process whose output provides, at a minimum, the time-tagged location of the object’s reference frame relative to a well-defined and specified external reference frame, but may also include the orientation, linear and angular velocity, and any derivatives of the linear and angular velocity of the object’s reference frame. |

#### Temporal Reference Frames

Just as spatial position must be related to a spatial reference frame, time must also be related to a temporal reference frame. Temporal reference frames can include a particular calendar, a particular time of day reference frame, or a relative frame such as seconds past mission start time or seconds past a predefined epoch (e.g. 1972-01-01T00:00:00.0).

A temporal reference frame can be defined within a physical process and is particularly useful if the component is a process that outputs its own measure of time. *TemporalReferenceFrame* is derived from *TM\_TemporalCRS*. (???)

### Physical Component Defined

Any processing device can be considered a physical component, if it provides a processing function with well-defined inputs and outputs, if there is no intent to further divide the device description into component subprocesses, and if knowledge of its physical location is useful. Such devices could include, but not be limited to, detectors, actuators, reflectors, electrical components (e.g transformers, capacitors, resistors), or perhaps even computational units (when knowing their location in a computational facility is helpful).

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/physicalComponent/definition> |
| 1. A process shall be considered a “physical component” if it provides a processing function with well-defined inputs and outputs, if there is no intent to further divide the device description into subprocess components, and if knowledge of its physical location is of importance. |

As shown in the models of Figure 7.16, the *PhysicalComponent* class is a concrete instantiation of an *AbstractPhysicalProcess* that adds the *method* property, which takes a *ProcessMethod* as its value. *ProcessMethod* was defined earlier in clause 7.3.2.

## Requirement Class: Physical System

|  |  |
| --- | --- |
| Requirements Class | |
| <http://www.opengis.net/spec/sensorML/2.0/req/model/physicalSystem> | |
| Target Type | Derived Models and Encodings |

A physical system is an aggregate process where the location of the process is known and of importance. Sensor and actuator systems (e.g. machines and robots) are typically physical systems that perform a particular feat through the coordinated actions of both physical and non-physical subprocesses. Even though a sensor system’s overall application is to sense something in the environment, the system itself can consist of sensing components (e.g. detectors and sensing subsystems), action (e.g. actuators and robotic subsystems), and computational components.

Example: A hand-held digital camera is a process with an overall task of sensing radiance in a scene and generating an image. However, the camera is an aggregate of various subprocesses and subprocessing systems, each of which can be physical or non-physical, and can be sensing, acting, or computational. For example, a light detector outputs a measure of brightness, which serves as the input of a computational process which outputs a signal that provides input into an actuator that controls the opening or closing of the iris. The final iris size is sensed by another detector which inputs that value into a process that encodes that value into an EXIF format that accompanies the image, which is generated by a entirely different subsystem of the camera.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/physicalSystem/definition> |
| 1. A process shall be considered a “physical system” if it provides a processing function with well-defined inputs and outputs, if the device description is further divided into subprocess components, and if knowledge of its physical location is of importance. |

The model for *PhysicalSystem*, as shown in Fig. 7.18, is derived from *AbstractPhysicalProcess*, and adds the *components* and *connections* properties that have been described in the non-physical counterpart, *AggregateProcess* (Clause 7.4).

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/physicalSystem/dependency-core> |
| 1. An encoding or software passing the “Physical System” model conformance class shall first pass the “Abstract Physical Process” requirements test class in Clause 7.6. |




Figure 7.18 – Model for Physical Processing System

## Requirements Class: Physical Processes

|  |  |
| --- | --- |
| Requirements Class | |
| <http://www.opengis.net/spec/sensorML/2.0/req/model/physicalProcess> | |
| Target Type | Derived Models and Encodings |
| Dependency | [**http://www.opengis.net/spec/sensorML/2.0/req/model/SimpleProcess**](http://www.opengis.net/spec/sensorML/2.0/req/model/SimpleProcess) |
| Dependency | [**http://www.opengis.net/spec/sensorML/2.0/req/model/AggregateProcess**](http://www.opengis.net/spec/sensorML/2.0/req/model/AggregateProcess) |
| Dependency | [**http://www.opengis.net/spec/sensorML/2.0/req/model/PhysicalComponent**](http://www.opengis.net/spec/sensorML/2.0/req/model/PhysicalComponent) |
| Dependency | [**http://www.opengis.net/spec/sensorML/2.0/req/model/PhysicalSystem**](http://www.opengis.net/spec/sensorML/2.0/req/model/PhysicalSystem) |

A software or data base system that conforms to the Physical Process Requirements class will be able to define physical process components (e.g. detectors, actuators, physical filters and encoders) and non-physical process components (e.g. Digital Signal Processing filters), as well as be able to fully comprehend the interaction of these components within complex physical systems (e.g. sensors, platforms, robotic systems, etc) and workflows.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/physicalProcess/supports> |
| 1. A derived model or encoding supporting physical processes shall meet the requirements for non-physical processes (clause 7.9) as well as both the physical component process (clause 7.10) and physical system (clause 7.11). |

## Requirements Class: Configurable Processes

|  |  |
| --- | --- |
| Requirements Class | |
| <http://www.opengis.net/spec/sensorML/2.0/req/model/configurableProcess> | |
| Target Type | Derived Models and Encodings |

Many processes, both physical and non-physical, are configurable in that they provide one with the ability to set parameters values, enable options, or select modes before or during execution. Thus a general configurable process can be defined and published specifying allowed values for parameters, modes that can be selected, and options that can be enabled or disabled.

A specific process that inherits from this general process can then refine the process in several ways by: (1) specifying values for parameters, (2) further constraining the allowable values of parameters, (3) selecting an operational mode (which then sets a group of parameter values), or (4) enabling or disabling particular options such as particular inputs or outputs.

In this document, we will specify the more general process as the “configurable process”, and the more specific process that inherits from it, the “configured process”.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/configurableProcess/definitionOfConfigurable> |
| 1. A process shall be considered “configurable” if it provides options, variable parameters, or modes that can be selected or set before or during deployment or execution. |

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/configurableProcess/definitionOfConfigured> |
| 1. A process shall be considered “configured” if it sets options, parameter values, or modes that were defined within the configurable process. |

Example: A configurable process based on the linear equation (y=mx+b) defines two parameters for “slope” and “y-intercept” but does not provide values for these parameters. A configured process can inherit from this configurable process and set the values of those parameters (e.g. y=2x+4).

A process becomes “configurable” by one or more of the following characteristics:

* 1. it defines *parameters*, but not defining their values
  2. it defines *parameters* and providing a range or selection of values using the *swe:AllowedValues* property
  3. it defines *modes* which in turn set a collection of parameter values when enabled
  4. it allows *inputs*, *outputs*, or *parameters* to be enabled or disabled

A process becomes “configured” by having both of the following two characteristics:

1. it inherits from a configurable process using the *typeOf* property
2. it specifies one or more settings within the *configuration* property

### Modes

A process mode is a specific configuration in which the values for multiple parameters can be set and multiple options selected by enabling that mode. Often modes are established as a convenience so that a process can be configured during deployment or execution in order to best meet some specific operational need.

Example: A Doppler radar for monitoring storms may have several modes from which one can select depending on the prevailing conditions at the time. For instance, there can be “clear-sky”, “storm”, and “severe-storm” modes in which the scanning properties, radar intensity, and gain settings can all change by simply changing the mode setting.

A configurable process can but is not required to contain one or more *modes* properties. The *modes* property takes an *AbstractModes* as its value. As shown in Fig. 7.19, the concrete *ModeChoice* class defined in this conformance clause is derived from *AbstractModes* and serves as the concrete instantiation for defining modes in this specification.

*ModeChoice* shall include two or more *mode* properties that take *Mode* as their value. In addition to metadata provided by the base *DescribedObject* class, *Mode* includes a *configuration* property that allows one to define a collection of settings for that mode.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/configurableProcess/twoModesRequired> |
| 1. A *ModeChoice* instantiation must include two or more *mode* properties. |




Figure 7.19 – Model for Modes

The *configuration* property takes a *Settings* object, which will be described in more detail below.

### Settings

The *configuration* property and it *Settings* value can be utilized in two cases:

* 1. within the *Mode* definition of a configurable process for defining a collection of settings for that particular mode
  2. as a required property within a configured process for setting one or more configurable properties

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/configurableProcess/settingsProperty> |
| 1. A configured process must include a *configuration* property that takes a *Settings* class as its value. |

The *Settings* class is shown in Fig. 7.20 with its possible property values shown in Fig. 7.21. For all settings, the property in the configurable process is specified by the *DataComponentPath* reference.

Within the *Settings* class, one may (a) set particular values for parameters (and only parameters), (b) set an array of values for a parameter (and only a parameter that takes a DataArray as its value, (c) further constrain allowed values for parameters, (d) set the operational mode, and (e) enable or disable an input or output.




Figure 7.20 – Model for Configured Process Settings

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/configurableProcess/setValueRestriction> |
| 1. The *setValue* property shall only reference and set values for a *parameter* defined in a configurable process. |

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/configurableProcess/setArrayValueRestriction> |
| 1. The *setArrayValues* property shall only reference and set array values for a *parameter* defined in a configurable process. |

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/model/configurableProcess/setConstraintRestriction> |
| 1. The *setConstraint* property shall only reference and set constraints for a *parameter* defined in a configurable process. |




Figure 7.21 – Model for Settings Elements

# XML Schema Implementation (normative)

This standard defines a normative XML Schema grammar and a set of patterns that represent an XML implementation of the conceptual models presented in Section 7. The standardization target type for all requirements classes in this clause is an XML instance that seeks compliance with this XML encoding model.

XML schemas defined in this section are a direct implementation of the UML conceptual models described in Section 7. They have been automatically generated from these models by strictly following well-defined encoding rules described in Annex C. All attributes and composition/aggregation associations contained in the UML models are encoded either as XML elements or XML attributes but the names are fully consistent. One XML schema file is produced for each UML package.

Schematron patterns implement most additional requirements stated in Section 7. One Schematron file is produced for each XML package.

All example instances given in this section are informative and are used solely for illustrating features of the normative model. Many of these examples reference semantic information by using URLs that are resolvable to definitions maintained in one of several online ontologies:

* The OGC online registry at <http://www.opengis.net/def/>.
* The general sensor community ontologies at <http://www.sensors.ws>/.
* The SWEET ontology maintained by NASA JPL at <http://sweet.jpl.nasa.gov/2.0/>.
* The MMI ontology registry and repository at <http://mmisw.org/orr/>.

All XML examples are marked by a light gray background and formatted with a fixed- width font.

## Requirements Class: Core Abstract Process Schema

|  |  |
| --- | --- |
| Requirements Class | |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess> | |
| Target Type | XML Instance |
| **Dependency** | <http://www.opengis.net/spec/SensorML/2.0/req/model/coreProcess> |
| **Dependency** | <http://www.opengis.net/spec/SWE/2.0/req/xml-encoding-principles> |
| **Dependency** | http://www.opengis.net/spec/gml/3.2.1/gml |
| **Dependency** | \*\*\* iso 19139/gmd |

XML Schema elements and types defined in the “*core.xsd*” schema file implements all classes defined in the “Core Abstract Process” UML package.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/schema-valid> |
| 1. The XML instance shall be valid with respect to the XML grammar defined in the “core.xsd”, as well as satisfy all Schematron patterns defined in “core.sch”. |

### General XML Principles

This section lists common requirements associated to the XML encoding rules used in the context of this standard. As mentioned above, the normative XML schemas in this standard have been generated by strictly following UML to XML encoding rules, such that the schemas are the exact image of the UML models. The same encoding principles shall be used by all extensions of this standard.

#### XML Encoding Conventions

The rules used to encode the SensorML models into an XML Schema are similar to those used to derive GML application schemas and defined in ISO 19136. Most extensions to these rules were defined and implemented within the OGC SWE Common Data v2.0 standard and have been defined to allow:

* Use of “soft-typed” properties. These properties are encoded as XML elements with a generic element name but provide a “*name*” attribute for further disambiguation.
* Encoding of certain properties as XML attributes. This type of encoding adds to the “element-only” rules defined by ISO 19136. It is restricted to properties with a primitive type and indicated by a new tagged value in the UML model.
* Use of a new abstract base type. A custom base type called “*AbstractSWEType”* is used for all complex types.

Following ISO 19136 encoding rules, each UML class with a <<Type>> or <<DataType>> stereotype, or no stereotype at all, is implemented in the schema as a global XML complex type with a corresponding global XML element (called object element). Each of these elements has the same name as the UML class (i.e. always UpperCamelCase) and the name of the associated complex type is a concatenation of this name and the word “Type”.

Each UML class attribute is implemented either as a global complex type and a corresponding local element (called property element), or as an XML attribute. Each property complex type is given a name composed of the UML attribute name (always lowerCamelCase) and the words “PropertyType”. The element is defined locally within the complex type representing the class carrying the attribute and named exactly like the attribute in UML (i.e. no global elements are created for class attributes). Class associations are implemented similarly except they cannot be implemented as an XML attributes.

#### IDs and Linkable Properties

The schemas defined in this standard make extensive use of “*xlink*” features to support hypertext referencing in XML. This allows most property elements to reference content either internally or externally to the instance document, instead of including this content inline. This is supported by extensive use of the “*id*” attribute (of type xs:ID) on most object elements, and of the “*swe:AssociationAttributeGroup*” attribute group, on most property elements.

According to settings in the SensorML models, values for properties can be provided inline, by reference, or by either method.

In properties that support “*xlink*” attributes, one can usually choose to define that property value inline, as in:

<swe:field>

<swe:Quantity id="TEMP" … />

</swe:field>

One can then reference an object within the same document by its ID:

<swe:field xlink:href="#TEMP"/>

An object within an external document can also be referenced by including the full URI:

<swe:field xlink:href="http://www.my.com/fields.xml#TEMP"/>

Typically, “*xlink*” references will be specified as resolvable URLs. It is required that the property has either the “*xlink:href*” attribute set or contain an inline value, even though this cannot be enforced by XML schema.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/ref-or-inline-value-present> |
| 1. A property element supporting the “swe:AssociationAttributeGroup” shall either contain the value inline or populate the “xlink:href” attribute with a valid reference, but shall not be empty. |

As later specified, further requirements may be placed on the use of objects reference by xlink. This includes in some case, the use of both *xlink:href* to provide a resolvable link to the object’s description as well as the use of an *xlink:title* to provide the uniqueID of the object. Particular properties ay also require the application of *xlink:role* or *xlink:arcrole* to provide the absolute and relative role of the object, respectively.

#### Extensibility Points

The SensorML schemas define extensibility points that can be used to insert ad-hoc XML content that is not specified by this standard. This is done via optional “*extension*” element of type “*xs:anyType*” in the base abstract complex type “*AbstractSWEType*”. Since all object types defined in this standard derive from this base type, extensions can be added for many properties in a SensorML instance.

This mechanism allows for a “laxist” way of including extended content in XML instances as the extended content is by default ignored by the validator. However, it is also possible to formally validate extended content by writing an XML schema for the extension and feeding it to the validator via the “*xsi:schemaLocation*” attribute in all instances using the extension.

The recommended way of extending the XML schema of this standard is to define new properties on existing objects by inserting them in an “*extension*” slot. Additionally this should be done in a way that these new properties can be safely ignored by an implementation that is not compatible with a given extension. However, it should be recognized that defining new XML object elements (such as new data component objects) rather than new properties will greatly reduce forward compatibility of implementations compliant to this standard with XML instances containing extensions of this standard.

In any case, all extensions of the XML schema described in this standard shall be defined in a new namespace (other than the namespaces used by this standard and its dependencies) in order to allow easy detection of extensions by implementations.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/extension-namespace-unique> |
| 1. All extensions of the XML schemas described in this standard shall be defined in a new unique namespace (other than the namespaces used by this standard and its dependencies). |

Extensions are not allowed to change the meaning or behavior of elements and types defined by this standard in any way (in this case, new classes or properties shall me defined). This guarantees that implementations that have no knowledge of an extension can still properly use XML instances containing these extensions.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/extension-coherent-with-core> |
| 1. Extensions of this standard shall not redefine or change the meaning or behavior of XML elements and types defined in this standard. |

The execution of the process should not depend on information contained within an extension. Data values required for process execution must be provided within the input, output, and parameter properties, and within the SensorML and SWE Common Data namespace elements (i.e. sml and swe, respectively), and cannot exclusively be contained in the extension classes.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/extension-process-execution> |
| 1. Extensions of this standard shall not exclusively contain information required for the successful execution of the process. |

Note that extension points are also supported by the SWE Common Data specification such that community-specific XML elements can be added to any property value that uses a SWE Common data type element as its value. Common anticipated applications of property-specific extension points include security tagging of individual properties and community-specific quality control characterization of property values.

### General XSD Dependencies and XML Heading

The header for all specified schema provides namespaces and dependencies. The header for core processes below specifices the namespaces and dependent schema for “sml”, “swe”, “gml”, “gco”, and “gmd”.

<schema xmlns="http://www.w3.org/2001/XMLSchema" xmlns:gco="http://www.isotc211.org/2005/gco"

xmlns:gmd="http://www.isotc211.org/2005/gmd" xmlns:sml="http://www.opengis.net/sensorML/2.0"

xmlns:gml="http://www.opengis.net/gml/3.2" xmlns:swe="http://www.opengis.net/swe/2.0"

targetNamespace="http://www.opengis.net/sensorML/2.0" elementFormDefault="qualified"

attributeFormDefault="unqualified">

<annotation>

<documentation>

The core elements of an abstract process from which all major elements of SensorML are derived.

</documentation>

</annotation>

<import namespace="http://www.isotc211.org/2005/gmd"

schemaLocation="http://schemas.opengis.net/iso/19139/20070417/gmd/gmd.xsd"/>

<import namespace="http://www.isotc211.org/2005/gco"

schemaLocation="http://schemas.opengis.net/iso/19139/20070417/gco/gco.xsd"/>

<import namespace="http://www.opengis.net/gml/3.2"

schemaLocation="http://schemas.opengis.net/gml/3.2.1/gml.xsd"/>

<import namespace=”http://www.opengis.net/swe/2.0”

schemaLocation="http://schemas.opengis.net/sweCommon/2.0/swe.xsd"/>

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/gml-dependency> |
| 1. This standard shall utilize and depend upon the OGC GML 3.2 standard schema within the http://www.opengis.net/gml/3.2 namespace and defined in http://schemas.opengis.net/gml/3.2.1/ |

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/swe-common-dependency> |
| 1. This standard shall utilize and depend upon the OGC SWE Common Data 2.0 standard within the <http://www.opengis.net/swe/2.0> namespace and defined in [http://schemas.opengis.net/sweCommon/2.0/*swe.xsd*](http://schemas.opengis.net/sweCommon/2.0/swe.xsd) *and any corregendum (i.e. any versions 2.0.\*).* |

Several base abstract types are defined in the SWE Common Data standard are used for derivation of elements within this SensorML specification. These are defined in the “swe” namespace and defined in:

[http://schemas.opengis.net/sweCommon/2.0/*basic\_types.xsd*](http://schemas.opengis.net/sweCommon/2.0/basic_types.xsd)

These basic types are used as base substitution groups for all global XML elements defined in this standard. Below are XML schema snippets for the “*AbstractSWE*”, “*AbstractSWEIdentifiable*” and “*AbstractSWEValue*” elements and corresponding complex types:

<element name="AbstractSWE" abstract="true" type="swe:AbstractSWEType"/>

<complexType name="AbstractSWEType">

<sequence>

<element name="extension" type="anyType" minOccurs="0" maxOccurs="unbounded"/>

</sequence>

<attribute name="id" use="optional"/>

</complexType>

The “*AbstractSWE*” complex type is the base for all derived complex types defined in this standard. It defines a first extension mechanism as an optional “*extension*” element that allows for any extended element content (in a namespace other than the SWE Common Data Model namespace). It also has an optional “*id*” attribute allowing referencing the object that derives from it.

<element name="AbstractSWEIdentifiable" abstract="true" substitutionGroup="swe:AbstractSWE"  
 type="swe:AbstractSWEIdentifiableType"/>

<complexType name="AbstractSWEIdentifiableType">

<complexContent>

<extension base="swe:AbstractSWEType">

<sequence>

<element name="identifier" type="anyURI" minOccurs="0"/>

<element name="label" type="string" minOccurs="0"/>

<element name="description" type="string" minOccurs="0"/>

</sequence>

</extension>

</complexContent>

</complexType>

The “*AbstractSWEIdentifiable*” complex type derives from “*AbstractSWE*” and adds three identification elements. These elements are to be used as described in the UML section of this standard.

### DescribedObject Properties

The *DescribedObject* element is an XML Schema implementation of the UML classes defined in clause 7.2.2. *DescribedObject* is the base class for all process objects defined in this standard. *DescribedObject* is derived from *gml:AbstractFeature*. In essence it provides a common set of metadata for a general feature. It is particularly suited for processes and functional devices, as later described in this specification.

The XML snippet for the *DescribedObject* element and its corresponding complex types is shown below:

<element name="DescribedObject" type="sml:DescribedObjectType" abstract="true"

substitutionGroup="gml:AbstractFeature">

<annotation>

<documentation>

A feature with generic metadata which further clarifies the object and supports object discovery.

</documentation>

</annotation>

</element>

<complexType name="DescribedObjectType" abstract="true">

<complexContent>

<extension base="gml:AbstractFeatureType">

<sequence>

<element name="extension" type="anyType" minOccurs="0" maxOccurs="unbounded"/>

<element name="keywords" type="sml:KeywordListPropertyType" minOccurs="0"

maxOccurs="unbounded"/>

<element name="identification" type="sml:IdentifierListPropertyType" minOccurs="0"

maxOccurs="unbounded">

<annotation>

<documentation>

Identifiers useful for discovery of the feature (e.g. short name, mission id, wing id, serial number, etc.)

</documentation>

</annotation>

</element>

<element name="classification" type="sml:ClassifierListPropertyType" minOccurs="0"

maxOccurs="unbounded">

<annotation>

<documentation>

Classifiers useful for discovery of the feature (e.g. process type, sensor type, intended

application, etc.)

</documentation>

</annotation>

</element>

<element name="validTime" minOccurs="0" maxOccurs="unbounded">

<annotation>

<documentation>

The time instance or time range during which this instance description is valid.

</documentation>

</annotation>

<complexType>

<sequence>

<group ref="sml:TimeInstantOrPeriod"/>

</sequence>

</complexType>

</element>

<element name="securityConstraints" type="anyType" minOccurs="0" maxOccurs="unbounded">

<annotation>

<documentation>

Overall security tagging of process description; individual tagging of properties can be

done using extension element.

</documentation>

</annotation>

</element>

<element name="legalConstraints" type="gmd:MD\_LegalConstraints\_PropertyType" minOccurs="0"

maxOccurs="unbounded">

<annotation>

<documentation>

Legal constraints applied to this description (e.g. copyrights, legal use, etc.)

</documentation>

</annotation>

</element>

<element name="characteristics" type="sml:CharacteristicListPropertyType" minOccurs="0"

maxOccurs="unbounded">

<annotation>

<documentation>

Useful properties of this process that do not further qualify the output values (e.g.

component dimensions, battery life, operational limits, etc).

</documentation>

</annotation>

</element>

<element name="capabilities" type="sml:CapabilityListPropertyType" minOccurs="0"

maxOccurs="unbounded">

<annotation>

<documentation>

Properties that further clarify or quantify the output of the process (e.g. dynamic range,

sensitivity, threshold, etc.). These can assist in the discovery of processes that meet

particular requirements.

</documentation>

</annotation>

</element>

<element name="contacts" type="sml:ContactListPropertyType" minOccurs="0"

maxOccurs="unbounded">

<annotation>

<documentation>

Persons or responsible parties that are relevant to this process (e.g. designer,

manufacturer, expert, etc.)

</documentation>

</annotation>

</element>

<element name="documentation" type="sml:DocumentListPropertyType" minOccurs="0"

maxOccurs="unbounded">

<annotation>

<documentation>

Additional external online documentation of relevance to this process (e.g. user's guides,

product manuals, specification sheets, images, technical papers, etc.)

</documentation>

</annotation>

</element>

<element name="history" type="sml:EventListPropertyType" minOccurs="0"

maxOccurs="unbounded">

<annotation>

<documentation>

A collection of time-tagged events relevant to this process.

</documentation>

</annotation>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

Most properties in DescribedObject are optional, thereby allowing the description to be as small or as robust as one desires.

All property elements in *DescribedObject* are of type *DescribedObjectPropertyType* which supports the ability to reference the value of the property externally through *xlink:href* or provide the value inline.

<complexType name="DescribedObjectPropertyType">

<sequence minOccurs="0">

<element ref="sml:DescribedObject"/>

</sequence>

<attributeGroup ref="gml:AssociationAttributeGroup"/>

<attributeGroup ref="gml:OwnershipAttributeGroup"/>

</complexType>

Additionally, most property values in *DescribedObject* are of type *AbstractMetadataListType,* which supports a list structure along with identification and definition properties.

<element name="AbstractMetadataList" type="sml:AbstractMetadataListType"

substitutionGroup="swe:AbstractSWEIdentifiable"/>

<complexType name="AbstractMetadataListType">

<complexContent>

<extension base="swe:AbstractSWEIdentifiableType">

<attribute name="definition" type="anyURI" use="optional"/>

</extension>

</complexContent>

</complexType>

<complexType name="AbstractMetadataListPropertyType">

<sequence minOccurs="0">

<element ref="sml:AbstractMetadataList"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

#### Description Property

The *description* property is inherited from *gml:AbstractFeature* and provides a textual description for the feature.

An example of a description is given below:

<gml:description>Thermometer on the window of the Cass Building, Room 315</gml:description>

#### Name Property

The name property is inherited from *gml:AbstractFeature* and provides a common name for the feature.

An example of the name property is given below:

<gml:name>Health Physics Instruments 2070 Gamma Detector</gml:name>

#### Unique Identifier

This specification reserves the *gml:identifier*, inherited from *gml:AbstractFeature*, as a means of providing a unique identifier for the *DescribedObject*. This unique identifier should be referenced in any other specification that involves this object, thereby providing a means of searching for all references to this object.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/globallyUniqueID> |
| 1. An instance supporting *DescribedObject* shall have one and only one *gml:identifier* and this element shall have a *codespace* attribute with a value set to “uniqueID”. The value of the *gml:identifier* shall be a globally unique identifier for the *DescribedObject*. |

The value of the gml:identifier can be a URI (e.g. URL or URN) or a series of string characters that uniquely identify the object. An example of a globally unique identifier for a weather station is given below:

<gml:identifier codeSpace="uid">urn:icd:stations:FR8766</gml:identifier>

<gml:identifier codeSpace="uid">38a7s8f9d55</gml:identifier>

#### Keywords

The *keyword* property and the *KeywordList* element are XML Schema implementations of the UML classes defined in clause 7.2.2.2.

The XML snippet for the *KeywordList* element and its corresponding complex types is shown below:

<element name="KeywordList" type="sml:KeywordListType" substitutionGroup="sml:AbstractMetadataList"/>

<complexType name="KeywordListType">

<complexContent>

<extension base="sml:AbstractMetadataListType">

<sequence>

<element name="codeSpace" type="swe:Reference" minOccurs="0" maxOccurs="1"/>

<element name="keyword" type="string" minOccurs="1" maxOccurs="unbounded"/>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="KeywordListPropertyType">

<sequence minOccurs="0">

<element ref="sml:KeywordList"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

The *KeywordList* element includes an optional *codespace* attribute that shall reference an external dictionary or keyword list that includes all possible keyword entries. An example of a keyword list without a codespace defined is shown below:

<keywords>

<KeywordList>

<keyword>weather station</keyword>

<keyword>precipitation</keyword>

<keyword>wind speed</keyword>

<keyword>temperature</keyword>

</KeywordList>

</keywords>

An example of a keyword list with codespace is shown below:

<keywords>

<KeywordList codespace="http://myAuthoritativeDomain.org/def/myKeywordList">

<keyword>weather station</keyword>

<keyword>precipitation</keyword>

<keyword>wind speed</keyword>

<keyword>temperature</keyword>

</KeywordList>

</keywords>

#### Identifiers

The *IdentifierList* and the *Term* elements are XML Schema implementations of the UML classes defined in clause 7.2.2.3. The *identifier* property of the *IdentifierList* takes a *Term* as its value. The *Term* element has an optional *definition* attribute that shall reference a resolvable definition of the term within an online dictionary or ontology.

The XML snippets for the *IdentifierList* and *Term* elements and their corresponding complex types are shown below:

*Term:*

<element name="Term" type="sml:TermType" substitutionGroup="swe:AbstractSWE"/>

<complexType name="TermType">

<complexContent>

<extension base="swe:AbstractSWEType">

<sequence>

<element name="label" type="string"/>

<element name="codeSpace" type="swe:Reference" minOccurs="0" maxOccurs="1"/>

<element name="value" type="string"/>

</sequence>

<attribute name="definition" type="anyURI" use="optional"/>

</extension>

</complexContent>

</complexType>

<complexType name="TermPropertyType">

<sequence minOccurs="0">

<element ref="sml:Term"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

*IdentifierList:*

<element name="IdentifierList" type="sml:IdentifierListType" substitutionGroup="sml:AbstractMetadataList"/>

<complexType name="IdentifierListType">

<complexContent>

<extension base="sml:AbstractMetadataListType">

<sequence>

<element name="identifier" minOccurs="1" maxOccurs="unbounded">

<complexType>

<sequence>

<element ref="sml:Term"/>

</sequence>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="IdentifierListPropertyType">

<sequence minOccurs="0">

<element ref="sml:IdentifierList"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

An example of an identifier list is shown below:

<sml:identification>

<sml:IdentifierList>

<sml:identifier>

<sml:Term definition="http://www.opengis.net/def/property/OGC/0/ShortName">

<sml:label>Short Name</sml:label>

<sml:value>Thermometer FR8766</sml:value>

</sml:Term>

</sml:identifier>

<sml:identifier>

<sml:Term definition="http://www.opengis.net/def/property/OGC/0/Manufacturer">

<sml:label>Manufacturer Name</sml:label>

<sml:value>ACME Inc</sml:value>

</sml:Term>

</sml:identifier>

<sml:identifier>

<sml:Term definition="http://www.opengis.net/def/property/OGC/0/ModelNumber">

<sml:label>Manufacturer Model</sml:label>

<sml:value>T911</sml:value>

</sml:Term>

</sml:identifier>

<sml:identifier>

<sml:Term definition="http://www.opengis.net/def/property/OGC/0/SerialNumber">

<sml:label>Serial Number</sml:label>

<sml:value>FT5743456566-997</sml:value>

</sml:Term>

</sml:identifier>

</sml:IdentifierList>

</sml:identification>

#### Classifiers

The *ClassifierList* is an XML Schema implementations of the UML classes defined in clause 7.2.2.4. The *classifier* property of the *ClassifierList* takes a *Term* as its value.

The XML snippet for the *ClassifierList* element and its corresponding complex types is shown below:

<element name="ClassifierList" type="sml:ClassifierListType" substitutionGroup="sml:AbstractMetadataList"/>

<complexType name="ClassifierListType">

<complexContent>

<extension base="sml:AbstractMetadataListType">

<sequence>

<element name="classifier" minOccurs="1" maxOccurs="unbounded">

<complexType>

<sequence>

<element ref="sml:Term"/>

</sequence>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="ClassifierListPropertyType">

<sequence minOccurs="0">

<element ref="sml:ClassifierList"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

An example of a classifier list is shown below:

<sml:classification>

<sml:ClassifierList>

<sml:classifier>

<sml:Term definition="http://www.opengis.net/def/property/OGC/0/SensorType">

<sml:label>Sensor Type</sml:label>

<sml:value>Weather Station</sml:value>

</sml:Term>

</sml:classifier>

<sml:classifier>

<sml:Term definition="http://www.opengis.net/def/property/OGC/0/IntendedApplication">

<sml:label>Intended Application</sml:label>

<sml:value>Weather</sml:value>

</sml:Term>

</sml:classifier>

</sml:ClassifierList>

</sml:classification>

#### Security Constraints

The *securityConstraints* property provides an overall security tagging for the overall document. Typically if any part of a document is classified as Secret, for instance, then the entire document is tagged as Secret.

Because various nations and other entities may have developed their own XML schema for supporting security tagging, the value of the *securityConstraints* property is provide as *xs:any*. Thus, like the *extension* property, the value of the *securityConstraint* property can be any XML, but this XML must be defined in a namespace other than those used in this standard.

|  |
| --- |
| Requirement |
| [http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/documentSecurityTags](http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/extension-namespace-unique) |
| 1. All values for the *securityConstraints* property shall be defined in a new unique namespace (other than the namespaces used by this standard and its dependencies). |

#### Note on Security Tagging Individual Properties

It is often required or desireable that security tagging exists not only for the entire document but for individual property values as well. SensorML supports tagging of individual property values and lists through the *extension* property that is inherited by all elements derived from *AbstractSWEType* and *AbstractSWEIdentifiableType*.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/individualSecurityTags> |
| 1. Security tagging of individual property values shall utilize the *extension* element within the appropriate SensorML or SWE Common data elements. |

#### Valid Time Constraints

The *validTime* element is an XML Schema implementation of the UML class defined in clause 7.2.2.6.

The XML Schema snippet from *DescribedObject* that pertains to the *validTime* property is given below. The *validTime* property takes either a GML *TimePeriod* or *TimeInstant* as its value.

<element name="validTime" minOccurs="0" maxOccurs="unbounded">

<annotation>

<documentation>

The time instance or time range during which this instance description is valid.

</documentation>

</annotation>

<complexType>

<sequence>

<group ref="sml:TimeInstantOrPeriod"/>

</sequence>

</complexType>

</element>

<group name="TimeInstantOrPeriod">

<annotation>

<documentation>Either a Time Instant or Time Period</documentation>

</annotation>

<choice>

<element ref="gml:TimePeriod"/>

<element ref="gml:TimeInstant"/>

</choice>

</group>

<complexType name="TimeInstantOrPeriodPropertyType">

<sequence minOccurs="0">

<group ref="sml:TimeInstantOrPeriod"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

An example of the valid time being given by a TimePeriod is shown below:

<validTime>

<gml:TimePeriod gml:id="deploymentDates">

<gml:beginPosition>2009-01-01T14:00:00Z</gml:beginPosition>

<gml:endPosition>2013-12-31T08:20:00Z</gml:endPosition>

</gml:TimePeriod>

</validTime>

#### Legal Constraints

The *legalConstraints* element is an XML Schema implementation of the UML class defined in clause 7.2.2.7.

The XML Schema snippet from *DescribedObject* that pertains to the *legalConstraints* property is given below. The *legalConstraints* property takes an ISO 19115 *MD\_LegalConstraints* element as its value, which is encoded according to ISO19139 schema.

<element name="legalConstraints" type="gmd:MD\_LegalConstraints\_PropertyType" minOccurs="0"

maxOccurs="unbounded">

<annotation>

<documentation>

Legal constraints applied to this description (e.g. copyrights, legal use, etc.)

</documentation>

</annotation>

</element>

An example of legalConstraints is provided below:

<legalConstraints>

<gmd:MD\_LegalConstraints>

<gmd:useLimitation>

<gco:CharacterString>

This document and the device that it describes should only be used for the purpose

as intended and defined in http://myCompany.com/legalBS.html

</gco:CharacterString>

</gmd:useLimitation>

<gmd:otherConstraints>

<gco:CharacterString>

LiabilityLimitations: MyCompany shall not be held responsible for any harm caused by

incorrect information provided in this document or for any failure of this device.

</gco:CharacterString>

</gmd:otherConstraints>

</gmd:MD\_LegalConstraints>

</legalConstraints>

#### Capabilities

The *capabilities* property and the *CapabilitiesList* element are XML Schema implementations of the UML classes defined in clause 7.2.2.9. The *capabilities* property takes a *CapabilitiesList* as its value. The *CapabilitiesList* *member* property accepts any SWE Common data component as its value.

The XML snippet for the *CapabilitiesList* element and its corresponding complex types is shown below:

<element name="CapabilityList" type="sml:CapabilityListType" substitutionGroup="sml:AbstractMetadataList"/>

<complexType name="CapabilityListType">

<complexContent>

<extension base="sml:AbstractMetadataListType">

<sequence>

<element name="member" minOccurs="1" maxOccurs="unbounded">

<complexType>

<complexContent>

<extension base="swe:AbstractDataComponentPropertyType">

<attribute name="name" type="NCName" use="required"/>

</extension>

</complexContent>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="CapabilityListPropertyType">

<sequence minOccurs="0">

<element ref="sml:CapabilityList"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

Thus capabilities can be described using SWE Common simple types, such as *Quantity*, *Count*, *Boolean*, *Category*, *Text*, and *Time* as well as be aggregate types such as *DataRecord*, *DataArray*, *Vector*, or *Matrix*.

An example of *capabilities* is given below:

<sml:capabilities>

<sml:CapabilityList>

<sml:member name="measurementProperties">

<swe:DataRecord definition="http://www.opengis.net/def/property/OGC/0/measurementProperties">

<swe:label>Measurement Properties</swe:label>

<swe:field name="RadiationRange">

<swe:QuantityRange definition="http://www.opengis.net/def/property/OGC/0/radiationLevel">

<swe:uom code="R/h"/>

<swe:value>0 30</swe:value>

</swe:QuantityRange>

</swe:field>

<swe:field name="Sensitivitity">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/radiationSensitivity">

<swe:uom code="{tot}/uR"/>

<swe:value>1</swe:value>

</swe:Quantity>

</swe:field>

<swe:field name="SamplePeriod">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/samplePeriod">

<swe:uom code="s"/>

<swe:value>1</swe:value>

</swe:Quantity>

</swe:field>

<swe:field name="MeasurementOutputTime">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/outputPeriod">

<swe:uom code="s"/>

<swe:value>450</swe:value>

</swe:Quantity>

</swe:field>

</swe:DataRecord>

</sml:member>

</sml:CapabilityList>

</sml:capabilities>

#### Characteristics

The *characteristics* property and the *CharacteristicsList* element are XML Schema implementations of the UML classes defined in clause 7.2.2.9. The *characteristics* property takes a *CharacteristicsList* as its value. The *CharacteristicsList* *member* property accepts any SWE Common data component as its value.

The XML snippet for the *CharacteristicsList* element and its corresponding complex types is shown below:

<element name="CharacteristicList" type="sml:CharacteristicListType"

substitutionGroup="sml:AbstractMetadataList"/>

<complexType name="CharacteristicListType">

<complexContent>

<extension base="sml:AbstractMetadataListType">

<sequence>

<element name="member" minOccurs="1" maxOccurs="unbounded">

<complexType>

<complexContent>

<extension base="swe:AbstractDataComponentPropertyType">

<attribute name="name" type="NCName" use="required"/>

</extension>

</complexContent>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="CharacteristicListPropertyType">

<sequence minOccurs="0">

<element ref="sml:CharacteristicList"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

Thus characteristics can be described using SWE Common simple types, such as *Quantity*, *Count*, *Boolean*, *Category*, *Text*, and *Time* as well as be aggregate types such as *DataRecord*, *DataArray*, *Vector*, or *Matrix*.

An example of *characteristics* that groups like properties in data records is given bleow:

<sml:characteristics>

<sml:CharacteristicList>

<sml:member name="physicalProperties">

<swe:DataRecord definition="http://www.opengis.net/def/property/OGC/0/physicalProperties">

<swe:label>Physical Properties</swe:label>

<swe:field name="PhysicalProperties">

<swe:DataRecord>

<swe:field name="Weight">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/weight">

<swe:uom code="oz"/>

<swe:value>10</swe:value>

</swe:Quantity>

</swe:field>

<swe:field name="Length">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/length">

<swe:uom code="in"/>

<swe:value>4.5</swe:value>

</swe:Quantity>

</swe:field>

<swe:field name="Width">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/width">

<swe:uom code="in"/>

<swe:value>2.5</swe:value>

</swe:Quantity>

</swe:field>

<swe:field name="Height">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/height">

<swe:uom code="in"/>

<swe:value>1.4</swe:value>

</swe:Quantity>

</swe:field>

<swe:field name="CasingMaterial">

<swe:Category definition="http://www.opengis.net/def/property/OGC/0/material">

<swe:value>Aluminum</swe:value>

</swe:Category>

</swe:field>

</swe:DataRecord>

</swe:field>

</swe:DataRecord>

</sml:member>

<sml:member name="electricalRequirements">

<swe:DataRecord definition="http://www.opengis.net/def/property/OGC/0/powerRequirement">

<swe:label>Electrical Requirements</swe:label>

<swe:field name="voltage">

<swe:QuantityRange definition="http://www.opengis.net/def/property/OGC/0/voltage">

<swe:uom code="V"/>

<swe:value>8 12</swe:value>

</swe:QuantityRange>

</swe:field>

<swe:field name="CurrentType">

<swe:Category definition="http://www.opengis.net/def/property/OGC/0/electricalCurrentType">

<swe:value>DC</swe:value>

</swe:Category>

</swe:field>

<swe:field name="AmpRange">

<swe:QuantityRange definition="http://www.opengis.net/def/property/OGC/0/electricalCurrent">

<swe:uom code="mA"/>

<swe:value>20 40</swe:value>

</swe:QuantityRange>

</swe:field>

</swe:DataRecord>

</sml:member>

</sml:CharacteristicList>

</sml:characteristics>

#### Contacts

The *contacts* property and the *ContactList* element are XML Schema implementations of the UML classes defined in clause 7.2.2.11. The *contacts* property takes a *ContactList* as its value. The *ContactList* *member* property supports an ISO 19115 *CI\_ResponsibleParty* as its value, which is encoded according to ISO19139 schema.

The XML snippet for the *ContactList* element and its corresponding complex types is shown below:

<element name="ContactList" type="sml:ContactListType" substitutionGroup="sml:AbstractMetadataList"/>

<complexType name="ContactListType">

<complexContent>

<extension base="sml:AbstractMetadataListType">

<sequence>

<element name="member" type="gmd:CI\_ResponsibleParty\_PropertyType" minOccurs="1"

maxOccurs="unbounded"/>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="ContactListPropertyType">

<sequence minOccurs="0">

<element ref="sml:ContactList"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

A contact can have multiple roles for which it is responsible. What is of most interest in this standard is the role the responsible party plays relative to the object being described. Therefore, the role of the responsible party (e.g. manufacturer, expert, owner, etc.) shall be given by the *xlink:arcrole* attribute in the *member* property of the *ContactList*.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/contactRole> |
| 1. The role of the responsible party relative to the described object shall be provided using the *xlink:arcrole* attribute of the relevant *member* property of the *ContactList*. |

An example of a *ContactList* is shown below.

<sml:contacts>

<sml:ContactList>

<sml:member xlink:arcrole="http://www.opengis.net/def/role/OGC/0/Operator">

<gmd:CI\_ResponsibleParty>

<gmd:organisationName>

<gco:CharacterString>METEO France</gco:CharacterString>

</gmd:organisationName>

<gmd:contactInfo>

<gmd:CI\_Contact>

<gmd:phone>

<gmd:CI\_Telephone>

<gmd:voice>

<gco:CharacterString>+33 5 99 11 22 33 44</gco:CharacterString>

</gmd:voice>

</gmd:CI\_Telephone>

</gmd:phone>

<gmd:address>

<gmd:CI\_Address>

<gmd:deliveryPoint>

<gco:CharacterString>42 Avenue Gaspard Coriolis</gco:CharacterString>

</gmd:deliveryPoint>

<gmd:city>

<gco:CharacterString>TOULOUSE</gco:CharacterString>

</gmd:city>

<gmd:postalCode>

<gco:CharacterString>31100</gco:CharacterString>

</gmd:postalCode>

<gmd:country>

<gco:CharacterString>FRANCE</gco:CharacterString>

</gmd:country>

</gmd:CI\_Address>

</gmd:address>

</gmd:CI\_Contact>

</gmd:contactInfo>

<gmd:role gco:nilReason="inapplicable"/>

</gmd:CI\_ResponsibleParty>

</sml:member>

</sml:ContactList>

</sml:contacts>

#### Documentation

The *documentation* property and the *DocumentList* element are XML Schema implementations of the UML classes defined in clause 7.2.2.11. The *documentation* property takes a *DocumentList* as its value. The *DocumentList* *member* property supports an ISO 19115 *CI\_OnlineResource* as its value, which is encoded according to ISO19139 schema.

The XML snippet for the *DocumentList* element and its corresponding complex types is shown below:

<element name="DocumentList" type="sml:DocumentListType" substitutionGroup="sml:AbstractMetadataList"/>

<complexType name="DocumentListType">

<complexContent>

<extension base="sml:AbstractMetadataListType">

<sequence>

<element name="member" type="gmd:CI\_OnlineResource\_PropertyType" minOccurs="1"

maxOccurs="unbounded"/>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="DocumentListPropertyType">

<sequence minOccurs="0">

<element ref="sml:DocumentList"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

An example of *documentation* is given below:

<documentation>

<DocumentList>

<member xlink:arcrole="userManual">

<gmd:CI\_OnlineResource>

<gmd:linkage>

<gmd:URL>http://myCompany.com/ref/2031manual.pdf</gmd:URL>

</gmd:linkage>

<gmd:name>

<gco:CharacterString>

User Manual for Model 2031

</gco:CharacterString>

</gmd:name>

<gmd:description>

<gco:CharacterString>

This document provides the complete Users Manual for the myCompany sensor model 2031.

</gco:CharacterString>

</gmd:description>

</gmd:CI\_OnlineResource>

</member>

<member xlink:arcrole="productImage">

<gmd:CI\_OnlineResource>

<gmd:linkage>

<gmd:URL>http://myCompany.com/ref/2031image.jpg</gmd:URL>

</gmd:linkage>

<gmd:name>

<gco:CharacterString>

Sensor Model 2031

</gco:CharacterString>

</gmd:name>

<gmd:description>

<gco:CharacterString>

This is an image of sensor model 2031.

</gco:CharacterString>

</gmd:description>

</gmd:CI\_OnlineResource>

</member>

</DocumentList>

</documentation>

#### History

The *history* property and the *EventList* and *Event* elements are XML Schema implementations of the UML classes defined in clause 7.2.2.12. The *history* property takes an *EventList* as its value. The *EventList* *member* property takes an *Event* as its value. The XML snippets for the *EventList* and *Event* elements and their corresponding complex types are shown below:

*EventList*:

<element name="EventList" type="sml:EventListType" substitutionGroup="sml:AbstractMetadataList"/>

<complexType name="EventListType">

<complexContent>

<extension base="sml:AbstractMetadataListType">

<sequence>

<element name="member" type="sml:EventPropertyType" minOccurs="1"

maxOccurs="unbounded"/>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="EventListPropertyType">

<sequence minOccurs="0">

<element ref="sml:EventList"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

*Event*:

<element name="Event" type="sml:EventType" substitutionGroup="swe:AbstractSWEIdentifiable">

<annotation>

<documentation>

A time tagged Event with description and relevant property values.

</documentation>

</annotation>

</element>

<complexType name="EventType">

<complexContent>

<extension base="swe:AbstractSWEIdentifiableType">

<sequence>

<element name="keywords" type="sml:KeywordListPropertyType" minOccurs="0" maxOccurs="1">

<annotation>

<documentation>

keywords useful for discovery of the event

</documentation>

</annotation>

</element>

<element name="identification" type="sml:IdentifierListPropertyType" minOccurs="0"

maxOccurs="1">

<annotation>

<documentation>

Identifiers relevant to the event

</documentation>

</annotation>

</element>

<element name="classification" type="sml:ClassifierListPropertyType" minOccurs="0"

maxOccurs="1">

<annotation>

<documentation>

Type of event (useful for discovery)

</documentation>

</annotation>

</element>

<element name="contacts" type="sml:ContactListPropertyType" minOccurs="0" maxOccurs="1">

<annotation>

<documentation>

Persons or parties relevant to this event

</documentation>

</annotation>

</element>

<element name="documentation" type="sml:DocumentListPropertyType" minOccurs="0"

maxOccurs="1">

<annotation>

<documentation>

Additional documentation relevant to this event

</documentation>

</annotation>

</element>

<element name="time">

<annotation>

<documentation>DateTime of the event</documentation>

</annotation>

<complexType>

<sequence>

<group ref="sml:TimeInstantOrPeriod"/>

</sequence>

</complexType>

</element>

<element name="property" type="swe:AbstractDataComponentPropertyType" minOccurs="0"

maxOccurs="1">

<annotation>

<documentation>

Properties of interest to the event (e.g. calibration values, condition category, error codes,

etc)

</documentation>

</annotation>

</element>

<element name="configuration" minOccurs="0" maxOccurs="1">

<annotation>

<documentation>

Configuration settings adjusted during event

</documentation>

</annotation>

<complexType>

<sequence>

<element ref="sml:AbstractSettings"/>

</sequence>

</complexType>

</element>

</sequence>

<attribute name="definition" type="anyURI" use="optional"/>

</extension>

</complexContent>

</complexType>

<complexType name="EventPropertyType">

<sequence minOccurs="0">

<element ref="sml:Event"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

An example of an *EventList* is shown below. *EventList* could of course be presented inline as a value of the *history* property, or could be maintained externally and referenced by the *xlink:href* attribute of the *history* property.

<sml:EventList>

<sml:member>

<sml:Event>

<swe:label>Scheduled Maintenance</swe:label>

<swe:description>

Monthly maintenance of station exterior.&#13;-Checked electronics&#13;-Checked casing&#13;Checked power

supply.&#13;Everything OK.

</swe:description>

<sml:time>

<gml:TimePeriod gml:id="MP1">

<gml:beginPosition>2002-03-01T10:00:00Z</gml:beginPosition>

<gml:endPosition>2002-03-01T11:00:00Z</gml:endPosition>

</gml:TimePeriod>

</sml:time>

</sml:Event>

</sml:member>

<sml:member>

<sml:Event>

<swe:label>Calibration</swe:label>

<swe:description>Recalibration of acquisition electronics using temperature reference</swe:description>

<sml:time>

<gml:TimeInstant gml:id="MP2">

<gml:timePosition>2002-03-01T18:00:00Z</gml:timePosition>

</gml:TimeInstant>

</sml:time>

<sml:configuration>

<sml:Settings>

<sml:setArrayValues sml:ref="base/components/raingauge/parameters/steady-state-response">

<sml:ArrayValues>

<sml:encoding>

<swe:TextEncoding tokenSeparator="," blockSeparator=" "/>

</sml:encoding>

<sml:value>1,2,3,4,5 2,4,6,8,10</sml:value>

</sml:ArrayValues>

</sml:setArrayValues>

</sml:Settings>

</sml:configuration>

<sml:previousDescription xlink:href="http://myDomain.com/Sensor\_2002-01-15.xml"/>

</sml:Event>

</sml:member>

</sml:EventList>

### Abstract Process

*AbstractProcessType* is derived from *DescribedObject* and serves as the base class for all processes modelled and encoded in this specification. Thus, all processes include the metadata described above plus the elements defined in this section and its subsections.

The *AbstractProcess* element is an XML Schema implementation of the UML class defined in clause 7.2.3.

The XML snippet for the *AbstractProcess* element and its corresponding complex types is shown below. The various properties of *AbstractProcess* will be discussed in more detail in the following subsections.

<element name="AbstractProcess" type="sml:AbstractProcessType" abstract="true"

substitutionGroup="sml:DescribedObject">

<annotation>

<documentation>

The general base model for any process.

</documentation>

</annotation>

</element>

<complexType name="AbstractProcessType" abstract="true">

<complexContent>

<extension base="sml:DescribedObjectType">

<sequence>

<element name="typeOf" type="gml:ReferenceType" minOccurs="0" maxOccurs="1">

<annotation>

<appinfo>

<gml:targetElement>sml:AbstractProcess</gml:targetElement>

</appinfo>

<documentation>

A reference to a base process from which this process inherits properties and constraints

(e.g. original equipment manufacturer's model description, generic equation, etc.). The

uniqueID of the referenced process must be provided using the xlink:title attribute while

the URL to the process description must be provided by the xlink:href attribute.

</documentation>

</annotation>

</element>

<element name="configuration" minOccurs="0" maxOccurs="1">

<annotation>

<documentation>

Value settings that further constrain the properties of the base process.

</documentation>

</annotation>

<complexType>

<sequence>

<element ref="sml:AbstractSettings"/>

</sequence>

</complexType>

</element>

<element name="featuresOfInterest" minOccurs="0" maxOccurs="1">

<annotation>

<documentation>

A collection of features relevant to a process (e.g. the Gulf of Mexico, the White House,

the set of all Fibonacci Numbers, etc.); can also support a sampling feature. The primary

purpose of the Features of Interest is to support discovery.

</documentation>

</annotation>

<complexType>

<sequence>

<element ref="sml:FeatureList"/>

</sequence>

</complexType>

</element>

<element name="inputs" minOccurs="0" maxOccurs="1">

<annotation>

<documentation>

The list of data components (and their properties and semantics) that the process will

accept as input; In the standard linear equation y=mx+b; x is the input, m and b are the

parameters, and y is the output.

</documentation>

</annotation>

<complexType>

<sequence>

<element ref="sml:InputList"/>

</sequence>

</complexType>

</element>

<element name="outputs" minOccurs="0" maxOccurs="1">

<annotation>

<documentation>

The list of data components (and their properties and semantics) that the process will

accept as output; In the standard linear equation y=mx+b; x is the input, m and b are the

parameters, and y is the output.

</documentation>

</annotation>

<complexType>

<sequence>

<element ref="sml:OutputList"/>

</sequence>

</complexType>

</element>

<element name="parameters" minOccurs="0" maxOccurs="1">

<annotation>

<documentation>

The list of data components (and their properties and semantics) that the process will

accept as parameters; In the standard linear equation y=mx+b; x is the input, m and b are

the parameters, and y is the output.

</documentation>

</annotation>

<complexType>

<sequence>

<element ref="sml:ParameterList"/>

</sequence>

</complexType>

</element>

<element name="modes" minOccurs="0" maxOccurs="unbounded">

<annotation>

<documentation>

A collection of parameters that can be set at once through the selection of a particular

predefined mode.

</documentation>

</annotation>

<complexType>

<sequence>

<element ref="sml:AbstractModes"/>

</sequence>

</complexType>

</element>

</sequence>

<attribute name="definition" type="anyURI"/>

</extension>

</complexContent>

</complexType>

<complexType name="AbstractProcessPropertyType">

<sequence minOccurs="0">

<element ref="sml:AbstractProcess"/>

</sequence>

<attributeGroup ref="gml:AssociationAttributeGroup"/>

<attributeGroup ref="gml:OwnershipAttributeGroup"/>

</complexType>

#### Definition

As with the *definition* attribute used in SWE Common simple and aggregate data components, the *definition* attribute for a *DescribedObject* provides the ability to link to a definition or classification within an online ontology. Relationships of this object with various other objects can then be inferred based on the ontology. There is some potential for overlap of functionality between the *definition* attribute and the *identification* and *classification* properties. Some communities may prefer to primarily use *classification* and *identification* elements, while others prefer to use the *definition* attribute or both.

#### TypeOf

The *typeOf* property provides a reference to a base process from which this process inherits properties and constraints. It is a key component in support of inheritance as described in the models in Clause 7.2.3.3.

Two pieces of information required in order to reference a base process instance, the uniqueID of the process and a resolvable URL reference to the process description. These shall be provided by the *xlink:title* and *xlink:href* attributes, respectively.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/typeOfReference> |
| 1. The *typeOf* property shall require meaningful values for the *xlink:title* and *xlink:href* attributes. The uniqueID of the referenced process, given by its *gml:identifier* property, shall be the value of the *xlink:title* attribute, while a resolvable URL to the reference process description shall be the value of the *xlink:href* attribute. |

An example of the *typeOf* property is given below:

<sml:typeOf xlink:title="urn:heath:2070"

xlink:href="http://www.sensors.ws/examples/sensorML-2.0/configuration/gamma2070.xml"/>

#### Abstract Configuration

The optional *configuration* property takes an *AbstractConfiguration* as its value, which provides a placeholder for configuration information in the *AbstractProcess*. A concrete class supporting configuration will be provided in a higher-level conformance class in Requirements Class: Configurable Process Schema in Clause 8.6.

#### FeatureOfInterest

The *featureOfInterest* property and the *FeatureList* element are XML Schema implementations of the UML classes defined in clause 7.2.3.1. The *featureOfInterest* property takes a *FeatureList* as its value. The *FeatureList* *member* property takes any object derived from GML *AbstractFeature* as its value. This feature can be described inline, but will most often be provided by reference using the *xlink:href* attribute.

The XML snippet for the *FeatureList* element and its corresponding complex types is shown below.

<element name="FeatureList" type="sml:FeatureListType" substitutionGroup="sml:AbstractMetadataList"/>

<complexType name="FeatureListType">

<complexContent>

<extension base="sml:AbstractMetadataListType">

<sequence>

<element name="member" type="gml:FeaturePropertyType" minOccurs="1"

maxOccurs="unbounded"/>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="FeatureListPropertyType">

<sequence minOccurs="0">

<element ref="sml:FeatureList"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

An example for a Feature-of-Interest list is given below. In this case, all features are by reference.

<sml:featureOfInterest>

<sml:FeatureList>

<sml:member xlink:arcrole="http://www.opengis.net/def/property/OGC//station"

xlink:title="urn:myDomain:station:A209"

xlink:href="http://myDomain.com/features/officeA209.xml"/>

<sml:member xlink:arcrole="http://www.opengis.net/def/property/OGC//observedFeature"

xlink:title="urn:mmi:features:GulfOfMexico"

xlink:href="http://mmi.org/features/GulfOfMexico.xml"/>

</sml:FeatureList>

</sml:featureOfInterest>

To better understand the role that the feature of interest plays with regard to the process, the *xlink:arcrole* attribute of the *member* property shall be used to specify this relationship. To aid in discovery, the unique ID or name of the feature shall be provided in the *xlink:title* attribute if it exists.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/foiArcroleAndTitle> |
| 1. Regardless of whether a feature of interest is described inline or provided by reference, the *xlink:arcrole* attribute of the *member* property of the *FeatureList* shall be used to specify the relationship of the associated feature to the process. If a unique identifier or name for the feature of interest exists, it shall be the value of the *xlink:title* of the *member* property of the *FeatureList*. |

#### Inputs, Outputs, and Parameters

The *input, output,* and *parameter* properties and the *InputList, OutputList,* and *ParameterList* elements are XML Schema implementations of the UML classes defined in clause 7.2.3.1. The *input, output,* and *parameter* properties takes *InputList, OutputList,* and *ParameterList* elements as their respective value. The *member* properties of these lists take any element of the *DataComponentOrObservable* Union as their value. This union and its components will be discussed in more detail in subsequent sections.

The XML snippets for the *InputList, OutputList,* and *ParameterList* elements and their corresponding complex types are shown below:

*Inputs:*

<element name="InputList" type="sml:InputListType" substitutionGroup="swe:AbstractSWE"/>

<complexType name="InputListType">

<complexContent>

<extension base="swe:AbstractSWEType">

<sequence>

<element name="input" minOccurs="1" maxOccurs="unbounded">

<complexType>

<complexContent>

<extension base="sml:DataComponentOrObservablePropertyType">

<attribute name="name" type="NCName" use="required"/>

</extension>

</complexContent>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="InputListPropertyType">

<sequence minOccurs="0">

<element ref="sml:InputList"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

*Outputs:*

<element name="OutputList" type="sml:OutputListType" substitutionGroup="swe:AbstractSWE"/>

<complexType name="OutputListType">

<complexContent>

<extension base="swe:AbstractSWEType">

<sequence>

<element name="output" minOccurs="1" maxOccurs="unbounded">

<complexType>

<complexContent>

<extension base="sml:DataComponentOrObservablePropertyType">

<attribute name="name" type="NCName" use="required"/>

</extension>

</complexContent>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="OutputListPropertyType">

<sequence minOccurs="0">

<element ref="sml:OutputList"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

*Parameters:*

<element name="ParameterList" type="sml:ParameterListType" substitutionGroup="swe:AbstractSWE"/>

<complexType name="ParameterListType">

<complexContent>

<extension base="swe:AbstractSWEType">

<sequence>

<element name="parameter" minOccurs="1" maxOccurs="unbounded">

<complexType>

<complexContent>

<extension base="sml:DataComponentOrObservablePropertyType">

<attribute name="name" type="NCName" use="required"/>

</extension>

</complexContent>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="ParameterListPropertyType">

<sequence minOccurs="0">

<element ref="sml:ParameterList"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

An example of inputs, outputs, and parameters from a particular process is given below (in this case, a gamma radiation sensor):

<!-- =================== -->

<!-- Inputs -->

<!-- =================== -->

<sml:inputs>

<sml:InputList>

<sml:input name="gammaRadiation">

<sml:ObservableProperty definition="http://www.opengis.net/def/property/OGC/0/radiation"/>

</sml:input>

</sml:InputList>

</sml:inputs>

<!-- ===================== -->

<!-- outputs -->

<!-- ===================== -->

<sml:outputs>

<sml:OutputList>

<sml:output name="dose">

<swe:DataRecord>

<swe:field name="averageDose">

<swe:Quantity definition="http://sensors.ws/ont/SWE/sensor-property/DoseRate.html">

<swe:uom code="uR/min"/>

</swe:Quantity>

</swe:field>

<swe:field name="InstantaneousDose">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/radiationDose">

<swe:uom code="uR"/>

</swe:Quantity>

</swe:field>

</swe:DataRecord>

</sml:output>

</sml:OutputList>

</sml:outputs>

<!-- ======================== -->

<!-- Parameters -->

<!-- ======================== -->

<sml:parameters>

<sml:ParameterList>

<sml:parameter name="energyResponse">

<swe:DataArray definition="http://sensors.ws/spectralResponse">

<swe:description>The normalized energy response per KeV</swe:description>

<swe:elementCount>

<swe:Count>

<swe:value>7</swe:value>

</swe:Count>

</swe:elementCount>

<swe:elementType name="energyResponse">

<swe:DataRecord>

<swe:label>Normalize Energy Response</swe:label>

<swe:field name="radiationEnergy">

<swe:Quantity definition="http://sensor.ws/def/radiationEnergy">

<swe:label>Radiation Energy</swe:label>

<swe:uom code="KeV"/>

</swe:Quantity>

</swe:field>

<swe:field name="relativeResponse">

<swe:Quantity definition="http://sensor.ws/def/relativeResponse">

<swe:label>Relative Response</swe:label>

<swe:uom code="%"/>

</swe:Quantity>

</swe:field>

</swe:DataRecord>

</swe:elementType>

<swe:encoding>

<swe:TextEncoding blockSeparator="&#10;" tokenSeparator=","/>

</swe:encoding>

<swe:values>

10.0,73 17.5,89.5 20.0,94.0 30.,95.5 40.0,96.0 50.0,96.0 100.0,94.0

</swe:values>

</swe:DataArray>

</sml:parameter>

</sml:ParameterList>

</sml:parameters>

##### Data Component Union

The *DataComponentOrObservable* group provides three choices to serve as process inputs, outputs, and parameters. These include *swe:AbstractDataComponent*, *sml:ObservableProperty*, and *sml:DataInterface*. These will each be discussed further in the following sections.

The XML snippet defining the *DataComponentOrObservable* group is given below:

<group name="DataComponentOrObservable">

<choice>

<element ref="swe:AbstractDataComponent">

<annotation>

<documentation>

A single digital number (DN) or aggregate of DNs that represent the value of some property.

Single data components can be of type Quantity, Count, Category, Boolean, Text, or Time; these

can be aggregated in records, arrays, vector, and matrices.

</documentation>

</annotation>

</element>

<element ref="sml:ObservableProperty">

<annotation>

<documentation>

A physical property of the environment that can be observed by an appropriate detector (e.g.

temperature, pressure, etc.); Typically,an ObservableProperty serves as the input of a detector

and the output of an actuator.

</documentation>

</annotation>

</element>

<element ref="sml:DataInterface">

<annotation>

<documentation>

A data interface serves as an intermediary between the pure digital domain and the physical

domain where DN are encoded into a format and perhaps transmitted through physical

connections using some well-defined protocol. The DataInterface element allows one to define

the components, semantics, encoding, connections, and protocol at an input, output, or parameter

port.

</documentation>

</annotation>

</element>

</choice>

</group>

<complexType name="DataComponentOrObservablePropertyType">

<sequence minOccurs="0">

<group ref="sml:DataComponentOrObservable"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

##### ObservableProperty

The *ObservableProperty* element is an XML encoding of the model defined in Clause 7.2.1 and discussed more in Clause 7.2.3.1. The *ObservableProperty* is used to represent an observable property or state in the environment. It is often used as an input field (e.g. stimulus) for a detector or the output field (e.g. action) of an actuator.

The XML snippet defining *ObservableProperty* and its associated complex types is shown below:

<element name="ObservableProperty" type="sml:ObservablePropertyType"

substitutionGroup="swe:AbstractSWEIdentifiable">

<annotation>

<documentation>

A physical property that can be observed and possibly measured (e.g. temperature, color, position). An

ObservableProperty has unambiguous definition, but does not have units of measure.

</documentation>

</annotation>

</element>

<complexType name="ObservablePropertyType">

<complexContent>

<extension base="swe:AbstractSWEIdentifiableType">

<attribute name="definition" type="anyURI" use="required"/>

</extension>

</complexContent>

</complexType>

<complexType name="ObservablePropertyPropertyType">

<sequence minOccurs="0">

<element ref="sml:ObservableProperty"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

The *ObservableProperty* element requires a URL as the value of its definition attribute, which shall resolve to a definition for the observable within an online dictionary or ontology.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/observableDefinition> |
| 1. The *ObservableProperty* element shall include the *definition* attribute that shall take as its value, a resolvable URL referencing the definition of the observable within an online dictionary or ontology. |

An minimal example of the use of *ObservableProperty* as a value for an input property is given below:

<sml:input name="temperature">

<sml:ObservableProperty definition="http://www.opengis.net/def/property/OGC/0/AtmosphericTemperature"/>

</sml:input>

##### SWE Common Data

SWE Common data types support the description and encoding of determined values, those measured or calculated by a physical or computational process. In addition to the those properties described in ObservableProperty, SWE Common data types can also support other properties such as units of measure, constraints, quality indicators, and values. It is highly recommended that one become familiar with the SWE Common Data specification in OGC 08-094.

In addition to simple data types such as *Quantity*, *Count*, *Boolean*, *Category*, *Time*, and *Text*, SWE Common Data also supports several aggregate data types, such as *DataRecord*, *DataArray*, *Vector*, and *Matrix*. These allow appropriate grouping of data components, such as a *DataRecord* including an instantaneous snapshot of the atmosphere (e.g. temperature, pressure, wind direction, and wind speed), a *DataArray* providing the axes definitions and values for a calibration curve, a *Vector* providing the GPS location (e.g. latitude, longitude, and altitude) of a dynamic platform, or a *Matrix* providing the covariance of a set of measurements.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/DataRecord> |
| 1. Input, output, and parameter data components that are dependent on one another or represent the state at a given time, shall be surrounded by an appropriate aggregate data component, such as *swe:DataRecord*, *swe:Vector*, or *swe:Matrix*. |

The following example for a wind chill calculation process uses only SWE Common *Quantity* elements for inputs and outputs. Note that the input fields are surrounded by a *swe:DataRecord* element since the temperature and wind speed fields express the condition of the environment at a given time instance.

<!--================ -->

<!-- Inputs -->

<!-- ================ -->

<sml:inputs>

<sml:InputList>

<sml:input name="chillInputs">

<swe:DataRecord>

<swe:field name="temperature">

<swe:Quantity definition="http://sweet.jpl.nasa.gov/2.2/quanTemperature.owl#Temperature">

<swe:uom code="cel"/>

</swe:Quantity>

</swe:field>

<swe:field name="windSpeed">

<swe:Quantity definition="http://sweet.jpl.nasa.gov/2.2/quanSpeed.owl#WindSpeed">

<swe:uom code="m/s"/>

</swe:Quantity>

</swe:field>

</swe:DataRecord>

</sml:input>

</sml:InputList>

</sml:inputs>

<!-- ================ -->

<!-- Outputs -->

<!-- ================ -->

<sml:outputs>

<sml:OutputList>

<sml:output name="windChill">

<swe:Quantity definition="http://sweet.jpl.nasa.gov/2.2/quanTemperature.owl#WindChill">

<swe:uom code="cel"/>

</swe:Quantity>

</sml:output>

</sml:OutputList>

</sml:outputs>

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/VectorUse> |
| 1. A *swe:Vector* shall be used for any input, output, or parameter value that requires position to be specified relative to a specific axis of a reference frame. |

An example of position output provided as output of a system is given below. This example uses both Vector and DataRecord elements to group the fields appropriately.

<sml:output>

<swe:DataRecord>

<swe:field name="location">

<swe:Vector definition="http://www.opengis.net/def/property/OGC/0/SensorLocation"

referenceFrame="http://www.opengis.net/def/crs/EPSG/6.7/4979" localFrame="#SENSOR\_FRAME">

<swe:coordinate name="Lat">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC//latitude" axisID="Lat">

<swe:uom code="deg"/>

</swe:Quantity>

</swe:coordinate>

<swe:coordinate name="Lon">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC//longitude" axisID="Long">

<swe:uom code="deg"/>

</swe:Quantity>

</swe:coordinate>

<swe:coordinate name="Alt">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC//altitude" axisID="Alt">

<swe:uom code="m"/>

</swe:Quantity>

</swe:coordinate>

</swe:Vector>

</swe:field>

<swe:field name="orientation">

<swe:Vector definition="http://www.opengis.net/def/property/OGC/0/SensorOrientation"

referenceFrame="http://www.opengis.net/def/crs/NED" localFrame="#SENSOR\_FRAME">

<swe:coordinate name="TrueHeading">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC//trueHeading" axisID="Z">

<swe:uom code="deg"/>

</swe:Quantity>

</swe:coordinate>

<swe:coordinate name="Pitch">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC//pitch" axisID="Y">

<swe:uom code="deg"/>

</swe:Quantity>

</swe:coordinate>

</swe:Vector>

</swe:field>

</swe:DataRecord>

</sml:output>

##### Data Interface

The *DataInterface* element is an XML encoding of the model defined in Clause 7.10. *DataInterface* describes the data components as described in the previous clause, but also provides a description of the data encoding of a datastream flowing to or from a process interface as well as a description of interface characteristics itself (e.g. the communication protocols and perhaps physical nature as outlined in the OSI interface stack).

The XML snippet for the *DataInterface* element and its associated complex types is shown below:

<element name="DataInterface" type="sml:DataInterfaceType" substitutionGroup="swe:AbstractSWEIdentifiable">

<annotation>

<documentation>

The DataInterface description provides information sufficient for "plug-and-play" access to and parsing of

the data stream or file at the particular IO port.

</documentation>

</annotation>

</element>

<complexType name="DataInterfaceType">

<complexContent>

<extension base="swe:AbstractSWEIdentifiableType">

<sequence>

<element name="data" type="swe:DataStreamPropertyType">

<annotation>

<documentation>

The definition of the digital data components and encoding accessed through the data

interface.

</documentation>

</annotation>

</element>

<element name="interfaceParameters" type="swe:DataRecordPropertyType" minOccurs="0"

maxOccurs="1">

<annotation>

<documentation>

A set of property values that define the type and configuration of a data interface (e.g. the

port settings of an RS232 interface).

</documentation>

</annotation>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="DataInterfacePropertyType">

<sequence minOccurs="0">

<element ref="sml:DataInterface"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

The *DataInterface* essentially consists of a required *data* property, which takes a SWE Common *DataStream* element as its value, and an optional *interfaceParameters* property that defines the interface as a set of fields within a SWE Common *DataRecord*. This specification does not define the specific fields required to define the interface, but it is expected that one or more profiles will be defined for common interface definitions.

In the following example, the *values* property reference a RESTful resource (e.g. a daily record of weather) available on the web through html protocol. This example is for a network of weather sensors; thus the network stream includes station ID and location as part of the data components. In this case, a description of the InterfaceParameters is neither required nor useful.

<sml:output name="sensorNetworkStream">

<sml:DataInterface>

<sml:data>

<swe:DataStream>

<swe:description>

This stream is for a sensor network where all output are homogeneous;

The station ID and location is provided with each reading;

</swe:description>

<swe:elementType name="weather\_data">

<swe:DataRecord>

<swe:label>Atmospheric Conditions</swe:label>

<swe:field name="time">

<swe:Time

definition="http://www.opengis.net/def/property/OGC/0/SamplingTime">

<swe:uom

xlink:href="http://www.opengis.net/def/uom/ISO-8601/0/Gregorian"/>

</swe:Time>

</swe:field>

<swe:field name="sensorID">

<swe:Text

definition="http://www.opengis.net/def/property//OGC/0/sensorUID"/>

</swe:field>

<swe:field name="location">

<swe:Vector

definition="http://www.opengis.net/def/property/OGC/0/PlatformLocation"

referenceFrame="http://www.opengis.net/def/crs/EPSG/0/4979">

<swe:coordinate name="lat">

<swe:Quantity

definition="http://sweet.jpl.nasa.gov/2.0/spaceCoordinates.owl#Latitude"

axisID="Lat">

<swe:uom code="deg"/>

</swe:Quantity>

</swe:coordinate>

<swe:coordinate name="lon">

<swe:Quantity

definition="http://sweet.jpl.nasa.gov/2.0/spaceCoordinates.owl#Longitude"

axisID="Long">

<swe:uom code="deg"/>

</swe:Quantity>

</swe:coordinate>

<swe:coordinate name="alt">

<swe:Quantity

definition="http://sweet.jpl.nasa.gov/2.0/spaceExtent.owl#Altitude"

axisID="h">

<swe:uom code="m"/>

</swe:Quantity>

</swe:coordinate>

</swe:Vector>

</swe:field>

<swe:field name="temp">

<swe:Quantity

definition="http://mmisw.org/ont/cf/parameter/air\_temperature">

<swe:uom code="Cel"/>

</swe:Quantity>

</swe:field>

<swe:field name="pressure">

<swe:Quantity

definition="http://mmisw.org/ont/cf/parameter/barometric\_pressure">

<swe:uom code="kPa"/>

</swe:Quantity>

</swe:field>

<swe:field name="wind\_speed">

<swe:Quantity

definition="http://mmisw.org/ont/cf/parameter/wind\_speed">

<swe:uom code="km/h"/>

</swe:Quantity>

</swe:field>

<swe:field name="wind\_dir">

<swe:Quantity

definition="http://mmisw.org/ont/cf/parameter/wind\_to\_direction">

<swe:uom code="deg"/>

</swe:Quantity>

</swe:field>

</swe:DataRecord>

</swe:elementType>

<swe:encoding>

<swe:TextEncoding tokenSeparator="," blockSeparator=""/>

</swe:encoding>

<swe:values xlink:href="http://mySensors.com/weatherNetwork201.txt"/>

</swe:DataStream>

</sml:data>

</sml:DataInterface>

</sml:output>

The returned resource “weatherNetwork201.txt” might return the most recent reading from the network and look like:

2009-05-23T19:36:15Z,urn:myNet:stations:76455,35.4,135.6,5.0,25.4,100.3,7.31,270.8

2009-05-23T19:36:15Z,urn:myNet:stations:55577,34.1,138.9,4.1,25.5,100.5,7.54,271.4

2009-05-23T19:38:15Z,urn:myNet:stations:85643,43.9,141.0,3.8,25.7,100.1,7.44,260.2

2009-05-23T19:39:15Z,urn:myNet:stations:22298,46.7,140.0,1.2,26.5,100.6,7.30,271.9

2009-05-23T19:40:15Z,urn:myNet:stations:92675,43.1,131.0,6.7,25.5,100.2,7.54,271.0

The following example also references an external source for the values of the stream, but instead of a static resource, it references a Real-Time-Protocol (RTP) server that will continue to send real-time measurements until the client disconnects.

<sml:output name="gammaRadiation">

<sml:DataInterface>

<!-- data description -->

<sml:data>

<swe:DataStream>

<swe:elementType name="temperatureStream">

<swe:DataRecord>

<swe:field name="averageDose">

<swe:Quantity definition="http://sensors.ws/ont/SWE/sensor-property/DoseRate.html">

<swe:label>Average Dose of Gamma Radiation</swe:label>

<swe:uom code="uR/min"/>

</swe:Quantity>

</swe:field>

<swe:field name="InstantaneousDose">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/radiationDose">

<swe:label>Instantaneous Dose of Gamma Radiation</swe:label>

<swe:uom code="uR"/>

</swe:Quantity>

</swe:field>

</swe:DataRecord>

</swe:elementType>

<!-- encoding description -->

<swe:encoding>

<swe:TextEncoding tokenSeparator="," blockSeparator=" "/>

</swe:encoding>

<swe:values xlink:href="rtp://myServer.com:4563/sensor/02080"/>

</swe:DataStream>

</sml:data>

</sml:DataInterface>

</sml:output>

Once one establishes connection to such a server, the server would then begin streaming over real-time values for the data as they become available. Such a stream might look like:

7248,26 7248,26 7248,28 7251,29 7251,30 ... [continues until disconnected]

Since SWE Common also supports binary encodings, the same sensor system could describe binary data, as in the current example:

<sml:output name="gammaRadiation">

<sml:DataInterface>

<!-- data description -->

<sml:data>

<swe:DataStream>

<swe:elementType name="gammaRadiation">

<swe:DataRecord>

<swe:field name="averageDose">

<swe:Quantity definition="http://sensors.ws/ont/SWE/sensor-property/DoseRate.html">

<swe:label>Average Dose of Gamma Radiation</swe:label>

<swe:uom code="uR/min"/>

</swe:Quantity>

</swe:field>

<swe:field name="InstantaneousDose">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/radiationDose">

<swe:label>Instantaneous Dose of Gamma Radiation</swe:label>

<swe:uom code="uR"/>

</swe:Quantity>

</swe:field>

</swe:DataRecord>

</swe:elementType>

<swe:encoding>

<swe:BinaryEncoding byteEncoding="raw" byteOrder="bigEndian">

<swe:member>

<swe:Component ref="averageDose"

dataType="http://www.opengis.net/def/dataType/OGC/0/float32"/>

</swe:member>

<swe:member>

<swe:Component ref="instantaneousDose"

dataType="http://www.opengis.net/def/dataType/OGC/0/float32"/>

</swe:member>

</swe:BinaryEncoding>

</swe:encoding>

<swe:values xlink:href="rtp://myServer.com:4563/sensor/02080"/>

</swe:DataStream>

</sml:data>

</sml:DataInterface>

</sml:output>

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/DataStreamURL> |
| 1. When the values of a *DataStream* can be referenced by a resolvable URL, that URL shall be the value of of the *xlink:href* attribute in the *value* property of the *DataStream*. |

Using the SWE Common Data element, *DataChoice*, it is also possible to define and stream a collection of disparate packets within the same *DataStream*. According to the SWE Common Data specification, the structure of each packet shall be defined as a separate *item* within the *DataChoice* object. The subsequent values of each packet shall be preceded by the item name, as in the example XML and data stream below:

<sml:output name="tempAndWind">

<sml:DataInterface>

<sml:data>

<swe:DataStream>

<swe:elementType name="message">

<swe:DataChoice>

<!-- packet definition 1 - temperature -->

<swe:item name="TEMP">

<swe:DataRecord>

<swe:label>Temperature Measurement</swe:label>

<swe:field name="time">

<swe:Time definition="http://www.opengis.net/def/property/OGC/0/SamplingTime">

<swe:uom xlink:href="http://www.opengis.net/def/uom/ISO-8601/0/Gregorian"/>

</swe:Time>

</swe:field>

<swe:field name="temp">

<swe:Quantity definition="http://mmisw.org/ont/cf/parameter/air\_temperature">

<swe:uom code="Cel"/>

</swe:Quantity>

</swe:field>

</swe:DataRecord>

</swe:item>

<!-- packet definition 2 - wind -->

<swe:item name="WIND">

<swe:DataRecord>

<swe:label>Wind Measurement</swe:label>

<swe:field name="time">

<swe:Time definition="http://www.opengis.net/def/property/OGC/0/SamplingTime">

<swe:uom xlink:href="http://www.opengis.net/def/uom/ISO-8601/0/Gregorian"/>

</swe:Time>

</swe:field>

<swe:field name="wind\_speed">

<swe:Quantity definition="http://mmisw.org/ont/cf/parameter/wind\_speed">

<swe:uom code="km/h"/>

</swe:Quantity>

</swe:field>

<swe:field name="wind\_dir">

<swe:Quantity definition="http://mmisw.org/ont/cf/parameter/wind\_to\_direction">

<swe:uom code="deg"/>

</swe:Quantity>

</swe:field>

</swe:DataRecord>

</swe:item>

</swe:DataChoice>

</swe:elementType>

<swe:encoding>

<swe:TextEncoding tokenSeparator="," blockSeparator=""/>

</swe:encoding>

<swe:values xlink:href="rtp://mySensors.com:4356/76455"/>

</swe:DataStream>

</sml:data>

</sml:DataInterface>

</sml:output>

With an example streaming values looking like:

TEMP,2009-05-23T19:36:15Z,25.5

TEMP,2009-05-23T19:37:15Z,25.6

WIND,2009-05-23T19:37:17Z,56.3,226.3

TEMP,2009-05-23T19:38:15Z,25.5

WIND,2009-05-23T19:38:16Z,58.4,225.1

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/MultiplexedDataStream> |
| 1. When the values of a *DataStream* consist of a series of multiplexed packets, the value of the *elementType* property shall be specified using the SWE Common Data *DataChoice* element. |

In addition to online interfaces to data, *DataInterface* can also support physical interfaces such as RS232 or USB. In such cases, the *value* property is ignored, and the *interfaceParameters* property of the *DataInterface* element shall be used to specify the interface characteristics.

An example of an interface description is given below. Since interface description profiles will be created under separate documents, the following example is informative, not normative.

<sml:interfaceParameters>

<swe:DataRecord definition="http://www.opengis.net/def/profiles/OGC/0/serialPortSettings">

<swe:field name="portType">

<swe:Category definition="http://www.opengis.net/def/property/OGC/0/serialPortType">

<swe:label>Port Type</swe:label>

<swe:value>RS232</swe:value>

</swe:Category>

</swe:field>

<swe:field name="portNumber">

<swe:Count definition="http://www.opengis.net/def/property/OGC/0/portNumber">

<swe:label>Port Number</swe:label>

<swe:value>0</swe:value>

</swe:Count>

</swe:field>

<swe:field name="baudRate">

<swe:Count definition="http://www.opengis.net/def/property/OGC/0/baudRate">

<swe:label>Baud Rate</swe:label>

<swe:value>9600</swe:value>

</swe:Count>

</swe:field>

<swe:field name="bits">

<swe:Count definition="http://www.opengis.net/def/property/OGC/0/DataBitSize">

<swe:label>Data Bits</swe:label>

<swe:value>8</swe:value>

</swe:Count>

</swe:field>

<swe:field name="parity">

<swe:Category definition="http://www.opengis.net/def/property/OGC/0/baudRate">

<swe:label>Parity</swe:label>

<swe:value>N</swe:value>

</swe:Category>

</swe:field>

<swe:field name="stopBits">

<swe:Count definition="http://www.opengis.net/def/property/OGC/0/stopBits">

<swe:label>Stop Bits</swe:label>

<swe:value>1</swe:value>

</swe:Count>

</swe:field>

</swe:DataRecord>

</sml:interfaceParameters>

#### Modes

The *AbstractModes* element provides a base class from which will be derived a concrete *Modes* class in the higher-level conformance class specified by the Requirements Class: Configurable Process Schema in Clause 8.6.

The XML Schema implementation of AbstractModes and its related complex type is given below:

<element name="AbstractModes" type="sml:AbstractModesType" substitutionGroup="swe:AbstractSWE"/>

<complexType name="AbstractModesType">

<complexContent>

<extension base="swe:AbstractSWEType"/>

</complexContent>

</complexType>

<complexType name="AbstractModesPropertyType">

<sequence minOccurs="0">

<element ref="sml:AbstractModes"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

## Requirements Class: Simple Process Schema

|  |  |
| --- | --- |
| Requirements Class | |
| http://www.opengis.net/spec/SensorML/2.0/req/xml/simpleProcess | |
| Target Type | XML Instance |
| **Dependency** | <http://www.opengis.net/spec/SensorML/2.0/req/model/simpleProcess> |
| **Dependency** | <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess> |

XML Schema elements and types defined in the “*simple\_process.xsd*” schema file implement all classes defined respectively in the “simpleProcess” UML package defined in Clause 7.3.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/simpleProcess/schema-valid> |
| 1. The XML instance shall be valid with respect to the XML grammar defined in the “simple\_process.xsd”, as well as satisfy all Schematron patterns defined in “simple\_process.sch”. |

The following XML snippet provides the appropriate header and import statements for the simple\_process.xsd:

<schema xmlns="http://www.w3.org/2001/XMLSchema" xmlns:sml="http://www.opengis.net/sensorML/2.0"

xmlns:gml="http://www.opengis.net/gml/3.2" xmlns:swe="http://www.opengis.net/swe/2.0"

targetNamespace="http://www.opengis.net/sensorML/2.0" elementFormDefault="qualified"

attributeFormDefault="unqualified">

<annotation>

<documentation>

The elements of a concrete simple non-physical process derived from the core process model.

</documentation>

</annotation>

<import namespace="http://www.opengis.net/gml/3.2"

schemaLocation="http://schemas.opengis.net/gml/3.2.1/gml.xsd"/>

<import namespace="http://www.opengis.net/swe/2.0"

schemaLocation="http://schemas.opengis.net/sweCommon/2.0/swe.xsd"/>

<include schemaLocation="core.xsd"/>

### Simple Process

The “*SimpleProcesss*” element is the XML schema implementation of the “*SimpleProcess*” UML class defined in clause 7.3.1. The schema snippet for this element and its corresponding complex type is shown below:

<element name="SimpleProcess" type="sml:SimpleProcessType" substitutionGroup="sml:AbstractProcess"/>

<complexType name="SimpleProcessType">

<complexContent>

<extension base="sml:AbstractProcessType">

<sequence>

<element name="method" type="sml:ProcessMethodPropertyType" minOccurs="0" maxOccurs="1"/>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="SimpleProcessPropertyType">

<sequence minOccurs="0">

<element ref="sml:SimpleProcess"/>

</sequence>

<attributeGroup ref="gml:AssociationAttributeGroup"/>

<attributeGroup ref="gml:OwnershipAttributeGroup"/>

</complexType>

The *SimpleProcess* element and complex type is derived from *AbstractProcess* and adds a *method* property to the properties inherited from *AbstractProcess*. The *method* property takes a *ProcessMethod* element as its value.

### Process Method

The “*ProcessMethod*” element is the XML schema implementation of the “*ProcessMethod*” UML class defined in clause 7.3.2. The schema snippet for this element and its corresponding complex type is shown below:

<element name="ProcessMethod" type="sml:ProcessMethodType"

substitutionGroup="swe:AbstractSWEIdentifiable">

<annotation>

<documentation>

The method describes (as an algorithm or text) how the process takes the input and parameter values

and generates output values.

</documentation>

</annotation>

</element>

<complexType name="ProcessMethodType">

<complexContent>

<extension base="swe:AbstractSWEIdentifiableType">

<sequence>

<element name="algorithm" minOccurs="0" maxOccurs="unbounded">

<complexType>

<sequence>

<element ref="sml:AbstractAlgorithm"/>

</sequence>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="ProcessMethodPropertyType">

<sequence minOccurs="0">

<element ref="sml:ProcessMethod"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

<element name="AbstractAlgorithm" type="sml:AbstractAlgorithmType" abstract="true"

substitutionGroup="gml:AbstractObject"/>

<complexType name="AbstractAlgorithmType" abstract="true">

<sequence/>

<attribute ref="gml:id" use="optional"/>

</complexType>

<complexType name="AbstractAlgorithmPropertyType">

<sequence minOccurs="0">

<element ref="sml:AbstractAlgorithm"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

The *ProcessMethod* element is derived from *SWEIdentifiableType* and thus supports the *swe:identifier*, *swe:label*, and *swe:description* properties, as well as the *swe:extension* property, which supports the ability to specify community-specific XML elements for describing the method.

Furthermore, *ProcessMethod* has an *algorithm* property that takes an *AbstractAlgorithm* element as its value. It is anticipated that profiles will be specified in separate specifications that will support algorithms descriptions through schema such as MathML.

## Requirements Class: Aggregate Process Schema

|  |  |
| --- | --- |
| Requirements Class | |
| http://www.opengis.net/spec/SensorML/2.0/req/xml/aggregateProcess | |
| Target Type | XML Instance |
| **Dependency** | <http://www.opengis.net/spec/SensorML/2.0/req/model/aggregateProcess> |
| **Dependency** | <http://www.opengis.net/spec/SensorML/2.0/req/xml/simpleProcess> |

XML Schema elements and types defined in the “*aggregate\_process.xsd*” schema file implement all classes defined respectively in the “aggregateProcess” UML package defined in Clause 7.4.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/aggregateProcess/schema-valid> |
| 1. The XML instance shall be valid with respect to the XML grammar defined in the “aggregate\_process.xsd”, as well as satisfy all Schematron patterns defined in “aggregate\_process.sch”. |

The following XML snippet provides the appropriate header and import statements for the simple\_process.xsd:

<schema xmlns="http://www.w3.org/2001/XMLSchema" xmlns:sml="http://www.opengis.net/sensorML/2.0"

xmlns:gml="http://www.opengis.net/gml/3.2" xmlns:swe="http://www.opengis.net/swe/2.0"

targetNamespace="http://www.opengis.net/sensorML/2.0" elementFormDefault="qualified"

attributeFormDefault="unqualified">

<annotation>

<documentation>

The elements of a concrete aggregate non-physical process derived from the core process model.

</documentation>

</annotation>

<import namespace="http://www.opengis.net/gml/3.2"

schemaLocation="http://schemas.opengis.net/gml/3.2.1/gml.xsd"/>

<import namespace="http://www.opengis.net/swe/2.0"

schemaLocation="http://schemas.opengis.net/sweCommon/2.0/swe.xsd"/>

<include schemaLocation="simple\_process.xsd"/>

### Aggregate Process

The “*AggregateProcess*” element is the XML schema implementation of the “*AggregateProcess*” UML class defined in clause 7.4.1. The schema snippet for this element and its corresponding complex type is shown below:

<element name="AggregateProcess" type="sml:AggregateProcessType" substitutionGroup="sml:AbstractProcess">

<annotation>

<documentation>

A process that consist of a collection of linked component processes resulting in a specified output.

</documentation>

</annotation>

</element>

<complexType name="AggregateProcessType">

<complexContent>

<extension base="sml:AbstractProcessType">

<sequence>

<element name="components" type="sml:ComponentListPropertyType" minOccurs="0"

maxOccurs="1"/>

<element name="connections" type="sml:ConnectionListPropertyType" minOccurs="0"

maxOccurs="1">

<annotation>

<documentation>

The explicit definition of data links between outputs, inputs, and parameters of the

components within an aggregate process.

</documentation>

</annotation>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="AggregateProcessPropertyType">

<sequence minOccurs="0">

<element ref="sml:AggregateProcess"/>

</sequence>

<attributeGroup ref="gml:AssociationAttributeGroup"/>

<attributeGroup ref="gml:OwnershipAttributeGroup"/>

</complexType>

The *AggregateProcess* element and complex type is derived from *AbstractProcess* and adds *components* and *connections* properties to the properties inherited from *AbstractProcess*. The *components* and *connections* properties take *ComponentList* and *ConnectionList* as their values, respectively.

The following two examples show the same aggregate process. A graphic of this “Slice and Clip” *AggregateProcess* is shown in Figure 8.1. In this diagram, inputs to the aggregate process and its components are shown on the left of the object, while outputs are on the right and parameters are on top. In this example, the parameter values are set and constant, as shown by the values assigned them. However, parameters can be variable and supplied by connections as can inputs.

This diagram and the following SensorML instances illustrate that an AggregateProcess can have multiple components and connections that will be discussed in more detail in the following Sections 8.3.2 and 8.3.3. Notice that inputs, outputs, and parameters can be defined for the aggregate process as well as for the individual components.




Figure 8.1. A diagram showing the components and connections of the “Scale and Clip” AggregateProcess.

The first example provides a complete definition of the component processes and the setting of parameter values inline.

<?xml version="1.0" encoding="UTF-8"?>

<sml:AggregateProcess gml:id="scaleAndClip01"

xmlns:sml="http://www.opengis.net/sensorML/2.0"

xmlns:swe="http://www.opengis.net/swe/2.0"

xmlns:gml="http://www.opengis.net/gml/3.2"

xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"

xmlns:xlink="http://www.w3.org/1999/xlink"

xsi:schemaLocation="http://www.opengis.net/sensorML/2.0 ../../sensorML.xsd"

definition="http://sensors.ws/process/linearInterpolator">

<!-- ============================= -->

<!-- Descriptions -->

<!-- ============================= -->

<gml:description>

A simple aggregate process that scales according to linear equation y = 2.3x + 1.76 and then clips if below 15.0

In this example all processes are defined inline with no configuration settings. Parameter values are set inline.

</gml:description>

<gml:identifier codeSpace="uid">urn:myCompany:swe:process:scaleAndClip01</gml:identifier>

<gml:name>Scale and Clip Aggregate Process 01</gml:name>

<!-- ============================= -->

<!-- Aggregate Process Inputs -->

<!-- ============================= -->

<sml:inputs>

<sml:InputList>

<sml:input name="valueIn">

<swe:Quantity definition="http://sensors.ws/def/simpleDN">

<swe:uom code="any"/>

</swe:Quantity>

</sml:input>

</sml:InputList>

</sml:inputs>

<!-- ============================= -->

<!-- Aggregate Process Outputs -->

<!-- ============================= -->

<sml:outputs>

<sml:OutputList>

<sml:output name="valueOut">

<swe:Quantity definition="http://sensors.ws/def/simpleDN">

<swe:uom code="any"/>

</swe:Quantity>

</sml:output>

</sml:OutputList>

</sml:outputs>

<!-- ======================================= -->

<!-- Aggregate process components declared -->

<!-- ======================================== -->

<sml:components>

<sml:ComponentList >

<!-- Component 1 - Linear Interpolator -->

<sml:component name="scale">

<sml:SimpleProcess gml:id="linearInterpolator01"

definition="http://sensors.ws/process/linearInterpolator">

<!-- ============================= -->

<!-- Linear Interpolator Descriptions -->

<!-- ============================= -->

<gml:description>A linear interpolator based on equation y = mx + b </gml:description>

<gml:identifier codeSpace="uid">urn:myCompany:process:8755d73ab</gml:identifier>

<gml:name>Linear Equation 01</gml:name>

<!-- ============================= -->

<!-- Linear Interpolator Inputs -->

<!-- ============================= -->

<sml:inputs>

<sml:InputList>

<sml:input name="x">

<swe:Quantity definition="http://sensors.ws/def/xCoordinate">

<swe:uom code="any"/>

</swe:Quantity>

</sml:input>

</sml:InputList>

</sml:inputs>

<!-- ============================= -->

<!-- Linear Interpolator Outputs -->

<!-- ============================= -->

<sml:outputs>

<sml:OutputList>

<!-- scaled output value -->

<sml:output name="y">

<swe:Quantity definition="http://sensors.ws/def/simpleDN">

<swe:uom code="any"/>

</swe:Quantity>

</sml:output>

</sml:OutputList>

</sml:outputs>

<!-- ============================= -->

<!-- Linear Interpolator Parameters -->

<!-- ============================= -->

<sml:parameters>

<sml:ParameterList>

<sml:parameter name="slope-intercept">

<swe:DataRecord>

<swe:field name="slope">

<swe:Quantity definition="http://sensors.ws/def/linearSlope">

<swe:uom code="any"/>

<!-- slope value set inline -->

<swe:value>2.3</swe:value>

</swe:Quantity>

</swe:field>

<swe:field name="intercept">

<swe:Quantity definition="http://sensors.ws/def/linearAxisIntercept">

<!-- y-intercept value set inline -->

<swe:uom code="any"/>

<swe:value>1.76</swe:value>

</swe:Quantity>

</swe:field>

</swe:DataRecord>

</sml:parameter>

</sml:ParameterList>

</sml:parameters>

</sml:SimpleProcess>

</sml:component>

<!-- Component 2 - Threshold clipper -->

<sml:component name="clip">

<sml:SimpleProcess gml:id="thresholdClipper"

definition="http://sensors.ws/process/thresholdClipper">

<!-- ============================= -->

<!-- Threshold Clipper Descriptions -->

<!-- ============================= -->

<gml:description>

A process that clips anything below threshold;

values higher than threshold to passValue output;

Values below threshold sent to failValue output</gml:description>

<gml:identifier codeSpace="uid">urn:myCompany:swe:process:65d74a65c</gml:identifier>

<gml:name>Threshold Clipper 01</gml:name>

<!-- ============================= -->

<!-- Threshold Clipper Inputs -->

<!-- ============================= -->

<sml:inputs>

<sml:InputList>

<sml:input name="valueIn">

<swe:Quantity definition="http://sensors.ws/def/simpleDN">

<swe:uom code="any"/>

</swe:Quantity>

</sml:input>

</sml:InputList>

</sml:inputs>

<!-- ============================= -->

<!-- Threshold Clipper Outputs -->

<!-- ============================= -->

<sml:outputs>

<sml:OutputList>

<!-- output for values that pass -->

<sml:output name="passValue">

<swe:Quantity definition="http://sensors.ws/def/passValue">

<swe:uom code="any"/>

</swe:Quantity>

</sml:output>

<!-- output for values that fail -->

<sml:output name="failValue">

<swe:Quantity definition="http://sensors.ws/def/failValue">

<swe:uom code="any"/>

</swe:Quantity>

</sml:output>

</sml:OutputList>

</sml:outputs>

<!-- ============================= -->

<!-- Threshold Clipper Parameters -->

<!-- ============================= -->

<sml:parameters>

<sml:ParameterList>

<sml:parameter name="threshold">

<swe:Quantity definition="http://sensors.ws/def/lowerThreshold">

<swe:uom code="any"/>

<!-- threshold value set inline -->

<swe:value>15.0</swe:value>

</swe:Quantity>

</sml:parameter>

</sml:ParameterList>

</sml:parameters>

</sml:SimpleProcess>

</sml:component>

</sml:ComponentList>

</sml:components>

<!-- ======================================= -->

<!-- Aggregate process links declared -->

<!-- ======================================== -->

<sml:connections>

<sml:ConnectionList>

<!-- Connect AggregateProcess input to LinearInterpolator (scale) input -->

<sml:connection>

<sml:Link>

<sml:source>inputs/valueIn</sml:source>

<sml:destination>components/scale/inputs/x</sml:destination>

</sml:Link>

</sml:connection>

<!-- Connect LinearInterpolator (scale) output to ThresholdClipper (clip) input -->

<sml:connection>

<sml:Link>

<sml:source>components/scale/outputs/y</sml:source>

<sml:destination>components/clip/inputs/valueIn</sml:destination>

</sml:Link>

</sml:connection>

<!-- Connect ThresholdClipper (clip) passValue output to AggregateProcess passValue output -->

<sml:connection>

<sml:Link>

<sml:source>components/clip/outputs/passValue</sml:source>

<sml:destination>outputs/valueOut</sml:destination>

</sml:Link>

</sml:connection>

<!-- Note: ThresholdClipper (clip) failValue output is ignored in this example -->

</sml:ConnectionList>

</sml:connections>

</sml:AggregateProcess>

Typically, however, aggregate processes will consist of well-defined, modular component processes that exist in a process repository and can be referenced and configured using the *typeOf* and *configuration* properties, respectively (discussed in subsequent Section 8.6. The second example utilizes components that are externally defined but are referenced and configured within the aggregate process description.

<?xml version="1.0" encoding="UTF-8"?>

<sml:AggregateProcess gml:id="scaleAndClip06"

xmlns:sml="http://www.opengis.net/sensorML/2.0"

xmlns:swe="http://www.opengis.net/swe/2.0"

xmlns:gml="http://www.opengis.net/gml/3.2"

xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"

xmlns:xlink="http://www.w3.org/1999/xlink"

xsi:schemaLocation="http://www.opengis.net/sensorML/2.0 ../../sensorML.xsd"

definition="http://sensors.ws/process/linearInterpolator">

<!-- ============================= -->

<!-- Descriptions -->

<!-- ============================= -->

<gml:description>

A simple aggregate process that scales according to linear equation y = 2.3x + 1.76 and then clips if below 15.0

In this example all processes are defined externally and configured.

</gml:description>

<gml:identifier codeSpace="uid">urn:myCompany:swe:process:scaleAndClip02</gml:identifier>

<gml:name>Scale and Clip Aggregate Process 06</gml:name>

<!-- ============================= -->

<!-- Aggregate Process Inputs -->

<!-- ============================= -->

<sml:inputs>

<sml:InputList>

<sml:input name="valueIn">

<swe:Quantity definition="http://sensors.ws/def/simpleDN">

<swe:uom code="any"/>

</swe:Quantity>

</sml:input>

</sml:InputList>

</sml:inputs>

<!-- ============================= -->

<!-- Aggregate Process Outputs -->

<!-- ============================= -->

<sml:outputs>

<sml:OutputList>

<sml:output name="valueOut">

<swe:Quantity definition="http://sensors.ws/def/simpleDN">

<swe:uom code="any"/>

</swe:Quantity>

</sml:output>

</sml:OutputList>

</sml:outputs>

<!-- ======================================= -->

<!-- Aggregate process components declared -->

<!-- ======================================== -->

<sml:components>

<sml:ComponentList >

<!-- Component 1 - Linear Interpolator -->

<sml:component name="scale">

<sml:SimpleProcess gml:id="linearInterpolatorConfigured"

definition="http://sensors.ws/process/linearInterpolator">

<!-- ============================= -->

<!-- Linear Interpolator Descriptions -->

<!-- ============================= -->

<gml:description>A linear interpolator with slope of 2.3 and intercept of 1.76</gml:description>

<gml:identifier codeSpace="uid">urn:myCompany:swe:process:09h57b21</gml:identifier>

<gml:name>Linear Equation 01 Configured</gml:name>

<!-- ======================================== -->

<!-- Base process referenced and configured -->

<!-- ======================================== -->

<sml:typeOf xlink:title="urn:net:swe:process:linearEquation01"

xlink:href="http://sensors.ws/processes/LinearInterpolator01"/>

<sml:configuration>

<sml:Settings>

<sml:setValue ref="base/parameter/slope-intercept/slope">2.3</sml:setValue>

<sml:setValue ref="base/parameter/slope-intercept/intercept">1.76</sml:setValue>

</sml:Settings>

</sml:configuration>

</sml:SimpleProcess>

</sml:component>

<!-- Component 2 - Threshold clipper -->

<sml:component name="clip">

<sml:SimpleProcess gml:id="thresholdClipperConfigured"

definition="http://sensors.ws/process/thresholdClipper">

<!-- ============================= -->

<!-- Threshold Clipper Descriptions -->

<!-- ============================= -->

<gml:description>

A process that passes values of 15.0 and above to the passValue output;

</gml:description>

<gml:identifier codeSpace="uid">urn:myCompany:swe:process:0678b365a</gml:identifier>

<gml:name>Threshold Clipper 01 Configured</gml:name>

<!-- ======================================== -->

<!-- Base process referenced and configured -->

<!-- ======================================== -->

<sml:typeOf xlink:title="urn:net:swe:process:thresholdClip01"

xlink:href="http://sensors.ws/processes/ThresholdClipper01"/>

<sml:configuration>

<sml:Settings>

<sml:setValue ref="base/parameter/threshold">15.0</sml:setValue>

</sml:Settings>

</sml:configuration>

</sml:SimpleProcess>

</sml:component>

</sml:ComponentList>

</sml:components>

<!-- ======================================= -->

<!-- Aggregate process links declared -->

<!-- ======================================== -->

<sml:connections>

<sml:ConnectionList>

<!-- Connect AggregateProcess input to LinearInterpolator (scale) input -->

<sml:connection>

<sml:Link>

<sml:source>inputs/valueIn</sml:source>

<sml:destination>components/scale/inputs/x</sml:destination>

</sml:Link>

</sml:connection>

<!-- Connect LinearInterpolator (scale) output to ThresholdClipper (clip) input -->

<sml:connection>

<sml:Link>

<sml:source>components/scale/outputs/y</sml:source>

<sml:destination>components/clip/inputs/valueIn</sml:destination>

</sml:Link>

</sml:connection>

<!-- Connect ThresholdClipper (clip) passValue output to AggregateProcess passValue output -->

<sml:connection>

<sml:Link>

<sml:source>components/clip/outputs/passValue</sml:source>

<sml:destination>outputs/valueOut</sml:destination>

</sml:Link>

</sml:connection>

<!-- Note: ThresholdClipper (clip) failValue output is ignored in this example -->

</sml:ConnectionList>

</sml:connections>

</sml:AggregateProcess>

### Components

The *components* property and the *ComponentList* elements are XML Schema implementations of the UML classes defined in clause 7.4. The *components* property takes a *ComponentList* as its value. The *ComponentList* *component* property takes an *AbstractProcess* as its value. Thus any SensorML process can be a component of an aggregate process, whether that process is itself simple or aggregate, non-physical or physical.

The XML snippet for the *ComponentList* element and its corresponding complex types is shown below:

<element name="ComponentList" type="sml:ComponentListType" substitutionGroup="swe:AbstractSWE"/>

<complexType name="ComponentListType">

<complexContent>

<extension base="swe:AbstractSWEType">

<sequence>

<element name="component" minOccurs="1" maxOccurs="unbounded">

<annotation>

<documentation>A description of a component of the aggregate process. If by reference, the

uniqueID of the referenced process must be provided using the xlink:title attribute while

the URL to the process description must be provided by the xlink:href attribute.

</documentation>

</annotation>

<complexType>

<complexContent>

<extension base="sml:AbstractProcessPropertyType">

<attribute name="name" type="NCName" use="required"/>

</extension>

</complexContent>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="ComponentListPropertyType">

<sequence minOccurs="0">

<element ref="sml:ComponentList"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

The component process can be described inline or be referenced through the xlink:href property. For a reference to an external process description, two pieces of information are required in order to reference a component process instance, the uniqueID of the process and a resolvable URL referencing the process description. These shall be provided by the *xlink:title* and *xlink:href* attributes, respectively.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/aggregateProcess/componentReference> |
| 1. When the value of the *component* property is “byReference”, there shall be meaningful values for the *xlink:title* and *xlink:href* attributes. The uniqueID of the referenced process, given by its *gml:identifier* property, shall be the value of the *xlink:title* attribute, while a resolvable URL to the referenced process description shall be the value of the *xlink:href* attribute. |

The examples in Section 8.3.1 show that the components of an aggregate process can be fully described inline, or be externally referenced processes that are configurable.

### Connections

The *connections* property and the *ConnectionList* elements are XML Schema implementations of the UML classes defined in clause 7.4. The *connections* property takes a *ConnectionList* as its value. The *ConnectionList* *connection* property takes a *Link* as its value.

The XML snippet for the *ConnectionList* and *Link* elements and their corresponding complex types is shown below:

*ConnectionList:*

<element name="ConnectionList" type="sml:ConnectionListType" substitutionGroup="swe:AbstractSWE"/>

<complexType name="ConnectionListType">

<complexContent>

<extension base="swe:AbstractSWEType">

<sequence>

<element name="connection" minOccurs="1" maxOccurs="unbounded">

<complexType>

<sequence>

<element ref="sml:Link"/>

</sequence>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="ConnectionListPropertyType">

<sequence minOccurs="0">

<element ref="sml:ConnectionList"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

*Link:*

<element name="Link" type="sml:LinkType" substitutionGroup="gml:AbstractObject"/>

<complexType name="LinkType">

<sequence>

<element name="source" type="sml:DataComponentPathType">

<annotation>

<documentation>The output from which the link originates.</documentation>

</annotation>

</element>

<element name="destination" type="sml:DataComponentPathType">

<annotation>

<documentation>The input or parameter into which the data flows.</documentation>

</annotation>

</element>

</sequence>

<attribute ref="gml:id" use="optional"/>

</complexType>

<complexType name="LinkPropertyType">

<sequence minOccurs="0">

<element ref="sml:Link"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

<simpleType name="DataComponentPathType">

<restriction base="token">

<pattern value="([a-zA-Z\_][a-zA-Z0-9\_\-\.]\*)(/[a-zA-Z\_][a-zA-Z0-9\_\-\.]\*)\*"/>

</restriction>

</simpleType>

#### Rules for Connections

The *Link* element may define a data connection between any properties of a process, but it typically connects inputs, outputs, and parameters. However, certain rules apply regarding sources for data (provided by the *source* property of the *Link* element) and destinations for data (provided by the *destination* property of the *Link* element).

Typical data flow is from an aggregate processes input to one or more component’s input, from a component output to another component’s input, or from a component’s output to an output of the aggregate process.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/aggregateProcess/inputConnectionRestrictions> |
| 1. The input of an enclosing aggregate process can connect to the input of one or more of its components; otherwise an input cannot connect to another input. |

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/aggregateProcess/outputConnectionRestrictions> |
| 1. The output of a component can connect to an output of its enclosing aggregate process; otherwise an output cannot connect to another output. |

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/aggregateProcess/multipleConnections> |
| 1. An output can connect to multiple destinations, but an input can only have one source connection. |

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/aggregateProcess/parameterConnectionRestrictions> |
| 1. A parameter can only be connected as a destination; a parameter cannot serve as a source. |

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/aggregateProcess/propertyConnectionRestrictions> |
| 1. Process properties other than inputs, outputs, or parameters can only serve as sources of data not destinations. |

#### Rules for Path Designation

While the use of XPath was considered as a means of designating *Link* sources and destinations, this protocol was rejected on the grounds that its was too complicated for our needs and because it did not allow continues designation of paths for “byReference” objects. The designation of a path starts at the base element of the aggregate process and only uses property elements. Where the attribute name exists for an element, it is used; otherwise the element name is used.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/aggregateProcess/designatingLinkPaths> |
| 1. The following rules shall be used for designating the source and destination paths within the Linked element.    1. **The path begins at the base of the cuurent process**    2. **The path includes only property elements (lowerCamelCase) and not value objects (UpperCamelCase)**    3. **If the property has an attribute name and it has a value, then it shall be used; otherwise the unqualified name of the property element should be used**    4. **The path can follow properties that are byReference** |

As an example, a snippet of the previous example is given below, highlighting the source path parts in yellow and the destination path parts in cyan. The subsequent example shows the appropriate source link path (in yellow) and the destination link path (in cyan).

<?xml version="1.0" encoding="UTF-8"?>

<sml:AggregateProcess gml:id="scaleAndClip06"

… deleted for brevity sake …

<!-- ============================= -->

<!-- Aggregate Process Inputs -->

<!-- ============================= -->

<sml:inputs>

<sml:InputList>

<sml:input name="valueIn">

<swe:Quantity definition="http://sensors.ws/def/simpleDN">

<swe:uom code="any"/>

</swe:Quantity>

</sml:input>

</sml:InputList>

</sml:inputs>

… deleted for brevity sake …

<sml:components>

<sml:ComponentList >

<!-- Component 1 - Linear Interpolator -->

<sml:component name="scale">

<sml:SimpleProcess gml:id="linearInterpolator01"

definition="http://sensors.ws/process/linearInterpolator">

… deleted for brevity sake …

<sml:inputs>

<sml:InputList>

<sml:input name="x">

<swe:Quantity definition="http://sensors.ws/def/xCoordinate">

<swe:uom code="any"/>

</swe:Quantity>

</sml:input>

</sml:InputList>

</sml:inputs>

… deleted for brevity sake …

<!-- Connect AggregateProcess input to LinearInterpolator (scale) input -->

<sml:connection>

<sml:Link>

<sml:source>inputs/valueIn</sml:source>

<sml:destination>components/scale/inputs/x</sml:destination>

</sml:Link>

</sml:connection>

## Requirements Class: Physical Component Schema

|  |  |
| --- | --- |
| Requirements Class | |
| http://www.opengis.net/spec/SensorML/2.0/req/xml/physicalComponent | |
| Target Type | XML Instance |
| **Dependency** | http://www.opengis.net/spec/SensorML/2.0/req/model/physicalComponent |
| **Dependency** | <http://www.opengis.net/spec/SensorML/2.0/req/xml/simpleProcess> |

XML Schema elements and types defined in the “*physical\_component.xsd*” schema file implement all classes defined respectively in the “physicalComponent” UML package defined in Clause 7.6.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/physicalComponent/schema-valid> |
| 1. The XML instance shall be valid with respect to the XML grammar defined in the “physical\_component.xsd”, as well as satisfy all Schematron patterns defined in “physical\_component.sch”. |

The following XML snippet provides the appropriate header and import statements for the physical\_component.xsd:

<schema xmlns="http://www.w3.org/2001/XMLSchema" xmlns:sml="http://www.opengis.net/sensorML/2.0"

xmlns:gml="http://www.opengis.net/gml/3.2" xmlns:swe="http://www.opengis.net/swe/2.0"

targetNamespace="http://www.opengis.net/sensorML/2.0" elementFormDefault="qualified"

attributeFormDefault="unqualified">

<annotation>

<documentation>

The elements of a concrete simple physical process derived from the core process model.

</documentation>

</annotation>

<import namespace="http://www.opengis.net/swe/2.0"

schemaLocation="http://schemas.opengis.net/sweCommon/2.0/swe.xsd"/>

<import namespace="http://www.opengis.net/gml/3.2"

schemaLocation="http://schemas.opengis.net/gml/3.2.1/gml.xsd"/>

<include schemaLocation="simple\_process.xsd"/>

### Abstract Physical Process

*AbstractPhysicalProcess* is derived from *AbstractProcess* and serves as the base class for all physical processes modelled and encoded in this specification..

The “*AbstractPhysicalProcess*” element is the XML schema implementation of the “*AbstractPhysicalProcess*” UML class defined in clause 7.6. The schema snippet for this element and its corresponding complex type is shown below.

<element name="AbstractPhysicalProcess" type="sml:AbstractPhysicalProcessType" abstract="true"

substitutionGroup="sml:AbstractProcess">

<annotation>

<documentation>

A physical process where the spatial and temporal state of the process is relevant.

</documentation>

</annotation>

</element>

<complexType name="AbstractPhysicalProcessType" abstract="true">

<complexContent>

<extension base="sml:AbstractProcessType">

<sequence>

<element name="attachedTo" type="gml:ReferenceType" minOccurs="0" maxOccurs="1">

<annotation>

<appinfo>

<gml:targetElement>sml:AbstractPhysicalProcess</gml:targetElement>

</appinfo>

<documentation>

References the physical component or system (e.g. platform) to which to which this

component or system is attached.

</documentation>

</annotation>

</element>

<element name="localReferenceFrame" minOccurs="0" maxOccurs="1">

<annotation>

<documentation>

A spatial reference frame of the physical component itself; this reference frame is

absolute and defines the relationship of the reference frame to the physical body of the

component; position of the component relates this reference frame to some external

reference frame.

</documentation>

</annotation>

<complexType>

<sequence>

<element ref="sml:ReferenceFrame"/>

</sequence>

</complexType>

</element>

<element name="temporalReferenceFrame" minOccurs="0" maxOccurs="unbounded">

<annotation>

<documentation>

supports local time reference frames such as "milliseconds past mission start"

</documentation>

</annotation>

<complexType>

<sequence>

<element ref="gml:TimeReferenceSystem"/>

</sequence>

</complexType>

</element>

<element name="position" type="sml:PositionUnionPropertyType" minOccurs="0" maxOccurs="1">

<annotation>

<documentation>

Provides positional information relating the component's spatial reference frame to an

external spatial reference frame. Positional information can be given by location, by full

body state, by a time-tagged trajectory, or by a measuring or computational process.

</documentation>

</annotation>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="AbstractPhysicalProcessPropertyType">

<sequence minOccurs="0">

<element ref="sml:AbstractPhysicalProcess"/>

</sequence>

<attributeGroup ref="gml:AssociationAttributeGroup"/>

<attributeGroup ref="gml:OwnershipAttributeGroup"/>

</complexType>

*AbstractPhysicalProcess* element adds the following properties to the *AbstractProcess*: *attachedTo*, *localReferenceFrame*, *temporalReferenceFrame*, and *position*. These properties of *AbstractPhysicalProcess* will be discussed in more detail in the following subsections.

#### AttachedTo

The *attachedTo* property provides a reference to either a *PhysicalComponent* or *PhysicalSystem*. It provides a means for an attached component to reference back to the component or system to which it is attached. This is particularly useful when the movement of the parent affects the movement of the component.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/physicalComponent/attachedToTarget> |
| 1. The *attachedTo* property shall provide a reference to an object of type *PhysicalComponent* or *PhysicalSystem*. |

The same rules shall apply as those for component references stated earlier.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/physicalComponent/attachedToReference> |
| 1. The *attachedTo* property shall require meaningful values for the *xlink:title* and *xlink:href* attributes. The uniqueID of the referenced process, given by its *gml:identifier* property, shall be the value of the *xlink:title* attribute, while a resolvable URL to the reference process description shall be the value of the *xlink:href* attribute. |

#### Local Reference Frame

The *localReferenceFrame* property takes a *ReferenceFrame* as its value. The “*ReferenceFrame*” element is an XML schema implementation of the “*ReferenceFrame*” UML class defined in clause 7.6. The schema snippet for this element and its corresponding complex type is shown below.

<element name="ReferenceFrame" type="sml:ReferenceFrameType"

substitutionGroup="swe:AbstractSWEIdentifiable">

<annotation>

<documentation>

A general spatial Cartesian Reference Frame where the axes and origin will be defined textually relative

to a physical component.

</documentation>

</annotation>

</element>

<complexType name="ReferenceFrameType">

<complexContent>

<extension base="swe:AbstractSWEIdentifiableType">

<sequence>

<element name="origin" type="string">

<annotation>

<documentation>

A textual description of the origin of the reference frame relative to the physical device

(e.g. "the origin is at the point of attachment of the sensor to the platform").

</documentation>

</annotation>

</element>

<element name="axis" minOccurs="1" maxOccurs="unbounded">

<annotation>

<documentation>

Axis with name attribute and a textual description of the relationship of the axis to the

physical device; the order of the axes listed determines their relationship according to the

right-handed rule (e.g. axis 1 cross axis 2 = axis 3).

</documentation>

</annotation>

<complexType>

<simpleContent>

<extension base="string">

<attribute name="name" type="NCName" use="required"/>

</extension>

</simpleContent>

</complexType>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="ReferenceFramePropertyType">

<sequence minOccurs="0">

<element ref="sml:ReferenceFrame"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

The ReferenceFrame element provides a textual description of the physical process’ local coordinate reference frame. The position of this physical component or system is based on relating this local reference frame to some external reference frame (e.g. a platform or geographic reference frame).

An example of a local reference frame description is given below:

<sml:localReferenceFrame>

<sml:ReferenceFrame id="SENSOR\_FRAME">

<sml:origin>Origin is at the intersection of the symmetric axis of the cylinder and the rear of the sensor</sml:origin>

<sml:axis name="Z">Z is along the symmetric axis of the sensor in the direction of view</sml:axis>

<sml:axis name="X">X is perdendicular to the symmetric axis and intersects the indicator marked "x"

on the casing</sml:axis>

<sml:axis name="Y">Y = Z cross X</sml:axis>

</sml:ReferenceFrame>

</sml:localReferenceFrame>

#### Temporal Reference Frame

The *temporalReferenceFrame* property takes a *TemporalReferenceFrame* as its value and is an XML schema implementation of the “*TemporalReferenceFrame*” UML class defined in clause 7.6. The schema snippet for this element and its corresponding complex type is shown below.

<element name="temporalReferenceFrame" minOccurs="0" maxOccurs="unbounded">Look more at thi

<annotation>

<documentation>

supports local time reference frames such as "milliseconds past mission start"

</documentation>

</annotation>

<complexType>

<sequence>

<element ref="gml:TimeReferenceSystem"/>

</sequence>

</complexType>

</element>

#### Position

The *position* property of a physical component can be defined by one of several methods, including (1) by description, (2) by point, (3) by position, (4) by dynamic state, (5) by trajectory, or (6) by process. These are defined by the *PositionUnion* element shown below:

<group name="PositionUnion">

<annotation>

<documentation>

A choice of elements for defining spatial state (e.g. location, orientation, linear/angular velocity and

linear/angular acceleration.

</documentation>

</annotation>

<choice>

<element ref="swe:Text">

<annotation>

<documentation>

Provides positional information in textual form (e.g. "located on the intake line before the catalytic

converter"); shall only be used when a more precise location is unknown or irrelevant.

</documentation>

</annotation>

</element>

<element ref="gml:Point">

<annotation>

<documentation>

Provides static location only using a gml:Point element.

</documentation>

</annotation>

</element>

<element ref="swe:Vector">

<annotation>

<documentation>Provides a static location using a swe:Vector.</documentation>

</annotation>

</element>

<element ref="swe:DataRecord">

<annotation>

<documentation>

Provides location and orientation as a DataRecord consisting of one or two Vector elements.

</documentation>

</annotation>

</element>

<element ref="swe:DataArray">

<annotation>

<documentation>

Provides time-tagged dynamic state information that can include, for instance, location,

orientation, velocity, acceleration, angular velocity, angular acceleration; shall be a DataArray

consisting of a DataRecord element of multiple Vector fields.

</documentation>

</annotation>

</element>

<element ref="sml:AbstractProcess">

<annotation>

<documentation>

Provides for positional information to be provided by a process; example processes could include

a physical sensor such as a GPS, a computational process such as an orbital propagation model,

a specific web service such as a SOS, or any process who's output provides positional

information.

</documentation>

</annotation>

</element>

</choice>

</group>

<complexType name="PositionUnionPropertyType">

<sequence minOccurs="0">

<group ref="sml:PositionUnion"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

The location of a component is the location of origin of the components local reference frame relative to the origin of some defined external reference frame (e.g. the reference frame of a sensor’s platform or a geospatial reference frame). Likewise, the orientation of the component is the angular displacement of the x-y-z axes of the local reference frame relative to the corresponding axes of the external reference frame. For dynamic state, the velocity and acceleration are the first and second time derivatives of location, respectively, while angular velocity and angular acceleration are the first and second time derivatives of orientation.

Each option is defined in more detail below with appropriate examples.

##### Position by Description

There are physical components for which the precise location is either not known or is not really relevant. One example would be an O2 sensor on the exhaust line of a car as shown in the following example:

<sml:position>

<swe:Text>Located on the exhaust manifold before the catalytic converter</swe:Text>

</sml:position>

##### Position by Point

Position by point supports a static location using the *gml:Point* element. It is not appropriate if the orientation of the component is relevant or the component is has a dynamic location.

<sml:position>

<!-- EPSG 4326 is for latitude-longitude, in that order -->

<gml:Point gml:id="stationLocation" srsName="http://www.opengis.net/def/crs/EPSG/0/4326">

<gml:coordinates>47.8 88.56</gml:coordinates>

</gml:Point>

</sml:position>

##### Position by Location

As an alternative to using the *gml:Point*, a static location can also be provided using a *swe:Vector*, as in the example below:

<sml:position>

<swe:Vector definition="http://www.opengis.net/def/property/OGC/0/SensorLocation"

referenceFrame="http://www.opengis.net/def/crs/EPSG/6.7/4326">

<swe:coordinate name="Lat">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/Latitude" axisID="Lat">

<swe:uom code="deg"/>

<swe:value>47.8</swe:value>

</swe:Quantity>

</swe:coordinate>

<swe:coordinate name="Lon">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/Longitude" axisID="Long">

<swe:uom code="deg"/>

<swe:value>2.3</swe:value>

</swe:Quantity>

</swe:coordinate>

</swe:Vector>

</sml:position>

##### Position by Position

Position is defined here as consisting of both location and orientation. A static position shall be provided using a *swe:DataRecord* consisting of two *swe:Vector* elements, one for location and one for orientation.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/physicalComponent/position-by-position> |
| 1. The *position* property shall take a *swe:DataRecord* as its value when both location and orientation are relevant. This *swe:DataRecord* shall consist of two *swe:Vector* fields, the first for location and the second for orientation. |

An example of location and orientation defined for the position is shown below:

<sml:position>

<swe:DataRecord>

<swe:field name="location">

<swe:Vector definition="http://www.opengis.net/def/property/OGC/0/SensorLocation"

referenceFrame="http://www.opengis.net/def/crs/EPSG/6.7/4979" localFrame="#SENSOR\_FRAME">

<swe:coordinate name="Lat">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC//latitude" axisID="Lat">

<swe:uom code="deg"/>

<swe:value>47.8</swe:value>

</swe:Quantity>

</swe:coordinate>

<swe:coordinate name="Lon">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC//longitude" axisID="Long">

<swe:uom code="deg"/>

<swe:value>2.3</swe:value>

</swe:Quantity>

</swe:coordinate>

<swe:coordinate name="Alt">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC//altitude" axisID="Alt">

<swe:uom code="m"/>

<swe:value>40.8</swe:value>

</swe:Quantity>

</swe:coordinate>

</swe:Vector>

</swe:field>

<swe:field name="orientation">

<swe:Vector definition="http://www.opengis.net/def/property/OGC/0/SensorOrientation"

referenceFrame="http://www.opengis.net/def/crs/NED" localFrame="#SENSOR\_FRAME">

<swe:coordinate name="TrueHeading">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC//trueHeading" axisID="Z">

<swe:uom code="deg"/>

<swe:value>-6.8</swe:value>

</swe:Quantity>

</swe:coordinate>

<swe:coordinate name="Pitch">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC//pitch" axisID="Y">

<swe:uom code="deg"/>

<swe:value>0.3</swe:value>

</swe:Quantity>

</swe:coordinate>

</swe:Vector>

</swe:field>

</swe:DataRecord>

</sml:position>

##### Position by Trajectory

For components moving within an external reference frame, the state of the component through time shall be expressed using a *swe:DataArray* or process (described in the following section).

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/physicalComponent/dynamicState> |
| 1. The dynamic state through time of a moving physical component shall be described using a *swe:DataArray* or a *sml:AbstractProcess*. |

The data array shall describe the time-dependent state of the physical component as appropriate and may include location, orientation, linear and angular velocity, and linear and angular acceleration.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/physicalComponent/positionByTrajectory> |
| 1. A *swe:DataArray* describing the trajectory of a moving component shall contain as its *elementType* a *swe:DataRecord* that includes a time field plus one or more *swe:Vector* fields supporting any or all appropriate properties of dynamic state (e.g. location, orientation, linear velocity, linear acceleration, angular velocity, and angular acceleration). |

An example of dynamic position being defined as a trajectory is shown below. In this example the values for the location are provided inline within the *DataArray* element.

<sml:position>

<swe:DataArray definition="http://www.opengis.net/def/trajectory">

<swe:elementCount>

<swe:Count>

<swe:value>10</swe:value>

</swe:Count>

</swe:elementCount>

<swe:elementType name="trajectory">

<swe:DataRecord definition="http://www.opengis.net/def/trajectory">

<swe:field name="samplingTime">

<swe:Time definition="http://www.opengis.net/def/property/OGC/0/SamplingTime">

<swe:label>Sampling Time</swe:label>

<swe:uom xlink:href="http://www.opengis.net/def/uom/ISO-8601/0/Gregorian"/>

</swe:Time>

</swe:field>

<swe:field name="location">

<swe:Vector definition="http://www.opengis.net/def/location"

referenceFrame="http://www.opengis.net/def/crs/EPSG/6.7/4326" localFrame="#SENSOR\_CRS">

<swe:label>Platform Location</swe:label>

<swe:coordinate name="Lat">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/Latitude" axisID="Lat">

<swe:uom code="deg"/>

</swe:Quantity>

</swe:coordinate>

<swe:coordinate name="Lon">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/Longitude" axisID="Long">

<swe:uom code="deg"/>

</swe:Quantity>

</swe:coordinate>

</swe:Vector>

</swe:field>

</swe:DataRecord>

</swe:elementType>

<swe:encoding>

<swe:TextEncoding blockSeparator="&#10;" tokenSeparator=","/>

</swe:encoding>

<swe:values>

2011-03-01T04:20:00Z,25.72,-61.75

2011-03-14T13:10:00Z,25.49,-61.70

2011-03-21T18:43:00Z,25.35,-61.63

2011-03-30T05:13:00Z,24.87,-61.43

2011-04-08T01:45:00Z,24.86,-61.42

2011-04-12T08:34:00Z,24.32,-61.67

2011-04-15T09:12:00Z,24.54,-61.53

2011-04-21T03:21:00Z,24.53,-61.68

2011-04-27T04:34:00Z,24.32,-61.76

2011-05-01T12:01:00Z,24.28,-61.56

</swe:values>

</swe:DataArray>

</sml:position>

It is also possible to support “out-of-band” values by referencing an external “flat file” through the *xlink:href* attribute of the *values* property, such as:

<swe:values xlink:href="http://myDomain/data/aircraftLocation\_20048763">

Futhermore, the trajectory does not need to be constrained to provide only location. A trajectory *DataRecord* could include time, location, and orientation (e.g. pitch, roll, yaw), as well as perhaps velocity, and acceleration.

Finally, if part of the physical process (e.g. a sensor system) outputs its own position (e.g. using a GPS), that DataRecord can be referenced as in the following example:

<sml:outputs>

<sml:OutputList>

<!-- for the case of moving thermometer output in sync with GPS location -->

<sml:output name="tempStream">

<swe:DataRecord>

<swe:field name="sampleTime">

<swe:Time definition="http://www.opengis.net/def/property/OGC/0/SamplingTime"

referenceFrame="http://www.opengis.net/def/trs/OGC/0/GPS">

<swe:label>Sampling Time</swe:label>

<swe:uom xlink:href="http://www.opengis.net/def/uom/ISO-8601/0/Gregorian"/>

</swe:Time>

</swe:field>

<swe:field name="temperature">

<swe:Quantity definition="http://sweet.jpl.nasa.gov/2.2/quanTemperature.owl#Temperature">

<swe:label>Air Temperature</swe:label>

<swe:uom code="Cel"/>

</swe:Quantity>

</swe:field>

<swe:field name="location">

<swe:Vector id="MY\_LOCATION" definition="http://www.opengis.net/def/location"

referenceFrame="http://www.opengis.net/def/crs/EPSG/6.7/4326" localFrame="#SENSOR\_CRS">

<swe:coordinate name="Lat">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/Latitude" axisID="Lat">

<swe:uom code="deg"/>

</swe:Quantity>

</swe:coordinate>

<swe:coordinate name="Lon">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/Longitude" axisID="Long">

<swe:uom code="deg"/>

</swe:Quantity>

</swe:coordinate>

</swe:Vector>

</swe:field>

</swe:DataRecord>

</sml:output>

</sml:OutputList>

</sml:outputs>

<!-- ======================================= -->

<!-- Sensor Location from on-board GPS -->

<!-- ======================================= -->

<sml:position xlink:href="#MY\_LOCATION"/>

##### Position by Process

With dynamic sensor systems, it is often necessary or more efficient to calculate position or dynamic state as-needed, on-demand or to retrieve position values from a web service as-needed.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/physicalComponent/position-by-process> |
| 1. The position property shall take a SensorML-encoded process (either inline or by reference) when those values are calculated or retrieved on-demand as-needed. The output of that process shall be a *swe:DataArray* describing the trajectory of the component, or a *swe:DataRecord* describing instantaneous position or state of the component. |

The following example shows a configured SimpleProcess that calculates position on-demand using an orbital mechanics model. The process takes time as input and provides dynamic state as output. The example utilizes a configurable process to be discussed in a later section.

<sml:position>

<sml:SimpleProcess gml:id="OrbitalPropagationModel">

<sml:validTime>

<gml:TimePeriod gml:id="TimeSegment">

<gml:beginPosition>2010-03-01T00:20:00Z</gml:beginPosition>

<gml:endPosition>2010-03-02T04:01:00Z</gml:endPosition>

</gml:TimePeriod>

</sml:validTime>

<sml:typeOf xlink:title="urn:sensors:sgp4" xlink:href="http://myDomain.org/processes/sgp4Propagation.xml"/>

<sml:configuration>

<sml:Settings>

<sml:setValue ref="base/parameters/elements/epoch">2010-03-01T02:00:14.32994Z</sml:setValue>

<sml:setValue ref="base/parameters/elements/star">0.11897E-4</sml:setValue>

<sml:setValue ref="base/parameters/elements/inclination">98.7187</sml:setValue>

<sml:setValue ref="base/parameters/elements/rightAscension">128.3968</sml:setValue>

<sml:setValue ref="base/parameters/elements/eccentricity">0.00000571</sml:setValue>

<sml:setValue ref="base/parameters/elements/argOfPerigee">101.8476</sml:setValue>

<sml:setValue ref="base/parameters/elements/meanAnomaly">258.2808</sml:setValue>

<sml:setValue ref="base/parameters/elements/meanMotion">14.20027191</sml:setValue>

</sml:Settings>

</sml:configuration>

<sml:method xlink:href="http://myDomain.org/processMethods/sgp4\_method.xml"/>

</sml:SimpleProcess>

</sml:position>

The following example shows position obtained as-needed from an oline SOS web service. The SimpleProcess is a configured instance of an SOS client process. The process takes time as input and provides position as output.

<sml:position>

<!-- position by process -->

<sml:SimpleProcess gml:id="SOS\_Client">

<sml:typeOf xlink:title="urn:ogc:service:sos-orbitalPropagator"

xlink:href="http://blah.blah/def/processes/sos-orbit.xml"/>

<sml:configuration>

<sml:Settings>

<sml:setValue ref="base/parameters/URI">http://sensors.ws/services/mySOS</sml:setValue>

<sml:setValue ref="base/parameters/layer">position</sml:setValue>

<sml:setValue ref="base/parameters/procedure">mySat1</sml:setValue>

</sml:Settings>

</sml:configuration>

<sml:method xlink:href="http://blah.blah/processes/sos\_method.xml"/>

</sml:SimpleProcess>

</sml:position>

### Physical Component

*PhysicalComponent* is derived from *AbstractPhysicalProcess* and is the XML schema implementation of the “*PhysicalComponent*” UML class defined in clause 7.6. The schema snippet for this element and its corresponding complex type is shown below.

<element name="PhysicalComponent" type="sml:PhysicalComponentType"

substitutionGroup="sml:AbstractPhysicalProcess">

<annotation>

<documentation>

A PhysicalComponent is a physical process that will not be further divided into smaller components.

</documentation>

</annotation>

</element>

<complexType name="PhysicalComponentType">

<complexContent>

<extension base="sml:AbstractPhysicalProcessType">

<sequence>

<element name="method" type="sml:ProcessMethodPropertyType" minOccurs="0" maxOccurs="1">

<annotation>

<documentation>

The method describes (as an algorithm or text) how the process takes the input and,

based on the parameter values, generates output values.

</documentation>

</annotation>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="PhysicalComponentPropertyType">

<sequence minOccurs="0">

<element ref="sml:PhysicalComponent"/>

</sequence>

<attributeGroup ref="gml:AssociationAttributeGroup"/>

<attributeGroup ref="gml:OwnershipAttributeGroup"/>

</complexType>

The example below illustrates the definition of a local coordinate reference frame as well as the definition of position (i.e. both location and orientation) of the physical component. While the position of the component is specified here relative to a geospatial reference frame, it could also be specified relative to some other external reference frame, such as the reference frame of a platform.

<?xml version="1.0" encoding="UTF-8"?>

<sml:PhysicalComponent gml:id="MY\_SENSOR"

xmlns:sml="http://www.opengis.net/sensorML/2.0"

xmlns:swe="http://www.opengis.net/swe/2.0"

xmlns:gml="http://www.opengis.net/gml/3.2"

xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"

xmlns:xlink="http://www.w3.org/1999/xlink"

xsi:schemaLocation="http://www.opengis.net/sensorML/2.0 ../../sensorML.xsd">

<!-- ================================================= -->

<!-- System Description -->

<!-- ================================================= -->

<gml:description>

Stationary Location and Orientation - Single-beam Motion Detector

</gml:description>

<!-- ================================================= -->

<!-- Observed Property = Output -->

<!-- ================================================= -->

<sml:outputs>

<sml:OutputList>

<sml:output name="motionDetection">

<swe:Boolean definition="http://www.opengis.net/def/observable/motion"/>

</sml:output>

</sml:OutputList>

</sml:outputs>

<!-- ==================================== -->

<!-- Station Reference Frame -->

<!-- ==================================== -->

<!-- Particularly when dealing with orientations, one needs to understand the sensor's

reference frame as defined by the OEM or sensor deployer; the position and

orientation of this local frame is then described relative to an external reference

frame in the "position" property -->

<sml:localReferenceFrame>

<sml:ReferenceFrame id="SENSOR\_FRAME">

<sml:origin>

Origin is at the intersection of the symmetric axis of the cylinder and the rear of the sensor

</sml:origin>

<sml:axis name="Z">

Z is along the symmetric axis of the sensor in the direction of view

</sml:axis>

<sml:axis name="X">

X is perdendicular to the symmetric axis and intersects the indicator marked "x" on the casing

</sml:axis>

<sml:axis name="Y">Y = Z cross X</sml:axis>

</sml:ReferenceFrame>

</sml:localReferenceFrame>

<!-- ================================================= -->

<!-- Station Location and Orientation -->

<!-- ================================================= -->

<sml:position>

<swe:DataRecord>

<swe:field name="location">

<swe:Vector

definition="http://www.opengis.net/def/property/OGC/0/SensorLocation"

referenceFrame="http://www.opengis.net/def/crs/EPSG/6.7/4979"

localFrame="#SENSOR\_FRAME">

<swe:coordinate name="Lat">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC//latitude" axisID="Lat">

<swe:uom code="deg"/>

<swe:value>47.8</swe:value>

</swe:Quantity>

</swe:coordinate>

<swe:coordinate name="Lon">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC//longitude" axisID="Long">

<swe:uom code="deg"/>

<swe:value>2.3</swe:value>

</swe:Quantity>

</swe:coordinate>

<swe:coordinate name="Alt">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC//altitude" axisID="Alt">

<swe:uom code="m"/>

<swe:value>40.8</swe:value>

</swe:Quantity>

</swe:coordinate>

</swe:Vector>

</swe:field>

<swe:field name="orientation">

<swe:Vector

definition="http://www.opengis.net/def/property/OGC/0/SensorOrientation"

referenceFrame="http://www.opengis.net/def/crs/NED"

localFrame="#SENSOR\_FRAME">

<swe:coordinate name="TrueHeading">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC//trueHeading" axisID="Z">

<swe:uom code="deg"/>

<swe:value>-6.8</swe:value>

</swe:Quantity>

</swe:coordinate>

<swe:coordinate name="Pitch">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC//pitch" axisID="Y">

<swe:uom code="deg"/>

<swe:value>0.3</swe:value>

</swe:Quantity>

</swe:coordinate>

</swe:Vector>

</swe:field>

</swe:DataRecord>

</sml:position>

</sml:PhysicalComponent>

## Requirements Class: Physical System Schema

|  |  |
| --- | --- |
| Requirements Class | |
| http://www.opengis.net/spec/SensorML/2.0/req/xml/physicalSystem | |
| Target Type | XML Instance |
| **Dependency** | http://www.opengis.net/spec/SensorML/2.0/req/model/physicalSystem |
| **Dependency** | <http://www.opengis.net/spec/SensorML/2.0/req/xml/aggregateProcess> |
| **Dependency** | <http://www.opengis.net/spec/SensorML/2.0/req/xml/physicalComponent> |

XML Schema elements and types defined in the “*physical\_system.xsd*” schema file implement all classes defined respectively in the “physicalSystem” UML package defined in Clause 7.7.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/physicalSystem/schema-valid> |
| 1. The XML instance shall be valid with respect to the XML grammar defined in the “physical\_system.xsd”, as well as satisfy all Schematron patterns defined in “physical\_system.sch”. |

The following XML snippet provides the appropriate header and import statements for the physical\_component.xsd:

<schema xmlns="http://www.w3.org/2001/XMLSchema" xmlns:sml="http://www.opengis.net/sensorML/2.0"

xmlns:gml="http://www.opengis.net/gml/3.2" xmlns:swe="http://www.opengis.net/swe/2.0"

targetNamespace="http://www.opengis.net/sensorML/2.0" elementFormDefault="qualified"

attributeFormDefault="unqualified">

<annotation>

<documentation>

The elements of a concrete aggregate physical process derived from the core process model.

</documentation>

</annotation>

<import namespace="http://www.opengis.net/swe/2.0"

schemaLocation="http://schemas.opengis.net/sweCommon/2.0/swe.xsd"/>

<import namespace="http://www.opengis.net/gml/3.2"

schemaLocation="http://schemas.opengis.net/gml/3.2.1/gml.xsd"/>

<include schemaLocation="physical\_component.xsd"/>

<include schemaLocation="aggregate\_process.xsd"/>

### Physical System

The *PhysicalSystem* element and complex type are derived from the *AbstractPhysicalProcessType* and ths has all of the inherited properties defined in Clause 7.6. *PhysicalSystem* also has the components and connections properties that have already been described in Clause 7.4.

The schema snippet for this element and its corresponding complex type is shown below.

<element name="PhysicalSystem" type="sml:PhysicalSystemType"

substitutionGroup="sml:AbstractPhysicalProcess">

<annotation>

<documentation>

A PhysicalSystem is an aggregate system that can include multiple components (both physical and non-

physical) with explicit links between the outputs, inputs, and parameters of the individual components. In a

PhysicalSystem, the spatial position of the System itself is relevant to its application.

</documentation>

</annotation>

</element>

<complexType name="PhysicalSystemType">

<complexContent>

<extension base="sml:AbstractPhysicalProcessType">

<sequence>

<element name="components" type="sml:ComponentListPropertyType" minOccurs="0"

maxOccurs="1">

<annotation>

<documentation>

The collection of processes that make up a process aggregation.

</documentation>

</annotation>

</element>

<element name="connections" type="sml:ConnectionListPropertyType" minOccurs="0"

maxOccurs="1">

<annotation>

<documentation>

The explicit definition of data links between outputs, inputs, and parameters of the

components within an aggregate process.

</documentation>

</annotation>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="PhysicalSystemPropertyType">

<sequence minOccurs="0">

<element ref="sml:PhysicalSystem"/>

</sequence>

<attributeGroup ref="gml:AssociationAttributeGroup"/>

<attributeGroup ref="gml:OwnershipAttributeGroup"/>

</complexType>

A *PhysicalSystem* is a physical process that consists of multiple components that can be both physical and non-physical. As with the non-physical *AggregateProcess*, the *PhysicalSystem* allows for listing of the components as well as explicit mapping of the flow of data throughout the system.

In the example below there are three *components*: a thermometer that outputs temperature, an anemometer that outputs both wind speed and wind direction, and a non-physical windchill process that takes temperature and wind speed and calculates a windchill factor. The components are provided “by reference” using the *xlink:href* attribute. The outputs of these three components connect to the outputs of the system itself, as shown in the *ConnectionsList*.

<?xml version="1.0" encoding="UTF-8"?>

<sml:PhysicalSystem gml:id="MY\_WEATHER\_STATION"

xmlns:sml="http://www.opengis.net/sensorML/2.0"

xmlns:swe="http://www.opengis.net/swe/2.0"

xmlns:gml="http://www.opengis.net/gml/3.2"

xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"

xmlns:xlink="http://www.w3.org/1999/xlink"

xsi:schemaLocation="http://www.opengis.net/sensorML/2.0 ../../sensorML.xsd">

<!-- ================================================= -->

<!-- System Description -->

<!-- ================================================= -->

<gml:description> Weather station in my yard </gml:description>

<gml:identifier codeSpace="uid">urn:weather-we-is:stations:FR8766</gml:identifier>

<!-- ================================================= -->

<!-- Observed Property = Output -->

<!-- ================================================= -->

<sml:outputs>

<sml:OutputList>

<sml:output name="weather">

<swe:DataRecord>

<swe:field name="temperature">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/AtmosphericTemperature">

<swe:label>Air Temperature</swe:label>

<swe:uom code="cel"/>

</swe:Quantity>

</swe:field>

<swe:field name="wind\_chill">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/WindChillFactor">

<swe:label>Wind Chill Factor</swe:label>

<swe:uom code="cel"/>

</swe:Quantity>

</swe:field>

<swe:field name="wind\_speed">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/WindSpeed">

<swe:label>Wind Speed</swe:label>

<swe:uom code="km/h"/>

</swe:Quantity>

</swe:field>

<swe:field name="wind\_direction">

<swe:Quantity definition="http://www.opengis.net/def/property/OGC/0/WindDirection">

<swe:label>Wind Direction</swe:label>

<swe:uom code="deg"/>

</swe:Quantity>

</swe:field>

</swe:DataRecord>

</sml:output>

</sml:OutputList>

</sml:outputs>

<!-- ================================================= -->

<!-- System Location -->

<!-- ================================================= -->

<sml:position>

<gml:Point gml:id="stationLocation" srsName="http://www.opengis.net/def/crs/EPSG/0/4326">

<gml:coordinates>47.8 88.56</gml:coordinates>

</gml:Point>

</sml:position>

<!-- ================================================= -->

<!-- System Components -->

<!-- ================================================= -->

<sml:components>

<sml:ComponentList>

<sml:component name="thermometer" xlink:title="urn:davis:sensors:7817"

xlink:href="http://www.sensors.ws/examples/sensorML-2.0/xml/sensors/Davis\_7817\_complete.xml"/>

<sml:component name="anemometer" xlink:title="urn:davis:sensors:barometer\_internal"

xlink:href="http://www.sensors.ws/examples/sensorML-2.0/xml/sensors/Davis\_7911.xml"/>

<sml:component name="windchill" xlink:title="urn:ogc:process:windchill-02"

xlink:href="http://www.sensors.ws/examples/sensorML-2.0/xml/processes/windchill-02.xml"/>

</sml:ComponentList>

</sml:components>

<!-- =================================================== -->

<!-- Connections between components and system output -->

<!-- =================================================== -->

<sml:connections>

<sml:ConnectionList>

<!-- connection between thermometer's output and system's temperature output -->

<sml:connection>

<sml:Link>

<sml:source>components/thermometer/outputs/temperature</sml:source>

<sml:destination>outputs/weather/temperature</sml:destination>

</sml:Link>

</sml:connection>

<!-- connection between anemometer's wind speed output and system's windspeed output -->

<sml:connection>

<sml:Link>

<sml:source>components/anemometer/outputs/wind\_state/wind\_speed</sml:source>

<sml:destination>outputs/weather/wind\_speed</sml:destination>

</sml:Link>

</sml:connection>

<!-- connection between anemometer's wind direction output and system's wind direction output -->

<sml:connection>

<sml:Link>

<sml:source>components/anemometer/outputs/wind\_state/wind\_direction</sml:source>

<sml:destination>outputs/weather/wind\_direction</sml:destination>

</sml:Link>

</sml:connection>

<!-- connection between thermometer's output and windchill temperature input -->

<sml:connection>

<sml:Link>

<sml:source>components/thermometer/outputs/temperature</sml:source>

<sml:destination>components/windchill/inputs/process\_inputs/temperature</sml:destination>

</sml:Link>

</sml:connection>

<!-- connection between anemometer's wind speed output and windchill wind\_speed input -->

<sml:connection>

<sml:Link>

<sml:source>components/thermometer/outputs/wind\_state/wind\_speed</sml:source>

<sml:destination>components/windchill/inputs/process\_inputs/wind\_speed</sml:destination>

</sml:Link>

</sml:connection>

<!-- connection between windchill process output and system's windchill output -->

<sml:connection>

<sml:Link>

<sml:source>components/thermometer/outputs/windchill</sml:source>

<sml:destination>outputs/weather/windchill</sml:destination>

</sml:Link>

</sml:connection>

</sml:ConnectionList>

</sml:connections>

</sml:PhysicalSystem>

## Requirements Class: Configurable Process Schema

|  |  |
| --- | --- |
| Requirements Class | |
| http://www.opengis.net/spec/SensorML/2.0/req/xml/configuration | |
| Target Type | XML Instance |
| **Dependency** | http://www.opengis.net/spec/SensorML/2.0/req/model/configuration |
| **Dependency** | <http://www.opengis.net/spec/SensorML/2.0/req/xml/simpleProcess> |
| **Dependency** | [http://www.opengis.net/spec/SWE/2.0/req/xml\*\*\*\*\*\*](http://www.opengis.net/spec/SWE/2.0/req/xml******) |

XML Schema elements and types defined in the “*configurable\_process.xsd*” schema file implement all classes defined respectively in the “configurable\_process” UML package defined in Clause 7.7.

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/configuration/schema-valid> |
| 1. The XML instance shall be valid with respect to the XML grammar defined in the “configuration.xsd”, as well as satisfy all Schematron patterns defined in “configuration.sch”. |

The following XML snippet provides the appropriate header and import statements for the configurable\_process.xsd:

<schema xmlns="http://www.w3.org/2001/XMLSchema" xmlns:sml="http://www.opengis.net/sensorML/2.0"

xmlns:swe="http://www.opengis.net/swe/2.0" targetNamespace="http://www.opengis.net/sensorML/2.0"

elementFormDefault="qualified" attributeFormDefault="unqualified">

<annotation>

<documentation>

The elements supporting configurability and configuration settings of a instance of any process.

</documentation>

</annotation>

<import namespace="http://www.opengis.net/swe/2.0"

schemaLocation="http://schemas.opengis.net/sweCommon/2.0/swe.xsd"/>

<include schemaLocation="simple\_process.xsd"/>

The primary elements supporting configurable processes will be discussed in more detail in the following subclauses.

### Modes

The *Mode* element is an XML schema implementation of the models defined in Clause 7.9.1. It allows one to define a choice of modes, each of which in turn sets the values for a collection of parameters.

The XML snippet for the *Mode* and *ModeChoice* elements and their complex types is given below:

*Mode:*

<element name="Mode" type="sml:ModeType" substitutionGroup="sml:DescribedObject"/>

<complexType name="ModeType">

<complexContent>

<extension base="sml:DescribedObjectType">

<sequence>

<element name="configuration" type="sml:SettingsPropertyType"/>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="ModePropertyType">

<sequence minOccurs="0">

<element ref="sml:Mode"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

*ModeChoice*:

<element name="ModeChoice" type="sml:ModeChoiceType" substitutionGroup="sml:AbstractModes">

<annotation>

<documentation>

A collection of modes from which one can exclusively select during configuration of a process.

</documentation>

</annotation>

</element>

<complexType name="ModeChoiceType">

<complexContent>

<extension base="sml:AbstractModesType">

<sequence>

<element name="mode" type="sml:ModePropertyType" minOccurs="1" maxOccurs="unbounded"/>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="ModeChoicePropertyType">

<sequence minOccurs="0">

<element ref="sml:ModeChoice"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

A *Mode* is restricted in the values that it can set. In essence, a *Mode* is restricted to setting only the values of previously defined parameters of the enclosed process and its base processes, and the values of these parameters must be set consistent with the parameters allowed values.

|  |
| --- |
| Requirement |
| [http://www.opengis.net/spec/SensorML/2.0/req/xml/configuration/modeRestriction](http://www.opengis.net/spec/SensorML/2.0/req/xml/configuration/schema-valid) |
| 1. A *Mode* shall not set any process property values, other than the values of parameters defined within the same process or its parent processes. |

|  |
| --- |
| Requirement |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/configuration/parameterValues> |
| 1. The parameter values set by a *Mode* cannot be outside of the values allowed by the *AllowedValues* property of the *parameter*. |

In the following example, the definition of the parameters, samplingRate and gain are defined within the parameters section of the process description. Then two modes (“lowThreat” and “highThreat”) are defined, each of which defines specific values for these the two parameters.

<!-- ==================================== -->

<!-- Parameters -->

<!-- ==================================== -->

<sml:parameters>

<sml:ParameterList>

<sml:parameter name="samplingRate">

<swe:Quantity definition="http://sensors.ws/def/samplingRate" updatable="false">

<swe:label>Sampling Rate</swe:label>

<swe:uom code="Hz"/>

<swe:constraint>

<swe:AllowedValues>

<swe:interval>0.01 10.0</swe:interval>

</swe:AllowedValues>

</swe:constraint>

</swe:Quantity>

</sml:parameter>

<sml:parameter name="gain">

<swe:Quantity definition="http://sensors.ws/def/gain" updatable="false">

<swe:label>Gain</swe:label>

<swe:uom code="Hz"/>

<swe:constraint>

<swe:AllowedValues>

<swe:interval>1.0 2.5</swe:interval>

</swe:AllowedValues>

</swe:constraint>

</swe:Quantity>

</sml:parameter>

</sml:ParameterList>

</sml:parameters>

<!-- ==================================== -->

<!-- Modes -->

<!-- ==================================== -->

<sml:modes>

<sml:ModeChoice id="THREAT\_LEVEL\_MODE">

<sml:mode>

<sml:Mode gml:id="lowThreat">

<gml:description> Setting when nothing has been detected </gml:description>

<gml:name>Low Threat Mode</gml:name>

<sml:configuration>

<sml:Settings>

<sml:setValue ref="parameters/samplingRate">0.1</sml:setValue>

<sml:setValue ref="parameters/gain">1.0</sml:setValue>

</sml:Settings>

</sml:configuration>

</sml:Mode>

</sml:mode>

<sml:mode>

<sml:Mode gml:id="highThreat">

<gml:description> Setting when something has been detected </gml:description>

<gml:name>High Threat Mode</gml:name>

<sml:configuration>

<sml:Settings>

<sml:setValue ref="parameters/samplingRate">10.0</sml:setValue>

<sml:setValue ref="parameters/gain">2.5</sml:setValue>

</sml:Settings>

</sml:configuration>

</sml:Mode>

</sml:mode>

</sml:ModeChoice>

</sml:modes>

### Settings

The *Settings* element is an XML schema implementation of the models defined in Clause 7.9.2. It allows one to set values of parameters, to select modes, and to enable or disable components.

The XML snippet for the *Settings* element and its complex types is given below:

<element name="Settings" type="sml:SettingsType" substitutionGroup="sml:AbstractSettings"/>

<complexType name="SettingsType">

<complexContent>

<extension base="sml:AbstractSettingsType">

<sequence>

<element name="setValue" type="sml:ValueSettingPropertyType" minOccurs="0"

maxOccurs="unbounded">

<annotation>

<documentation>

Allows the setting of a particular property value.

</documentation>

</annotation>

</element>

<element name="setArrayValues" type="sml:ValueSettingPropertyType" minOccurs="0"

maxOccurs="unbounded">

<annotation>

<documentation>

Allows the setting of array values for a particular property.

</documentation>

</annotation>

</element>

<element name="setConstraint" type="sml:ConstraintSettingPropertyType" minOccurs="0"

maxOccurs="unbounded">

<annotation>

<documentation>

Allows one to further restrain the allowed values of a particular property.

</documentation>

</annotation>

</element>

<element name="setMode" type="sml:ModeSettingPropertyType" minOccurs="0"

maxOccurs="unbounded">

<annotation>

<documentation>

Allows one to select a predefined mode, which by inference sets a collection of property

values according to the definition of that mode.

</documentation>

</annotation>

</element>

<element name="setStatus" type="sml:StatusSettingPropertyType" minOccurs="0"

maxOccurs="unbounded">

<annotation>

<documentation>

Allows one to set the status (enabled, disabled, etc) of a particular input, output, or

parameter.

</documentation>

</annotation>

</element>

</sequence>

</extension>

</complexContent>

</complexType>

<complexType name="SettingsPropertyType">

<sequence minOccurs="0">

<element ref="sml:Settings"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

*setValue PropertyType*:

<complexType name="ValueSettingPropertyType">

<simpleContent>

<extension base="token">

<attribute name="ref" type="sml:DataComponentPathType" use="required"/>

</extension>

</simpleContent>

</complexType>

*setArrayValue PropertyType*:

<complexType name="ArraySettingPropertyType">

<sequence>

<element name="ArrayValues">

<complexType>

<sequence>

<element name="encoding">

<complexType>

<sequence>

<element ref="swe:AbstractEncoding"/>

</sequence>

</complexType>

</element>

<element name="value" type="swe:EncodedValuesPropertyType"/>

</sequence>

</complexType>

</element>

</sequence>

<attribute name="ref" type="sml:DataComponentPathType" use="required"/>

</complexType>

*setMode PropertyType*:

<complexType name="ModeSettingPropertyType">

<simpleContent>

<extension base="NCName">

<attribute name="ref" type="sml:DataComponentPathType" use="required"/>

</extension>

</simpleContent>

</complexType>

*setStatus PropertyType*:

<complexType name="StatusSettingPropertyType">

<simpleContent>

<extension base="sml:StatusType">

<attribute name="ref" type="sml:DataComponentPathType" use="required"/>

</extension>

</simpleContent>

</complexType>

*setConstraint PropertyType*:

<complexType name="ConstraintSettingPropertyType">

<sequence>

<group ref="sml:Constraint"/>

</sequence>

<attribute name="ref" type="sml:DataComponentPathType" use="required"/>

</complexType>

<group name="Constraint">

<choice>

<element ref="swe:AllowedTimes"/>

<element ref="swe:AllowedTokens"/>

<element ref="swe:AllowedValues"/>

</choice>

</group>

<complexType name="ConstraintPropertyType">

<sequence minOccurs="0">

<group ref="sml:Constraint"/>

</sequence>

<attributeGroup ref="swe:AssociationAttributeGroup"/>

</complexType>

<simpleType name="StatusType">

<restriction base="string">

<enumeration value="enabled"/>

<enumeration value="disabled"/>

</restriction>

</simpleType>

*setUnits PropertyType*:

\*\*\* add to models and schema \*\*\*

The following example shows use of the *configuration* property within a configured process. In this example, the value of the Averaging Period for the raingauge is set to 60.0 (in whatever units of measure are use by the parameter), the Sampling Period of the raingauge has been constrained between 30.0 and 60.0, and the rain gauge component has been enabled.

The path describing the properties and components shall be provided by the *ref* attribute and must follow the same rules set for connection *Links* in Section 8.3.3.2. \*\*\*\* add the “base” designation to the path or just assume that this (configured process) is the same process as the base process because of simple inheritance ????!!!!

<!-- ============================== -->

<!-- System Configuration -->

<!-- ============================== -->

<sml:typeOf xlink:title="urn:davis:stations:ProVantage2v4"

xlink:href="ManufacturerDescription.xml#DAVIS\_PRO\_VANTAGE2"/>

<sml:configuration>

<sml:Settings>

<sml:setValue ref="components/raingauge/parameters/Averaging\_Period">60.0</sml:setValue>

<sml:setConstraint ref="components/raingauge/parameters/Sampling\_Period">

<swe:AllowedValues>

<swe:interval>30.0 60.0</swe:interval>

</swe:AllowedValues>

</sml:setConstraint>

<sml:setStatus ref="components/raingauge">enabled</sml:setStatus>

</sml:Settings>

</sml:configuration>

1. (normative)  
     
   Abstract Conformance Test Suite
   1. Conformance Test Class: Core Concepts

|  |  |
| --- | --- |
| Conformance Test Class | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/core> | |
| Target Type | Derived Models and Software Implementations |

Tests described in this section shall be used to test conformance of software and encoding models implementing the Requirements Class: Core Concepts (normative core).

* + 1. Core concepts are the base of all derived models

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/core/core-concepts-used> | |
| Requirement Req 1 | A derived model or encoding shall correctly implement the modeling concepts defined in the core of this standard. |
| Test Method | Inspect the model or software implementation to verify the above. |
| Test Type | Capability |

* + 1. A process model has inputs, outputs, parameters, and method

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/core/processes> | |
| Requirement Req 2 | The core model for a process shall define inputs, outputs, parameters, and methodology of that process. |
| Test Method | Inspect the model or software implementation to verify the above. |
| Test Type | Capability |

* + 1. A process model has a unique ID

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/core/uniqueID> | |
| Requirement Req 3 | The core model for a process shall include a unique ID for distinguishing that process from any other. |
| Test Method | Inspect the model or software implementation to verify the above. |
| Test Type | Capability |

* + 1. A process model has metadata

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/core/metadata> | |
| Requirement Req 4 | The core model for a process shall include metadata that supports identification, discovery, and qualification of the process. |
| Test Method | Inspect the model or software implementation to verify the above. |
| Test Type | Capability |

* + 1. Metadata not used in process execution

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/core/execution> | |
| Requirement Req 5 | The metadata descriptions for a process shall not be required for successful execution of that process. All information required for execution of a simple process shall be contained within the inputs, outputs, parameters, and methodology descriptions of the process. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* 1. Conformance Test Class: Core Abstract Process

|  |  |
| --- | --- |
| Conformance Test Class | |
| <http://www.opengis.net/spec/sensorML/2.0/conf/model/coreProcess> | |
| Target Type | Derived Models and Software Implementations |
| **Dependency** | <http://www.opengis.net/spec/sensorML/2.0/conf/core> |

Tests described in this section shall be used to test conformance of software and encoding models implementing the conceptual models defined in Requirements Class: Core Abstract Process.

* + 1. Dependency on core

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/coreProcess/dependency-core> | |
| Requirement Req 6 | An encoding or software passing the “Core Abstract Process” model conformance class shall first pass the “Core Concepts” requirements test class. |
| Test Method | Apply all tests described in section A.1 |
| Test Type | Capability |

* + 1. DescribedObject derived from GML AbstractFeature

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/coreProcess/gmlDependency> | |
| Requirement Req 7 | *DescribedObject* shall derive from the GML base class, *AbstractFeature*, and is thus modeled as a feature with well-defined metadata properties. Any model or encoding derived from *DescribedObject* shall thus be of type *featureType*. |
| Test Method | Inspect the model or software implementation to verify the above. |
| Test Type | Capability |

* + 1. Using GML identifier for uniqueID in CoreProcess

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/coreProcess/uniqueID> | |
| Requirement Req 8 | A single, required *identifier* property inherited from GML *AbstractFeature* shall be used to provide a unique ID for the *DescribedObject*. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. Extensions must be in a separate namespace

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/coreProcess/extensionIndependence> | |
| Requirement Req 9 | Models inside of the extension property must exist within a namespace other than SensorML. |
| Test Method | Inspect the model or software implementation to verify the above. |
| Test Type | Capability |

* + 1. Extensions shall not be required for process execution

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/coreProcess/extensionRestrictions> | |
| Requirement Req 10 | Models inside of the extension property must not be required for execution of the process and shall not alter the execuition of the process. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. ObservableProperty and SWE Common Data used for process input, output, and parameters

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/coreProcess/SWE-Common-dependency> | |
| Requirement Req 11 | Any derived model or encoding for process shall utilize *ObservableProperty* or SWE Common Data Components as values for inputs, outputs, and parameters, and shall at a minimum conform to the SWE Common Data “Block Components Package” class (http://www.opengis.net/spec/SWE/2.0/req/uml-block-components). |
| Test Method | Inspect the model or software implementation to verify the above. |
| Test Type | Capability |

* + 1. Use of SWE Common Data aggregate models for process input, output, and parameters

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/coreProcess/aggregateData> | |
| Requirement Req 12 | Multiple input, output, and parameter values that are tightly related with one another shall be modelled as SWE Common Data aggregate data types, such as *DataRecord*, *Vector*, or *Matrix*. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. Application and requirements of *typeOf* property

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/coreProcess/typeOf> | |
| Requirement Req 13 | A process that is a specific instance of another process shall reference the more general process through its *typeOf* property. The value of the *typeOf* property shall be a resolvable link to an instance of a process derived from *AbstractProcess*. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. Simple inheritance extends a base class referenced by typeOf

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/coreProcess/simpleInheritance> | |
| Requirement Req 14 | A process instance that references another process through the *typeOf* property, but does not include the *configuration* property, shall inherit properties of the referenced process through simple inheritance. The complete description of that process is thus the simple addition of information from both process descriptions. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. Supporting configuration in processes

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/coreProcess/configuration> | |
| Requirement Req 15 | A process instance that references another process through the *typeOf* property, and further restricts options or allowed values provided in the referenced process, shall specify those restrictions through the *configuration* property. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* 1. Conformance Test Class: Simple Process

|  |  |
| --- | --- |
| Conformance Test Class | |
| <http://www.opengis.net/spec/sensorML/2.0/conf/model/simpleProcess> | |
| Target Type | Derived Models and Software Implementations |
| **Dependency** | <http://www.opengis.net/spec/sensorML/2.0/conf/model/coreProcess> |

Tests described in this section shall be used to test conformance of software and encoding models implementing the conceptual models defined in Requirements Class: Simple Process.

* + 1. Dependency on core

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/simpleProcess/dependency-core> | |
| Requirement Req 16 | An encoding or software passing the “Simple Process” model conformance class shall first pass the “Abstract Process” requirements test class. |
| Test Method | Apply all tests described in section A.2. |
| Test Type | Capability |

* + 1. Simple process definition

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/simpleProcess/definition> | |
| Requirement Req 17 | A process shall be considered a “simple process” if it provides a processing function with well-defined inputs and outputs, if there is no intent to further divide the process description into subprocess components, and if knowledge of its physical location is unknown or of no importance. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. Simple process has method

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/simpleProcess/method> | |
| Requirement Req 18 | Any derived model or encoding for simple process shall include a mandatory method property for identifying and describing the execution methodology. |
| Test Method | Inspect the model or software implementation to verify the above. |
| Test Type | Capability |

* 1. Conformance Test Class: Aggregate Process

|  |  |
| --- | --- |
| Conformance Test Class | |
| <http://www.opengis.net/spec/sensorML/2.0/conf/model/aggregateProcess> | |
| Target Type | Derived Models and Software Implementations |
| **Dependency** | <http://www.opengis.net/spec/sensorML/2.0/conf/model/coreProcess> |

Tests described in this section shall be used to test conformance of software and encoding models implementing the conceptual models defined in Requirements Class: Aggregate Process.

* + 1. Dependency on core

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/aggregateProcess/dependency-core> | |
| Requirement Req 19 | An encoding or software passing the “Aggregate Process” model conformance class shall first pass the “Abstract Process” requirements test class. |
| Test Method | Apply all tests described in section A.2. |
| Test Type | Capability |

* + 1. Definition of Aggregate Process

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/aggregateProcess/definition> | |
| Requirement Req 20 | A process shall be considered an “aggregate process” if it provides a processing function with well-defined inputs and outputs, if there is intent to further divide the process description into subprocessing components, and if knowledge of its physical location is unknown or of no importance. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. Aggregate Process requires one or more components

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/aggregateProcess/components> | |
| Requirement Req 21 | Any derived model or encoding for an aggregate process shall include one or more component processes and explicit linking of data flow between these components. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* 1. Conformance Test Class: Non-physical Processes

|  |  |
| --- | --- |
| Conformance Test Class | |
| http://www.opengis.net/spec/sensorML/2.0/conf/model/nonPhysicalProcesses | |
| Target Type | Derived Models and Software Implementations |
| **Dependency** | <http://www.opengis.net/spec/sensorML/2.0/conf/model/simpleProcess> |
| **Dependency** | <http://www.opengis.net/spec/sensorML/2.0/conf/model/aggregateProcess> |

Tests described in this section shall be used to test conformance of software and encoding models implementing the conceptual models defined in Requirements Class: Non-Physical Processes.

* + 1. Dependency on simple and aggregate processes

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/nonPhysicalProcess/supports> | |
| Requirement Req 22 | A derived model or encoding supporting non-physical processes shall meet the requirements for both simple process (clause 7.4) and aggregate process (clause 7.5). |
| Test Method | Apply all tests described in section A.3 and A.4. |
| Test Type | Capability |

* 1. Conformance Test Class: Physical Component

|  |  |
| --- | --- |
| Conformance Test Class | |
| <http://www.opengis.net/spec/sensorML/2.0/conf/model/physicalComponent> | |
| Target Type | Derived Models and Software Implementations |
| **Dependency** | <http://www.opengis.net/spec/sensorML/2.0/conf/model/coreProcess> |

Tests described in this section shall be used to test conformance of software and encoding models implementing the conceptual models defined in Requirement Class: Physical Component

* + 1. Dependency on core process

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/physicalComponent/dependency-core> | |
| Requirement Req 23 | An encoding or software passing the “Aggregate Process” model conformance class shall first pass the “Abstract Process” requirements test class. |
| Test Method | Apply all tests described in section A.2. |
| Test Type | Capability |

* + 1. Position by point

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/physicalComponent/byPointOrLocation> | |
| Requirement Req 24 | Specification of position byPoint or byLocation shall specify the location of the origin of the object’s reference frame relative to a well-defined and specified external reference frame. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. Position by location and orientation

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/physicalComponent/byPosition> | |
| Requirement Req 25 | Specification of position byPosition shall specify, using two Vectors, the location and orientation of the object’s reference frame relative to a well-defined and specified external reference frame.Specification of position byPosition shall specify, using two Vectors, the location and orientation of the object’s reference frame relative to a well-defined and specified external reference frame. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. Position by trajectory

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/physicalComponent/byTrajectory> | |
| Requirement Req 26 | Specification of position byTrajectory shall specify, at a minimum, the time-tagged location of the object’s reference frame relative to a well-defined and specified external reference frame, but may also include the orientation, linear and angular velocity, and any derivatives of the linear and angular velocity of the object’s reference frame. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. Position by process

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/physicalComponent/byProcess> | |
| Requirement Req 27 | Specification of position byProcess shall specify SensorML-modeled process whose output provides, at a minimum, the time-tagged location of the object’s reference frame relative to a well-defined and specified external reference frame, but may also include the orientation, linear and angular velocity, and any derivatives of the linear and angular velocity of the object’s reference frame. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. Physical Component definition

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/physicalComponent/byProcess> | |
| Requirement Req 28 | A process shall be considered a “physical component” if it provides a processing function with well-defined inputs and outputs, if there is no intent to further divide the device description into subprocess components, and if knowledge of its physical location is of importance. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* 1. Conformance Test Class: Physical System

|  |  |
| --- | --- |
| Conformance Test Class | |
| <http://www.opengis.net/spec/sensorML/2.0/conf/model/physicalSystem> | |
| Target Type | Derived Models and Software Implementations |
| **Dependency** | <http://www.opengis.net/spec/sensorML/2.0/conf/model/PhysicalComponent> |

Tests described in this section shall be used to test conformance of software and encoding models implementing the conceptual models defined in

* + 1. Physical System definition

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/physicalSystem/definition> | |
| Requirement Req 29 | A process shall be considered a “physical system” if it provides a processing function with well-defined inputs and outputs, if there is intent to further divide the device description into subprocess components, and if knowledge of its physical location is of importance. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. Physical System dependency

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/physicalSystem/dependency-core> | |
| Requirement Req 30 | An encoding or software passing the “Physical System” model conformance class shall first pass the “Abstract Physical Process” requirements test class in Clause 7.6. |
| Test Method | Inspect the model or software implementation to verify the above. |
| Test Type | Capability |

* 1. Conformance Test Class: Physical Processes

|  |  |
| --- | --- |
| Conformance Test Class | |
| <http://www.opengis.net/spec/sensorML/2.0/conf/model/physicalProcess> | |
| Target Type | Derived Models and Software Implementations |
| **Dependency** | <http://www.opengis.net/spec/sensorML/2.0/conf/model/SimpleProcess> |
| **Dependency** | <http://www.opengis.net/spec/sensorML/2.0/conf/model/AggregateProcess> |
| **Dependency** | <http://www.opengis.net/spec/sensorML/2.0/conf/model/PhysicalComponent> |
| **Dependency** | <http://www.opengis.net/spec/sensorML/2.0/conf/model/PhysicalSystem> |

Tests described in this section shall be used to test conformance of software and encoding models implementing the conceptual models defined in Requirements Class: Physical Processes

* + 1. Physical Process dependency

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/physicalProcess/dependency-core> | |
| Requirement Req 31 | A derived model or encoding supporting physical processes shall meet the requirements for non-physical processes (clause 7.9) as well as both the physical component process (clause 7.10) and physical system (clause 7.11). |
| Test Method | Inspect the model or software implementation to verify the above. |
| Test Type | Capability |

* 1. Conformance Test Class: Configurable Processes

|  |  |
| --- | --- |
| Conformance Test Class | |
| <http://www.opengis.net/spec/sensorML/2.0/conf/model/configurableProcess> | |
| Target Type | Derived Models and Software Implementations |
| **Dependency** | <http://www.opengis.net/spec/sensorML/2.0/conf/model/AbstractProcess> |

Tests described in this section shall be used to test conformance of software and encoding models implementing the conceptual models defined in Requirements Class: Configurable Processes.

* + 1. Definition of Configurable Process

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/configurableProcess/definitionOfConsfigurable> | |
| Requirement Req 32 | A process shall be considered “configurable” if it provides options, variable parameters, or modes that can be selected or set before or during deployment or execution. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. Definition of Configured Process

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/configurableProcess/definitionOfConsfigured> | |
| Requirement Req 33 | A process shall be considered “configured” if it sets options, parameter values, or modes that were defined within the configurable process. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. *ModeChoice* requires 2 or more *Modes*

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/configurableProcess/twoModesRequired> | |
| Requirement Req 34 | A *ModeChoice* instantiation must include two or more *mode* properties. |
| Test Method | Inspect the model or software implementation to verify the above. |
| Test Type | Capability |

* + 1. A configured process requires a Settings element

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/configurableProcess/settingsProperty> | |
| Requirement Req 35 | A configured process must include a *configuration* property that takes a *Settings* class as its value. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. Only *parameter* values can be set by *setValue*

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/configurableProcess/setValueRestriction> | |
| Requirement Req 36 | The setValue property shall only reference and set values for a parameter defined in a configurable process. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. Only *parameter* array values can be set by *setArrayValues*

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/configurableProcess/setArrayValueRestriction> | |
| Requirement Req 37 | The setArrayValues property shall only reference and set array values for a parameter defined in a configurable process. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* + 1. Only *parameter* values can be constrained with *setConstraint*

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/model/configurableProcess/setConstraintRestriction> | |
| Requirement Req 38 | The setConstraint property shall only reference and set constraints for a parameter defined in a configurable process. |
| Test Method | Verify that the implementation of the conceptual model has a constraint that enforces the above. |
| Test Type | Capability |

* 1. Conformance Test Class: Core Abstract Process Schema

|  |  |
| --- | --- |
| Conformance Test Class | |
| [http://www.opengis.net/spec/SensorML/2.0/conf/xml/coreProcess](http://www.opengis.net/spec/SWE/2.0/conf/xsd-simple-components) | |
| Target Type | XML Instance |
| Dependency | <http://www.opengis.net/spec/SensorML/2.0/req/model/coreProcess> |

All tests in this conformance test class and in the following shall be used to check conformance of XML instances created according to the schemas defined in this standard. They shall also be used to check conformance of software implementations that output XML instances.

* + 1. Compliance with core XML schemas and Schematron patterns

|  |  |
| --- | --- |
| **Conformance Test** | |
| [http://www.opengis.net/spec/SensorML/2.0/conf/xml/coreProcess /schema-valid](http://www.opengis.net/spec/SensorML/2.0/conf/xml/coreProcess%20/schema-valid) | |
| Requirement Req 39 | The XML instance shall be valid with respect to the XML grammar defined in the “core.xsd”, as well as satisfy all Schematron patterns defined in “core.sch”. |
| Test Method | Validate the XML instance containing core process with the “core.xsd” XML schema file and the Schematron patterns in “core.sch”. |
| Test Type | Capability |

* + 1. XML property values are included inline or by reference

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/coreProcess/ref-or-inline-value-present> | |
| Requirement Req 40 | A property element supporting the “swe:AssociationAttributeGroup” shall either contain the value inline or populate the “xlink:href” attribute with a valid reference but shall not be empty. |
| Test Method | Check that all properties either include an inline value or an “xlink:href” attribute. |
| Test Type | Capability |

* + 1. Each extension uses a different namespace

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/coreProcess/extension-namespace-unique> | |
| Requirement Req 41 | All extensions of the XML schemas described in this standard shall be defined in a new unique namespace (other than the namespaces used by this standard and its dependencies). |
| Test Method | If the standardization target is an extension of the XML schema defined in this standard, inspect the XML schema of the extension to verify the above. |
| Test Type | Capability |

* + 1. Extensions do not redefine XML elements or types

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/coreProcess/extension-coherent-with-core> | |
| Requirement Req 42 | Extensions of this standard shall not redefine or change the meaning or behavior of XML elements and types defined in this standard. |
| Test Method | Verify that all XML elements of the XML instance containing extensions can still be interpreted correctly without reading the extended information.  *Note:* *This test cannot be run automatically as the meaning the extension must be known and thus is not required to be implemented in the Executable Test Suite.* |
| Test Type | Capability |

* + 1. The value of the definition attribute is a resolvable URI

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/coreProcess/extension-process-execution> | |
| Requirement Req 43 | Extensions of this standard shall not exclusively contain information required for the successful execution of the process. |
| Test Method | Verify that the process execution does not require information to be retrieved from the extension element. |
| Test Type | Capability |

* + 1. Dependence on GML 3.2

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/gml-dependency> | |
| Requirement Req 44 | This standard shall utilize and depend upon the OGC GML 3.2 standard schema within the http://www.opengis.net/gml/3.2 namespace and defined in http://schemas.opengis.net/gml/3.2.1/ |
| Test Method | Validate the XML Instance according to GML 3.2 conformance tests |
| Test Type | Capability |

* + 1. Dependence on SWE Common Data 2.0

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/swe-common-dependency> | |
| Requirement Req 45 | This standard shall utilize and depend upon the OGC SWE Common Data 2.0 standard within the http://www.opengis.net/swe/2.0 namespace and defined in http://schemas.opengis.net/sweCommon/2.0/*swe.xsd and any corregendum (i.e. any versions 2.0.\*).* |
| Test Method | Validate the XML Instance according to SWE Common Data v2.0 conformance tests |
| Test Type | Capability |

* + 1. Globally unique ID required

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/globallyUniqueID> | |
| Requirement Req 46 | An instance supporting *DescribedObject* shall have one and only one *gml:identifier* and this element shall have a *codespace* attribute with a value set to “uniqueID”. The value of the *gml:identifier* shall be a globally unique identifier for the *DescribedObject*. |
| Test Method | Validate the XML Instance contains a unique ID for *gml:identifier* based on a well-defined protocol. |
| Test Type | Capability |

* + 1. External namespace required for security constraints

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/documentSecurityTags> | |
| Requirement Req 47 | All values for the securityConstraints property shall be defined in a new unique namespace (other than the namespaces used by this standard and its dependencies). |
| Test Method | Validate the XML Instance does not use namespaces used in this specification for the value of the securityConstraint property. |
| Test Type | Capability |

* + 1. *Extension* element used for security tagging of individual properties

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/individualSecurityTags> | |
| Requirement Req 48 | Security tagging of individual property values shall utilize the *extension* element within the appropriate SensorML or SWE Common data elements. |
| Test Method | Validate that security tagging of individual properties uses the *extension* element. |
| Test Type | Capability |

* + 1. Xlink role or arcrole shall be used to define relationship of contacts

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/contactRole> | |
| Requirement Req 49 | The role of the responsible party relative to the described object shall be provided using the *xlink:arcrole* attribute of the relevant *member* property of the *ContactList*. |
| Test Method | Validate within the XML Instance that either *xlink:arcrole* or *xlink:role* are present in the *member* element of *ContactList*. |
| Test Type | Capability |

* + 1. The *typeOf* property shall provide the uniqueID and resolvable location of the description on the referenced object

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/typeOfReference> | |
| Requirement Req 50 | The *typeOf* property shall require meaningful values for the *xlink:title* and *xlink:href* attributes. The uniqueID of the referenced process, given by its *gml:identifier* property, shall be the value of the *xlink:title* attribute, while a resolvable URL to the reference process description shall be the value of the *xlink:href* attribute. |
| Test Method | Validate that an *xlink:title* and *xlink:href* are present in any *typeOf* element of an XML Instance. |
| Test Type | Capability |

* + 1. The feature of interest property shall specify a role, and if available, the uniqueID of the feature

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/foiArcroleAndTitle> | |
| Requirement Req 51 | Regardless of whether a feature of interest is described inline or provided by reference, the *xlink:arcrole* attribute of the *member* property of the *FeatureList* shall be used to specify the relationship of the associated feature to the process. If a unique identifier or name for the feature of interest exists, it shall be the value of the *xlink:title* of the *member* property of the *FeatureList*. |
| Test Method | Validate that the *member* property of a *FeatureList* has a *xlink:arcrole* attribute present. |
| Test Type | Capability |

* + 1. The *definition* attribute required for *ObservableProperty*

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/observableDefinition> | |
| Requirement Req 52 | The *ObservableProperty* element shall include the *definition* attribute that shall take as its value, a resolvable URL referencing the definition of the observable within an online dictionary or ontology. |
| Test Method | Validate the presence and resolvability of the *definition* attribute for any *ObservableProperty* element. |
| Test Type | Capability |

* + 1. Use aggregate data for related data elements

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/DataRecord> | |
| Requirement Req 53 | Input, output, and parameter data components that are dependent on one another or represent the state at a given time, shall be surrounded by an appropriate aggregate data component, such as *swe:DataRecord*, *swe:Vector*, or *swe:Matrix*. |
| Test Method | Validate by inspection that dependent data components and those representing the state at a given time are encpsulted within an appropriate aggregate data component. |
| Test Type | Capability |

* + 1. Use Vector for *inputs*, *outputs*, and *parameters* that specify position

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/VectorUse> | |
| Requirement Req 54 | A *swe:Vector* shall be used for any input, output, or parameter value that requires position to be specified relative to a specific axis of a reference frame. |
| Test Method | Validate that positions within *inputs*, *outputs*, and *parameters* utilize the *swe:Vector* element. |
| Test Type | Capability |

* + 1. Use of resolvable URL to reference data streams

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/DataStreamURL> | |
| Requirement Req 55 | When the values of a *DataStream* can be referenced by a resolvable URL, that URL shall be the value of of the *xlink:href* attribute in the *value* property of the *DataStream*. |
| Test Method | Validate the presence of an *xlink:href* atribute with resolvable URL for *DataStream* *values* provided by reference. |
| Test Type | Capability |

* + 1. Use *DataChoice* in multiplexed data streams

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/req/xml/coreProcess/MultiplexedDataStream> | |
| Requirement Req 56 | When the values of a *DataStream* consist of a series of multiplexed packets, the value of the *elementType* property shall be specified using the SWE Common Data *DataChoice* element. |
| Test Method | Validate that a *DataStream* consisting of disparate packages utilizes *DataChoice* to encapsulate those packages and that each package is defined as an *item*. |
| Test Type | Capability |

* 1. Conformance Test Class: Simple Process Schema

|  |  |
| --- | --- |
| Conformance Test Class | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/simpleProcess> | |
| Target Type | XML Instance |
| Dependency | <http://www.opengis.net/spec/SensorML/2.0/req/model/simpleProcess> |

All tests in this conformance test class and in the following shall be used to check conformance of XML instances created according to the schemas defined in this standard. They shall also be used to check conformance of software implementations that output XML instances.

* + 1. Compliance with simple\_process XML schemas and Schematron patterns

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/simpleProcess/schema-valid> | |
| Requirement Req 57 | The XML instance shall be valid with respect to the XML grammar defined in the “simple\_process.xsd”, as well as satisfy all Schematron patterns defined in “simple\_process.sch”. |
| Test Method | Validate the XML instance containing core process with the “simple\_process.xsd” XML schema file and the Schematron patterns in “simple\_process.sch”. |
| Test Type | Capability |

* 1. Conformance Test Class: Aggregate Process Schema

|  |  |
| --- | --- |
| Conformance Test Class | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/aggregateProcess> | |
| Target Type | XML Instance |
| Dependency | <http://www.opengis.net/spec/SensorML/2.0/req/model/aggregateProcess> |

All tests in this conformance test class and in the following shall be used to check conformance of XML instances created according to the schemas defined in this standard. They shall also be used to check conformance of software implementations that output XML instances.

* + 1. Compliance with simple\_process XML schemas and Schematron patterns

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/aggregateProcess/schema-valid> | |
| Requirement Req 58 | The XML instance shall be valid with respect to the XML grammar defined in the “aggregate\_process.xsd”, as well as satisfy all Schematron patterns defined in “aggregate\_process.sch”. |
| Test Method | Validate the XML instance containing core process with the “aggregate\_process.xsd” XML schema file and the Schematron patterns in “aggregate\_process.sch”. |
| Test Type | Capability |

* + 1. Title and resolvable URL required for components provided by Reference

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/aggregateProcess/componentReference> | |
| Requirement Req 59 | The *component* property shall require meaningful values for the *xlink:title* and *xlink:href* attributes. The uniqueID of the referenced process, given by its *gml:identifier* property, shall be the value of the *xlink:title* attribute, while a resolvable URL to the reference process description shall be the value of the *xlink:href* attribute. |
| Test Method | Validate the presence of *xlink:title* and *xlink:href* for the *component* property when its value is provided by reference. |
| Test Type | Capability |

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/aggregateProcess/inputConnectionRestrictions> | |
| Requirement Req 60 | The input of an enclosing aggregate process can connect to the input of one or more of its components; otherwise an input cannot connect to another input. |
| Test Method | Validate that there are no input-to-input connections, other than from the aggregate process to one or more of its components. |
| Test Type | Capability |

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/aggregateProcess/outputConnectionRestrictions> | |
| Requirement Req 61 | The output of a component can connect to an output of its enclosing aggregate process; otherwise an output cannot connect to another output. |
| Test Method | Validate that there are no output-to-output connections, other than from a component process to the output of the aggregate process to. |
| Test Type | Capability |

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/aggregateProcess/multipleConnections> | |
| Requirement Req 62 | An output can connect to multiple destinations, but an input can only have one source connection. |
| Test Method | Validate that there are no multiple connection within any given input port. |
| Test Type | Capability |

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/aggregateProcess/parameterConnectionRestrictions> | |
| Requirement Req 63 | A parameter can only be connected as a destination; a parameter cannot serve as a source. |
| Test Method | Validate that there are no parameter ports in any destination path. |
| Test Type | Capability |

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/aggregateProcess/propertyConnectionRestrictions> | |
| Requirement Req 64 | Process properties other than inputs, outputs, or parameters can only serve as sources of data not destinations. |
| Test Method | Validate that no properties other than inputs, outputs, and parameters are included as a destination. |
| Test Type | Capability |

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/aggregateProcess/inputConnectionRestrictions> | |
| Requirement Req 65 | The following rules shall be used for designating the source and destination paths within the Linked element.  (a) The path begins at the base of the current process  (b) The path includes only property elements (lowerCamelCase) and not value objects (UpperCamelCase)  (c) If the property has an attribute name and it has a value, then it shall be used; otherwise the unqualified name of the property element should be used  (d) The path can follow properties that are byReference |
| Test Method | Validate that all paths lead to valid ports. |
| Test Type | Capability |

* 1. Conformance Test Class: Physical Component Schema

|  |  |
| --- | --- |
| Conformance Test Class | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/physicalComponent> | |
| Target Type | XML Instance |
| Dependency | <http://www.opengis.net/spec/SensorML/2.0/req/model/physicalComponent> |

All tests in this conformance test class and in the following shall be used to check conformance of XML instances created according to the schemas defined in this standard. They shall also be used to check conformance of software implementations that output XML instances.

* + 1. Compliance with physical\_component XML schemas and Schematron patterns

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/physicalSystem/schema-valid> | |
| Requirement Req 66 | The XML instance shall be valid with respect to the XML grammar defined in the “physical\_component.xsd”, as well as satisfy all Schematron patterns defined in “physical\_component.sch”. |
| Test Method | Validate the XML instance containing core process with the “physical\_component.xsd” XML schema file and the Schematron patterns in “physical\_component.sch”. |
| Test Type | Capability |

* + 1. A physical process can only attach to a physical process

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/physicalComponent/attachedToTarget> | |
| Requirement Req 67 | The *attachedTo* property shall provide a reference to an object of type *PhysicalComponent* or *PhysicalSystem*. |
| Test Method | Validate that the target for the *attachedTo* property is a *PhysicalComponent* or *PhysicalSystem*. |
| Test Type | Capability |

* + 1. The *attachedTo* element must have *xlink:title* and *xlink:href*

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/physicalComponent/attachedToReference> | |
| Requirement Req 68 | The *attachedTo* property shall require meaningful values for the *xlink:title* and *xlink:href* attributes. The uniqueID of the referenced process, given by its *gml:identifier* property, shall be the value of the *xlink:title* attribute, while a resolvable URL to the reference process description shall be the value of the *xlink:href* attribute. |
| Test Method | Validate that the the *attachedTo* property has values for the *xlink:href* and *xlink:title* attributes. |
| Test Type | Capability |

* + 1. Position requires a DataRecord with two Vectors

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/physicalComponent/position-by-position> | |
| Requirement Req 69 | The *position* property shall take a *swe:DataRecord* as its value when both location and orientation are relevant. This *swe:DataRecord* shall consist of two *swe:Vector* fields, the first for location and the second for orientation. |
| Test Method | When the *position* element takes a *swe:DataRecord* as its value, validate that the *DataRecord* contains two *swe:Vector* elements as its fields. |
| Test Type | Capability |

* + 1. Dynamic state requires a Data Array or Process

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/physicalComponent/dynamicState> | |
| Requirement Req 70 | The dynamic state through time of a moving physical component shall be described using a *swe:DataArray* or a *sml:AbstractProcess*. |
| Test Method | Validate through inspection that time-tagged locations, positions, or state values are provided by either *swe:DataArray* or a class derived from *sml:AbstractProcess*. |
| Test Type | Capability |

* + 1. Trajectory requires a DataArray with a time field and one or more Vectors

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/physicalComponent/positionByTrajectory> | |
| Requirement Req 71 | A *swe:DataArray* describing the trajectory of a moving component shall contain as its *elementType* a *swe:DataRecord* that includes a time field plus one or more *swe:Vector* fields supporting any or all appropriate properties of dynamic state (e.g. location, orientation, linear velocity, linear acceleration, angular velocity, and angular acceleration). |
| Test Method | When the *position* element takes a *swe:DataArray* as its value, validate that the *DataArray* contains a time field and one or more *swe:Vector* elements as its fields. |
| Test Type | Capability |

* + 1. Process required for positions or state provided on-demand

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/physicalComponent/position-by-process> | |
| Requirement Req 72 | The position property shall take a SensorML-encoded process (either inline or by reference) when those values are calculated or retrieved on-demand as-needed. The output of that process shall be a *swe:DataArray* describing the trajectory of the component, or a *swe:DataRecord* describing instantaneous position or state of the component. |
| Test Method | When the *position* element takes an instance of *sml:AbstractProcess* as its value, validate that the output of the process contains a *swe:DataArray* with time-tagged trajectory data, or a *swe:DataRecord* with time-tagged position or state data. |
| Test Type | Capability |

* 1. Conformance Test Class: Physical System Schema

|  |  |
| --- | --- |
| Conformance Test Class | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/physicalSystem> | |
| Target Type | XML Instance |
| Dependency | <http://www.opengis.net/spec/SensorML/2.0/req/model/physicalSystem> |

All tests in this conformance test class and in the following shall be used to check conformance of XML instances created according to the schemas defined in this standard. They shall also be used to check conformance of software implementations that output XML instances.

* + 1. Compliance with physical\_system XML schemas and Schematron patterns

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/physicalSystem/schema-valid> | |
| Requirement Req 73 | The XML instance shall be valid with respect to the XML grammar defined in the “physical\_system.xsd”, as well as satisfy all Schematron patterns defined in “physical\_system.sch”. |
| Test Method | Validate the XML instance containing core process with the “physical\_system.xsd” XML schema file and the Schematron patterns in “physical\_system.sch”. |
| Test Type | Capability |

* 1. Conformance Test Class: Configurable Process Schema

|  |  |
| --- | --- |
| Conformance Test Class | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/configuration> | |
| Target Type | XML Instance |
| Dependency | <http://www.opengis.net/spec/SensorML/2.0/req/model/configuration> |

All tests in this conformance test class and in the following shall be used to check conformance of XML instances created according to the schemas defined in this standard. They shall also be used to check conformance of software implementations that output XML instances.

* + 1. Compliance with configuration XML schemas and Schematron patterns

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/configuration/schema-valid> | |
| Requirement Req 74 | The XML instance shall be valid with respect to the XML grammar defined in the “configuration.xsd”, as well as satisfy all Schematron patterns defined in “configuration.sch”. |
| Test Method | Validate the XML instance containing core process with the “configuration.xsd” XML schema file and the Schematron patterns in “configuration.sch”. |
| Test Type | Capability |

* + 1. Modes can change values of parameters

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/configuration/modeRestriction> | |
| Requirement Req 75 | A *Mode* shall not set any process property values, other than the values of parameters defined within the same process or its parent processes. |
| Test Method | Validate that *setValue* references only *parameter* properties and only *parameter* properties within the current process or a parent process. |
| Test Type | Capability |

* + 1. Modes can only set values of parameters to those allowed by its constraints

|  |  |
| --- | --- |
| **Conformance Test** | |
| <http://www.opengis.net/spec/SensorML/2.0/conf/xml/configuration/parameterValues> | |
| Requirement Req 76 | The parameter values set by a *Mode* cannot be outside of the values allowed by the *AllowedValues* property of the *parameter*. |
| Test Method | Validate that the *parameter* values set within *Mode* are within the appropriate range as defined in the *swe:AllowedValues* property of that *parameter*. |
| Test Type | Capability |

**Annex B  
(normative)  
  
UML to XML Schema Encoding Rules**

This standard follows a model-driven approach to automatically generate the XML Schema detailed in Section 8 from the UML models introduced in Section 7. The encoding rules used by this standard to generate XML schema are derived from GML encoding rules defined in ISO 19136.

A few changes have been introduced to GML encoding rules in order to accommodate for Sensor Web Enablement specific needs. These changes are listed and explained below:

* Relaxed rule on the mandatory gml:id attribute. gml:id is thus optional in SWE schemas.
* Introduced new stereotype for soft-typed-properties.
* Added support for encoding simple-type properties as XML attributes.
* Use different base type for <<Type>> stereotype (Elements are derived from anyType and made substitutable for gml:AbstractValue instead of gml:AbstractGML).